SECTION 08 71 00.18

WEATHERSTRIPS, THESHOLDS AND DOOR BOTTOMS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2016 -  2020 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Weatherstrips, thresholds, door bottoms and auxiliary products.
1.2	RELATED SECTIONS
A.	Section 08 71 00 - Door Hardware.
1.3	REFERENCES
A.	American National Standards Institute (ANSI): ANSI 117.1 - Standard for Accessible and Usable Buildings and Facilities.
B.	ASTM International (ASTM):
1.	ASTM D2287: Standard Specification for Nonrigid Vinyl Chloride Polymer and Copolymer Molding and Extrusion Compounds.
2.	ASTM E 90: Standard Test Method for Laboratory Measurement of Airborne Sound Transmission Loss of Building Partitions and Elements. 
3.	ASTM E152: Methods of Fire Tests of Door Assemblies.
4.	ASTM E283: Standard Test Method for Determining Rate of Air Leakage Through Exterior Windows, Curtain Walls, and Doors Under Specified Pressure Differences Across the Specimen.
C.	National Fire Protection Association (NFPA): NFPA 252 - Standard Methods of Fire Test for Door Assemblies.
D.	Underwriter's Laboratory (UL): 
1.	UL 10B - Standard for Fire Tests of Door Assemblies.
2.	UL 10C - Standard for Positive Pressure Fire Tests of Door Assemblies. 
3.	UL 1784 - Standard for Air Leakage Tests of Door Assemblies and Other Opening Protectives.
1.4	PERFORMANCE REQUIREMENTS
A.	Sound Rating: Provide products compatible with assemblies for sound-control doors identical to assemblies tested by an independent testing agency per ASTM E90 with the specified minimum certified STC rating per ASTM E413 for the configurations indicated.
B.	Compliance for Fire-Rated Sound-Control Door and Frame Assemblies: 
1.	NFPA 80 compliant, listed and labeled by a testing and inspection agency acceptable to authorities having jurisdiction
2.	Test at equalized pressure per UL 10C.
C.	Compliance with Accessibility Requirements: 
1.	_________________
2.	Accessibility Guidelines for Buildings and Facilities (ADAAG).
3.	ANSI A117.1.
1.5	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Maintenance instructions and recommendations. 
1.6	QUALITY ASSURANCE
A.	Manufacturer Qualifications: The manufacturer of products specified herein shall have a minimum 5 years of experience in the fabrication and installation of similar products.
B.	Installer Qualifications: The installer shall have a minimum 2 years of experience in the installation of products similar to those specified herein.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Deliver, store and handle materials and products in strict compliance with manufacturer's instructions and recommendations. 
B.	Store materials within absolute limits for temperature and humidity recommended by manufacturer. Protect from damage.
1.8	PROJECT CONDITIONS
A.	Environmental Limitations: Do not deliver or install products until spaces are enclosed and weather tight, wet work in spaces is complete and dry, HVAC system is operating and maintaining ambient temperature at occupancy levels during the remainder of the construction period.
B.	Field Measurements: Verify field measurements as indicated on Shop Drawings. Where measurements are not possible, provide control dimensions and templates. 
1.	Coordinate installation and location of blocking and supports as required. 
2.	Verify openings, clearances, storage requirements and other dimensions relevant to the installation and final application.
1.9	WARRANTY
A.	Provide manufacturer's standard limited warranty for products. All Reese products are guaranteed for five years against defects in material or workmanship.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Reese Enterprises, Inc., which is located at:<BR />16350 Asher Ave., P. O. Box 459<BR />Rosemount, MN 55068-0459<BR />Toll Free Tel: 800-328-0953<BR />Tel: 651-423-1126<BR />Fax: 651-423-2662<BR />Email: request info (info@reeseusa.com);Web: https://www.reeseusa.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	THRESHOLDS AND AUXILIARY PRODUCTS
A.	Thresholds and Auxiliary Products: Including but not limited to products as listed below as manufactured by Reese Enterprises, Inc.
1.	Product: Reese model number_______________, quantities, fasteners, lengths and locations as indicated on Drawings with attributes as specified below in this Article.
2.	Products and Attributes: Provide models in quantities, lengths and locations with fasteners as indicated on Drawings with attributes as specified below in this Article. 
3.	Products and Attributes: Provide models in quantities, lengths and locations with attributes and fasteners as scheduled and indicated on Drawings.
4.	Products and Attributes: Provide models in quantities, lengths and locations with fasteners as selected by Architect.
5.	Factory Drilling: As scheduled and indicated on Drawings.
6.	Factory Drilling: None, provide undrilled.
7.	Factory Drilling: Architect shall provide manufacturer with templates for factory drilled holes. Provide undrilled if Architect does not supply template.
8.	Assembly components. 
9.	Beveled aluminum plates. 
10.	Carpet separator thresholds.
11.	Carpet separator thresholds. Semi-rigid PVC.
12.	Hospitality, Carpet and tile transition thresholds. Semi-rigid PVC.
13.	Combination thresholds. 
14.	Combination thresholds. Carpet to tile. Semi-rigid PVC.
15.	Communicating door flat threshold. Semi-rigid PVC.
16.	Corrugated flat plates. 
17.	Fiberglass thresholds. 
18.	Half saddle thresholds. 
19.	Interlock/waterproof thresholds. 
20.	Offset saddle thresholds. 
21.	Panic type thresholds. 
22.	Metal ramps. 
23.	Rubber ramps. 
24.	Semi-rigid PVC carpet to ground ramps.
25.	Semi-rigid PVC carpet to VCT ramps.
26.	Saddle thresholds. 
27.	Stainless steel thresholds. 
28.	Thermal break thresholds. 
29.	Tile separator, handicap accessible thresholds. ADA compliant. Semi-rigid PVC.
30.	Vinyl top thresholds. 
B.	Assembly Components: As manufactured by Reese Enterprises, Inc. 
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: Aluminum, alloy 6063-T5, mill finish.
4.	Materials: Semi-rigid PVC. UL10B Fire tested.
a.	Color: Black
b.	Color: Grey stone.
c.	Color: Tan stone.
5.	Inserts: As scheduled and indicated on Drawings.
6.	Inserts: Silicone materials, black color.
7.	Inserts: Polyurethane, elastomeric thermoplastic, black color.
8.	Inserts: Polyprene, proprietary Reese thermoplastic rubber compound, black color.
9.	Inserts: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
10.	Inserts: None.
C.	Beveled Aluminum Plates: As manufactured by Reese Enterprises, Inc. 
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: Aluminum, alloy 6063-T5, mill finish.
4.	Minimum Plate Width Available: 2 inches (51 mm).
5.	Maximum Plate Width Available: 24 inches (610 mm).
6.	Plate Width: _______________.
7.	Plate Width: As scheduled and indicated on Drawings.
8.	Thickness: As scheduled and indicated on Drawings.
9.	Thickness: 1/8 inch (3.2 mm).
10.	Thickness: 1/4 inch (6.4 mm).
D.	Carpet Separator Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish.
5.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish.
6.	Materials: Semi-rigid PVC. UL10B Fire tested.
a.	Color: Black
b.	Color: Grey stone.
c.	Color: Tan stone.
7.	Depth: As scheduled and indicated on Drawings.
8.	Depth: As scheduled and indicated on Drawings.
9.	Depth: 7/16 inch (11.1 mm).
10.	Depth: 1/2 inch (12.7 mm).
11.	Depth: 23/32 inch (18.2 mm)
E.	Combination Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Depth: 5/8 inch (15.9 mm).
4.	Depth: 23/32 inch (18.2 mm)
5.	Materials: As scheduled and indicated on Drawings.
6.	Materials: Aluminum, alloy 6063-T5, mill finish.
7.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish.
8.	Materials: Semi-rigid PVC. UL10B Fire tested.
a.	Color: Black
b.	Color: Grey stone.
c.	Color: Tan stone.
9.	Width: As scheduled and indicated on Drawings.
10.	Width: 3 inches (76 mm).
11.	Width: 7-1/2 inches (191 mm).
12.	Inserts: As scheduled and indicated on Drawings.
13.	Inserts: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
14.	Inserts: None.
F.	Corrugated Flat Plates: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Thickness: 1/4 inch (6.4 mm).
4.	Minimum Plate Width: 2 inches (51 mm).
5.	Maximum Plate Width: 10 inches (254 mm).
6.	Plate Width: _______________.
7.	Plate Width: As scheduled and indicated on Drawings.
8.	Materials: As scheduled and indicated on Drawings.
9.	Materials: Aluminum, alloy 6063-T5, mill finish.
10.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish.
11.	Materials: Architectural brass, alloy 385, mill finish.
G.	Fiberglass Thresholds:
1.	Model Number: Reese Model FBR-555 as manufactured by Reese Enterprises, Inc.
2.	Materials: Fiberglass.
3.	Width: 5-1/2 inches (140 mm).
4.	Depth: 1/2 inch (12.7 mm).
H.	Half Saddle Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish.
5.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish.
6.	Materials: Architectural brass, alloy 385, mill finish.
7.	Inserts: As scheduled and indicated on Drawings.
8.	Inserts: Silicone materials, black color.
9.	Inserts: None.
I.	Interlock/Waterproof Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish.
5.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish.
6.	Materials: Architectural brass, alloy 385, mill finish.
7.	Inserts: As scheduled and indicated on Drawings.
8.	Inserts: Polyurethane, elastomeric thermoplastic, black color.
9.	Inserts: Polyprene, proprietary Reese thermoplastic rubber compound, black color.
10.	Inserts: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
11.	Inserts: Pile material, grey color.
12.	Inserts: None.
13.	Hooks: As scheduled and indicated on Drawings.
14.	Hooks: Rolled metal hooks, alloy 6063-T5, mill finish.
15.	Hooks: Rolled metal hooks, brass, alloy 385, mill finish.
16.	Hooks: Aluminum, alloy 6063-T5, clear anodized finish.
17.	Hooks: Aluminum, alloy 6063-T5, dark bronze anodized finish.
18.	Hooks: Aluminum, alloy 6063-T5, gold anodized finish.
19.	Hooks: None.
20.	Pans: Provide optional pans for each unit in patterns submitted by Architect.
21.	Pans: Provide optional pans for units as scheduled and indicated on Drawings.
22.	Pans: None.
23.	Weep Holes: Provide optional factory drilled weep holes in thresholds.
24.	Weep Holes: Provide optional factory drilled weep holes in as scheduled and indicated on Drawings.
25.	Weep Holes: None.
J.	Offset Saddle Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish.
5.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish.
6.	Materials: Architectural brass, alloy 385, mill finish.
7.	Width: As scheduled and indicated on Drawings.
8.	Width: 5-1/2 inches (140 mm).
9.	Width: 7 inches (178 mm).
10.	Depth/Offset: As scheduled and indicated on Drawings.
11.	Depth/Offset: 3/4 inch (19.1 mm) deep, 1/2 inch (12.7 mm) offset.
12.	Depth/Offset: 1/2 inch (12.7 mm) deep, 1/4 inch (6.4 mm) offset.
K.	Panic Type Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish.
5.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish.
6.	Materials: Architectural brass, alloy 385, mill finish.
7.	Width: As scheduled and indicated on Drawings.
8.	Width: 3-11/16 inches (94 mm).
9.	Width: 3-3/4 inches (95 mm).
10.	Width: 5 inches (127 mm).
11.	Offset: As scheduled and indicated on Drawings.
12.	Offset: 1/2 inches (12.7 mm).
13.	Offset: None.
14.	Inserts: As scheduled and indicated on Drawings.
15.	Inserts: Polyurethane, elastomeric thermoplastic, black color.
16.	Inserts: Polyprene, proprietary Reese thermoplastic rubber compound, black color.
17.	Inserts: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
18.	Inserts: Pile material, grey color.
19.	Inserts: None.
L.	Metal Ramp Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
M.	Rubber Ramp Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese EZ Ramp Model _______________.
2.	Model Numbers and Attributes: Reese EZ Ramp as scheduled and indicated on Drawings.
3.	Materials: 100 percent reclaimed, 20 mesh minimum, crumb rubber with urethane binders.
4.	Construction: Compression molded ramps and traction pads.
5.	Maximum Hardness (Shore A): 65.
6.	Flared Sides: 22 degree angle.
7.	Edges: 3/16 inch (4.8 mm) rounded edges.
8.	Width/Depth: As scheduled and indicated on Drawings.
9.	Width/Depth: 8 inches (94 mm) wide, 7/8 inch (22.3 mm) deep.
10.	Width/Depth: 12-1/4 inches (311 mm) wide, 1-1/4 inches (32 mm) deep.
N.	Saddle Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
6.	Materials: Aluminum, alloy 6063-T5, black anodized finish. 
7.	Materials: Architectural brass, alloy 385, mill finish. 
8.	Width/Depth: As scheduled and indicated on Drawings.
9.	Width/Depth: 3 inches (76 mm) wide, 3/8 inch (9.5 mm) deep.
10.	Width/Depth: 4 inches (102 mm) wide, 1/2 inch (12.7 mm) deep.
11.	Width/Depth: 4 inches (102 mm) wide, 5/8 inch (15.9 mm) deep.
12.	Width/Depth: 5 inches (127 mm) wide, 1/2 inch (12.7 mm) deep.
13.	Width/Depth: 5 inches (127 mm) wide, 5/8 inch (15.9 mm) deep.
14.	Width/Depth: 6 inches (152 mm) wide, 1/2 inch (12.7 mm) deep.
15.	Width/Depth: 7 inches (178 mm) wide, 1/2 inch (12.7 mm) deep.
16.	Width/Depth: 8 inches (203 mm) wide, 1/2 inch (12.7 mm) deep.
O.	Stainless Steel Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: 10 gauge, stainless steel, alloy 304, mill finish.
4.	Width/Depth: As scheduled and indicated on Drawings.
5.	Width/Depth: 4 inches (102 mm) wide, 1/4 inch (6.4 mm) deep.
6.	Width/Depth: 4 inches (102 mm) wide, 1/2 inch (12.7 mm) deep.
7.	Width/Depth: 5 inches (127 mm) wide, 1/4 inch (6.4 mm) deep.
8.	Width/Depth: 5 inches (127 mm) wide, 1/2 inch (12.7 mm) deep.
P.	Thermal Break Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Splines for Thermal Break: Flexible vinyl.
4.	Types: As scheduled and indicated on Drawings.
5.	Type: Thermal break, saddle thresholds.
6.	Type: Thermal break, offset thresholds.
7.	Type: Thermal break, panic thresholds.
8.	Type: Thermal break, offset panic thresholds.
9.	Materials: As scheduled and indicated on Drawings.
10.	Materials: Aluminum, alloy 6063-T5, mill finish. 
11.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
12.	Inserts: As scheduled and indicated on Drawings.
13.	Inserts: Neoprene material, black color.
14.	Inserts: Polyurethane, elastomeric thermoplastic, black color.
15.	Inserts: Polyprene, proprietary Reese thermoplastic rubber compound, black color.
16.	Inserts: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
17.	Inserts: Pile material, grey color.
18.	Inserts: None.
Q.	Vinyl Top Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings. 
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
2.3	WEATHERSTRIPPING AND AUXILIARY PRODUCTS
A.	Weatherstrips and Auxiliary Products: Including but not limited to products as listed below as manufactured by Reese Enterprises, Inc.
1.	Product: Reese model number_______________, quantities, fasteners, lengths and locations as indicated on Drawings with attributes as specified below in this Article.
2.	Products and Attributes: Provide models in quantities, lengths and locations with fasteners as indicated on Drawings with attributes as specified below in this Article. 
3.	Products and Attributes: Provide models in quantities, lengths and locations with attributes and fasteners as scheduled and indicated on Drawings.
4.	Products and Attributes: Provide models in quantities, lengths and locations with fasteners as selected by Architect.
5.	Factory Drilling: As scheduled and indicated on Drawings.
6.	Factory Drilling: None, provide undrilled.
7.	Factory Drilling: Architect shall provide manufacturer with templates for factory drilled holes. Provide undrilled if Architect does not supply template.
8.	Adjustable weatherstrips.
9.	Astragals.
10.	Brush weatherstrips.
11.	Door jamb weatherstrips.
12.	Edge seal systems/smoke and draft weatherstrips.
13.	Hardware compatible weatherstrips.
14.	Interlocking weatherstrips.
15.	Intumescent seals.
16.	Magnetic weatherstrips.
17.	Neoprene weatherstrips.
18.	Polyprene weatherstrips.
19.	Polyurethane weatherstrips.
20.	Self-adhesive strips.
21.	Silicone weatherstrips.
22.	Smoke and draft weatherstrips.
23.	Stainless Steel weatherstrips.
24.	Vinyl and pile weatherstrips.
B.	Adjustable Weatherstrips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Compliance: Fire rated for use as perimeter seals only; shall not be used in lieu of an integral pressed steel stop on fire rated installations.
4.	Mitered Sides: One side of each piece mitered for sets.
5.	Materials: As scheduled and indicated on Drawings.
6.	Materials: Aluminum, alloy 6063-T5, mill finish. 
7.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
8.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
9.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
10.	Maximum Adjustment Range: As scheduled and indicated on Drawings. 
11.	Maximum Adjustment Range: 1/4 inch (6.4 mm).
12.	Maximum Adjustment Range: 7/16 inch (11.1 mm).
13.	Edge Seals: As scheduled and indicated on Drawings.
14.	Edge Seals: Neoprene material, black color.
15.	Edge Seals: Silicone materials, black color.
C.	Astragals: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	When astragals used on double doors, two lengths must be ordered, one for each door.
4.	Description: As scheduled and indicated on Drawings.
5.	Description: Single astragals.
6.	Description: Single, adjustable astragals.
7.	Description: Single astragals for double doors.
8.	Description: Multi-component astragals for double doors.
9.	Description: Multi-component interlocking astragals for double doors.
10.	Description: Multi-component astragals for double doors, with snap covers to conceal fasteners.
11.	Description: Multi-component adjustable astragals for double doors.
12.	Description: Multi-component, self adjusting magnetic astragals for double doors.
13.	Materials: As scheduled and indicated on Drawings.
14.	Materials: Aluminum, alloy 6063-T5, mill finish. 
15.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
16.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
17.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
18.	Materials: Aluminum, alloy 6063-T5, black anodized finish. 
19.	Materials: Steel, grey prime finish. 
20.	Materials: Architectural brass, alloy 385, mill finish.
21.	Materials: Stainless steel, alloy 304, 10 gauge, mill finish.
22.	Edge Seals: As scheduled and indicated on Drawings.
23.	Edge Seals: Neoprene material, black color.
24.	Edge Seals: Silicone materials, black color.
25.	Edge Seals: Polyurethane, elastomeric thermoplastic, black color.
26.	Edge Seals: Polyprene, proprietary Reese thermoplastic rubber compound, black color.
27.	Edge Seals: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
28.	Edge Seals: Nylon brush, grey color.
29.	Edge Seals: Pile material, grey color.
30.	Edge Seals: None.
D.	Brush Weatherstrips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
6.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
8.	Materials: Aluminum, alloy 6063-T5, black anodized finish. 
9.	Brush Length: As scheduled and indicated on Drawings.
10.	Brush Length: 9/32 inch (7.1 mm).
11.	Brush Length: 3/8 inch (9.5 mm).
12.	Brush Length: 15/16 inch (24 mm).
13.	Brush Length: 1-3/16 inches (30 mm).
14.	Brush Length: 1-9/16 inches (40 mm).
15.	Brush Length: 1-5/8 inches (41 mm).
16.	Brush Length: 1-3/4 inches (44 mm).
17.	Brush Length: 2 inches (51 mm).
18.	Brush Length: 2-1/2 inches (64 mm).
19.	Brush Length: 3 inches (76 mm).
20.	Brush Length: 4 inches (102 mm).
E.	Door Jamb Weatherstrips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
6.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
8.	Materials: Architectural brass, alloy 385, mill finish.
9.	Materials: Stainless steel, alloy 304, 10 gauge, mill finish.
10.	Edge Seals: As scheduled and indicated on Drawings.
11.	Edge Seals: Neoprene material, black color.
12.	Edge Seals: Nylon brush.
13.	Edge Seals: Silicone materials, black color.
14.	Edge Seals: Polyurethane, elastomeric thermoplastic, black color.
15.	Edge Seals: Polyprene, proprietary Reese thermoplastic rubber compound, black color.
16.	Edge Seals: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
17.	Edge Seals: Pile material, grey color.
18.	Edge Seals: None.
F.	Combined Edge Seal Systems/Smoke and Draft Control Gasketing: Reese 588 Series as manufactured by Reese Enterprises, Inc.
1.	Compliance: 
a.	Tested to the requirement of UL 10C, ASTM E152, NFPA 252, UL 10B, UBC 7-2.
b.	Required for Category ' B' fire-rated doors to meet positive pressure and ' S' label. Category G listed and category H listed.
c.	Approved for installation with:
1)	Listed Wood Core Fire Doors with Wood or Steel Fire Door Frames rated 20 minutes (with hose stream).
2)	Listed Mineral Core Fire Doors and Steel Fire Door Frames rated 45, 60, 90 minutes.
2.	Description: 1/8 inch (3.2 mm) clearance required between door and frame.
a.	Has fin on one side to help seal for smoke and draft control.
b.	Expands and seals around door when heated, allows door to operate if needed..
3.	Materials: Graphite-based intumescent with a protective PVC covering.
4.	Width: 5/8 inch (15.9 mm).
5.	Color: As scheduled and indicated on Drawings.
6.	Color: Brown 588D.
7.	Color: Charcoal 588CH.
8.	Color: White 588W.
G.	Hardware Compatible Weatherstrips: As manufactured by Reese Enterprises, Inc. 
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Width: 1-1/2 inches (38 mm).
4.	Depth: 1/4 inch (6.4 mm).
5.	Materials: As scheduled and indicated on Drawings.
6.	Materials: Aluminum, alloy 6063-T5, mill finish. 
7.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
8.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
9.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
10.	Edge Seals: As scheduled and indicated on Drawings.
11.	Edge Seals: Neoprene material, black color.
12.	Edge Seals: Nylon brush.
13.	Edge Seals: Silicone materials, black color.
14.	Edge Seals: Polyurethane, elastomeric thermoplastic, black color.
15.	Edge Seals: Polyprene, proprietary Reese thermoplastic rubber compound, black color.
16.	Edge Seals: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
17.	Edge Seals: Pile material, grey color.
18.	Edge Seals: None.
H.	Interlocking Weatherstrips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Models _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
5.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
6.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
7.	Inserts: As scheduled and indicated on Drawings.
8.	Inserts: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
9.	Inserts: None.
10.	Brush Length: 4 inches (102 mm).
I.	Magnetic Weatherstrips: Reese 574 Series as manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Depth: 5/8 inch (15.9 mm).
4.	Width: 1 inch (25 mm).
5.	Materials: As scheduled and indicated on Drawings.
6.	Materials: Aluminum, alloy 6063-T5, clear anodized finish; 574C. 
7.	Materials: Aluminum, alloy 6063-T5, gold anodized finish; 574G. 
8.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish; 574D.
9.	Length: As scheduled and indicated on Drawings.
10.	Length: 36 inches (914 mm). 
11.	Length: 48 inches (1219 mm). 
12.	Length: 84 inches (2137 mm). 
13.	Length: 96 inches (2438 mm). 
J.	Neoprene Weatherstrips: As manufactured by Reese Enterprises, Inc. 
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Performance: Withstands temperatures from -40 deg F to 200 deg F (-40 deg C to 93 deg C).
4.	Materials: As scheduled and indicated on Drawings.
5.	Materials: Aluminum, alloy 6063-T5, mill finish. 
6.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
8.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
9.	Materials: Aluminum, alloy 6063-T5, black anodized finish. 
K.	Polyprene Weatherstrips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Wear Resistance: More wear resistant than silicone rubber.
4.	Depth: 1/4 inch (6.4 mm).
5.	Width: As scheduled and indicated on Drawings.
6.	Width: 7/8 inch (22.2 mm). 
7.	Width: 3/4 inch (19.1 mm). 
8.	Materials: As scheduled and indicated on Drawings.
9.	Materials: Aluminum, alloy 6063-T5, mill finish. 
10.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
11.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
12.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
13.	Materials: Aluminum, alloy 6063-T5, black anodized finish. 
L.	Polyurethane Weatherstrips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Performance:
a.	4 times the tear resistance compared to silicone rubber. 
b.	40 times the tensile strength compared to silicone rubber.
c.	Nearly 100 times the abrasion resistance compared to silicone rubber.
d.	Flexible to -58 deg F (-50 deg C).
e.	Resistant to ultraviolet light, fungus, petroleum based solvents and Halon fire extinguishant.
4.	Materials: As scheduled and indicated on Drawings.
5.	Materials: Aluminum, alloy 6063-T5, mill finish. 
6.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
8.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
9.	Materials: Aluminum, alloy 6063-T5, black anodized finish. 
M.	Self-Adhesive Strips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Compliance: 
a.	Meets UL 10B, UL 10C Category J and Category H. 
b.	Meets CANA4-S104.
c.	Can use on S labeled doors 17L5 9903
4.	Tape Width: 3/8 inch (9.5 mm).
5.	Overall Width: 1/2 inch (12.7 mm).
6.	Materials: As scheduled and indicated on Drawings.
7.	Materials: Polyurethane base, elastomeric thermoplastic, black color; and Polyprene fins, proprietary Reese thermoplastic rubber compound, black color.
8.	Materials: Neoprene material, black color.
9.	Materials: Silicone materials, black color.
10.	Materials: Polyurethane, elastomeric thermoplastic, black color.
11.	Materials: Polyprene, proprietary Reese thermoplastic rubber compound, black color.
12.	Color: As scheduled and indicated on Drawings.
13.	Color: Black.
14.	Color: Charcoal.
15.	Color: White.
N.	Silicone Weatherstrips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Performance: 
a.	Withstands temperatures from -75 deg F to 400 deg F (-59 deg C to 204 deg C).
b.	Resistant to ultraviolet light, fungus, mildew and moisture.
4.	Materials: As scheduled and indicated on Drawings.
5.	Materials: Aluminum, alloy 6063-T5, mill finish. 
6.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
8.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
9.	Materials: Aluminum, alloy 6063-T5, black anodized finish. 
O.	Stainless Steel Weatherstrips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: Stainless steel, alloy 304, 10 gauge, mill finish.
4.	Edge Seals: As scheduled and indicated on Drawings.
5.	Edge Seals: Neoprene material, black color.
6.	Edge Seals: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
P.	Vinyl And Pile Weatherstrips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
6.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
8.	Materials: Aluminum, alloy 6063-T5, black anodized finish. 
9.	Edge Seals: As scheduled and indicated on Drawings.
10.	Edge Seals: Pile material, grey color.
11.	Edge Seals: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
2.4	DOOR BOTTOMS AND AUXILIARY PRODUCTS
A.	Auxiliary Products for Use with Door Bottoms: As manufactured by Reese Enterprises, Inc.
1.	Product: Reese model number_______________, quantities, fasteners, lengths and locations as indicated on Drawings with attributes as specified below in this Article.
2.	Products and Attributes: Provide models in quantities, lengths and locations with fasteners as indicated on Drawings with attributes as specified below in this Article. 
3.	Products and Attributes: Provide models in quantities, lengths and locations with attributes and fasteners as scheduled and indicated on Drawings.
4.	Products and Attributes: Provide models in quantities, lengths and locations with fasteners as selected by Architect.
5.	Factory Drilling: As scheduled and indicated on Drawings.
6.	Factory Drilling: None, provide undrilled.
7.	Factory Drilling: Architect shall provide manufacturer with templates for factory drilled holes. Provide undrilled if Architect does not supply template.
8.	Automatic door bottoms.
9.	Door extenders.
10.	Door shoes.
11.	Door sweeps.
12.	Hospitality Dark-AN Door Bottoms with Pressure Regulating Alternating Notches.
13.	Door sweeps with nylon brushes.
14.	Rain drips.
B.	Automatic Door Bottoms: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
6.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
8.	Maximum Drop: As scheduled and indicated on Drawings. 
9.	Maximum Drop: 1/2 inch (12.7 mm).
10.	Maximum Drop: 3/4 inch (19.1 mm).
11.	Edge Seals: As scheduled and indicated on Drawings.
12.	Edge Seals: Neoprene material, black color.
13.	Edge Seals: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
14.	Edge Seals: Nylon brush.
15.	Edge Seals: Lead, for X-ray shielding. 
16.	Edge Seals: None.
C.	Door Extenders: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Internal Width: 1-3/4 inches (44 mm).
4.	Inserts: Pile material, grey color.
5.	Materials: As scheduled and indicated on Drawings.
6.	Materials: Aluminum, alloy 6063-T5, mill finish. 
7.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
8.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
9.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
D.	Door Shoes: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
6.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
8.	Edge Seals: As scheduled and indicated on Drawings.
9.	Edge Seals: Polyurethane smooth insert, elastomeric thermoplastic, black color.
10.	Edge Seals: Vinyl insert with fingers, ASTM D2287 and CS230-60 compliant, grey color.
11.	Edge Seals: Pile material, grey color.
12.	Edge Seals: None.
E.	Door Sweeps: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
6.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
8.	Materials: Aluminum, alloy 6063-T5, black anodized finish. 
9.	Materials: Architectural brass, alloy 385, mill finish.
10.	Materials: Stainless steel, alloy 304, 10 gauge, mill finish.
11.	Edge Seals: As scheduled and indicated on Drawings.
12.	Edge Seals: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
13.	Edge Seals: Nylon brush, black color.
14.	Edge Seals: Polyurethane, black color.
15.	Edge Seals: Neoprene, black color.
F.	Hospitality Dark-AN Door Bottoms with Pressure Regulating Alternating Notches: As manufactured by Reese Enterprises, Inc.
1.	Full PVC triple-fin door bottom with flexible triple fins.
a.	Alternating notches in fins for pressure regulation. 
2.	Model Number: Reese Model ________.
3.	Fire Rated: UL 10B - fire tested.
4.	Positive Pressure: UL 10C Category J.
5.	Materials: As scheduled and indicated on Drawings.
6.	Materials: Aluminum, alloy 6063-T5, mill finish. 
7.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
8.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
9.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
10.	Materials: Rigid and Flexible PVC. Color: Brown.
11.	Edge Seals: Rigid and Flexible PVC, black color.
G.	Door Sweeps with Nylon Brushes: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
6.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
8.	Materials: Aluminum, alloy 6063-T5, black anodized finish. 
9.	Brush Length: As scheduled and indicated on Drawings.
10.	Brush Length: 9/32 inch (7.1 mm).
11.	Brush Length: 3/8 inch (9.5 mm).
12.	Brush Length: 15/16 inch (24 mm).
13.	Brush Length: 1-3/16 inches (30 mm).
14.	Brush Length: 1-9/16 inches (40 mm).
15.	Brush Length: 1-5/8 inches (41 mm).
16.	Brush Length: 1-3/4 inches (44 mm).
17.	Brush Length: 2 inches (51 mm).
18.	Brush Length: 2-1/2 inches (64 mm).
19.	Brush Length: 3 inches (76 mm).
20.	Brush Length: 4 inches (102 mm).
H.	Rain Drips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: Aluminum, alloy 6063-T5, mill finish. 
4.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
5.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
6.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, black anodized finish. 
8.	Materials: Architectural brass, alloy 385, mill finish.
9.	Edge Seals: As scheduled and indicated on Drawings.
10.	Edge Seals: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
11.	Edge Seals: Nylon brush.
2.5	AUXILIARY PRODUCTS FOR WEATHERSTRIPS AND THESHOLDS
A.	Auxiliary Products for Use with Weatherstrips and Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Product: Reese model number_______________, quantities, fasteners, lengths and locations as indicated on Drawings with attributes as specified below in this Article.
2.	Products and Attributes: Provide models in quantities, lengths and locations with fasteners as indicated on Drawings with attributes as specified below in this Article. 
3.	Products and Attributes: Provide models in quantities, lengths and locations with attributes and fasteners as scheduled and indicated on Drawings.
4.	Products and Attributes: Provide models in quantities, lengths and locations with fasteners as selected by Architect.
5.	Factory Drilling: As scheduled and indicated on Drawings.
6.	Factory Drilling: None, provide undrilled.
7.	Factory Drilling: Architect shall provide manufacturer with templates for factory drilled holes. Provide undrilled if Architect does not supply template.
8.	Carpet/flooring separators. 
9.	Carpet/flooring transition edges. 
10.	Metal ramps
11.	Aluminum ramps.
12.	Surface applied and elevator stop strips. 
B.	Carpet/Flooring Separator Thresholds: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish.
5.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish.
6.	Depth: As scheduled and indicated on Drawings.
7.	Depth: As scheduled and indicated on Drawings.
8.	Depth: 7/16 inch (11.1 mm).
9.	Depth: 1/2 inch (12.7 mm).
C.	Carpet/Flooring Transition Edges: Beveled aluminum plates as manufactured by Reese Enterprises, Inc. 
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: Aluminum, alloy 6063-T5, mill finish.
4.	Minimum Plate Width Available: 2 inches (51 mm).
5.	Maximum Plate Width Available: 24 inches (610 mm).
6.	Plate Width: _______________.
7.	Plate Width: As scheduled and indicated on Drawings.
8.	Thickness: As scheduled and indicated on Drawings.
9.	Thickness: 1/8 inch (3.2 mm).
10.	Thickness: 1/4 inch (6.4 mm).
D.	Metal Ramps: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
E.	Rubber Ramps: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese EZ Ramp Model _______________.
2.	Model Numbers and Attributes: Reese EZ Ramp as scheduled and indicated on Drawings.
3.	Materials: 100 percent reclaimed, 20 mesh minimum, crumb rubber with urethane binders.
4.	Construction: Compression molded ramps and traction pads.
5.	Maximum Hardness (Shore A): 65.
6.	Flared Sides: 22 degree angle.
7.	Edges: 3/16 inch (4.8 mm) rounded edges.
8.	Width/Depth: As scheduled and indicated on Drawings.
9.	Width/Depth: 8 inches (94 mm) wide, 7/8 inch (22.3 mm) deep.
10.	Width/Depth: 12-1/4 inches (311 mm) wide, 1-1/4 inches (32 mm) deep.
F.	Surface Applied and Elevator Stop Strips: As manufactured by Reese Enterprises, Inc.
1.	Model Number: Reese Model _______________.
2.	Model Numbers and Attributes: As scheduled and indicated on Drawings.
3.	Materials: As scheduled and indicated on Drawings.
4.	Materials: Aluminum, alloy 6063-T5, mill finish. 
5.	Materials: Aluminum, alloy 6063-T5, clear anodized finish. 
6.	Materials: Aluminum, alloy 6063-T5, gold anodized finish. 
7.	Materials: Aluminum, alloy 6063-T5, dark bronze anodized finish. 
8.	Inserts: As scheduled and indicated on Drawings.
9.	Inserts: Polyprene, proprietary Reese thermoplastic rubber compound, black color.
10.	Inserts: Vinyl, ASTM D2287 and CS230-60 compliant, grey color.
11.	Inserts: None.
PART 3    EXECUTION
3.1	EXAMINATION AND PREPARATION
A.	Verify that field measurements, surfaces, substrates and conditions are as required, and ready to receive Work.
B.	Prepare substrates using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions. 
C.	Do not proceed with installation until substrates have been properly prepared and deviations from manufacturer's recommended tolerances are corrected. Commencement of installation constitutes acceptance of conditions.
D.	If preparation is the responsibility of another installer, notify Architect in writing of deviations from manufacturer's recommended installation tolerances and conditions
3.2	INSTALLATION
A.	Install units plumb, square, in proper alignment with adjacent construction and secured to substrate, within manufacturer's recommended tolerances. Comply with manufacturer's installation instructions and approved submittals.
3.3	ADJUSTING
A.	Prior to installation, adjust components to within tolerances recommended by manufacturer.
B.	Adjust units and hardware so doors operate smoothly close with uniform frame alignment and seal compression.
3.4	CLEANING AND PROTECTION
A.	Clean exposed surfaces. Touch up, refinish, or replace damaged components in a manner acceptable to Architect. 
B.	Protect installed products until completion of project. 
C.	Repair or replace defective work as directed by Architect upon inspection.

END OF SECTION