SECTION 23 82 29.13

RADIATORS, HYDRONIC AND ELECTRIC - RESIDENTIAL

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2025 -  2025 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Residential hydronic radiators.
B.	Residential hydronic towel radiators.
C.	Residential electric radiators.
D.	Residential electric towel radiators.
E.	Residential steam radiators.
F.	Specialty and made-to-order residential radiators.
1.2	RELATED SECTIONS
A.	Section 22 05 00 - Common Work Results for Plumbing.
B.	Section 26 05 00 - Common Work Results for Electrical.
1.3	SUBMITTALS
A.	Submit under the provisions of Section 01 30 00.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction.
1.4	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum of fifteen years' documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
1.5	PRE-INSTALLATION CONFERENCE
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.7	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.8	WARRANTY
A.	Manufacturer's standard limited warranty unless indicated otherwise.
1.	All Runtal North America Inc. radiators will have a five-year standard limited warranty per published Limited Warranty statement as published on the Runtal North America, Inc. web site.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Runtal North America, Inc., which is located at:<BR />187 Neck Rd.<BR />Ward Hill, MA 01835-0778<BR />Toll Free Tel: 800-526-2621<BR />Tel: 978-373-1666<BR />Fax: 978-372-7140<BR />Email: request info (info@runtalnorthamerica.com);Web: http://www.runtalnorthamerica.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with the provisions of Section 01 60 00.
2.2	RESIDENTIAL HYDRONIC RADIATORS
A.	Basis of Design: Baseboard Radiators. Low profile perimeter heating solution.
1.	Construction: Heavy gauge fully welded steel.
2.	Finish: Powder coat. Color: ________.
3.	Mounting: Wall. Hardware included. 1 to 3 inches from floor.
4.	Model UF-2: Height: 6 inches. BTUH per ft: 600.
5.	Model UF-3: Height: 9 inches. BTUH per ft: 770.
6.	Model UF-4: Height: 12 inches. BTUH per ft: 930.
7.	Lengths: 2 to 3.5 ft in 6 inch increments. 4 to 14 ft in 1 ft increments.
8.	Uniform Pipe Fittings: 1/2 inch NPT. Vent Fittings: 1/8 inch. Vent included.
9.	Air Vent: To be opposite the supply side of the radiator.
10.	Multiple piping configurations.
11.	Vertical Covers: For straight vertical pipe between the radiator and floor. Field cut for heights other than 3 and 10 inches.
12.	Horizontal Covers: Standard trims simply snap into place. Require a 2 inch overlap on the radiator for proper fit.
a.	Straight Trims: 12 inches long. Used as end and center trims.
b.	Inside Corners: 12 x 12 inch.
c.	Right End Cap: 6 x 2 inch.
d.	Left End Cap: 2 x 6 inch.
e.	Outside Corner Trims and Special Trims: Available by request.
B.	Basis of Design: Wall Panel Radiators:
1.	Construction: Heavy gauge fully welded steel.
2.	Finish: Powder coat. Color: ________.
3.	Model UF-6: Height: 18 inches. BTUH per ft: 1430.
4.	Model UF-8: Height: 24 inches. BTUH per ft: 1810.
5.	Lengths: 2 to 3.5 ft in 6 inch increments. 4 to 14 ft in 1 ft increments.
6.	Mounting: Wall. Hardware included. 1 to 3 inches from floor.
7.	Uniform Pipe Fittings: 1/2 inch NPT. Vent Fittings: 1/8 inch. Vent included.
8.	Air Vent: To be opposite the supply side of the radiator.
9.	Multiple piping configurations.
10.	Vertical Covers: For straight vertical pipe between the radiator and floor. Field cut for heights other than 3 and 10 inches.
11.	Horizontal Covers: Standard trims simply snap into place. Require a 2 inch overlap on the radiator for proper fit.
a.	Straight Trims: 12 inches long. Used as end and center trims.
b.	Inside Corners: 12 x 12 inch
c.	Right End Cap: 6 x 2 inch.
d.	Left End Cap: 2 x 6 inch.
e.	Outside Corner Trims and Special Trims: Available by request.
C.	Basis of Design: Vertical Panel Radiators:
1.	Construction: Heavy gauge fully welded steel.
2.	Finish: Powder coat. Color: ________.
3.	Mounting: Wall. Hardware included. 1 to 3 inches from floor.
4.	Model UHX-4 (HxWxD): 36 x 12 x 2 inches. BTUH: 1680.
5.	Model UHX-4 (HxWxD): 72 x 12 x 2 inches. BTUH: 3360.
6.	Model UHX-6 (HxWxD): 36 x 18 x 2 inches. BTUH: 2520.
7.	Model UHX-6 (HxWxD): 72 x 18 x 2 inches. BTUH: 5040.
8.	Model UHX-8 (HxWxD): 36 x 24 x 2 inches. BTUH: 3360.
9.	Model UHX-8 (HxWxD): 72 x 24 x 2 inches. BTUH: 6720.
10.	Uniform Pipe Fittings: 1/2 inch NPT. Vent Fittings: 1/8 inch. Vent included.
11.	Air Vent: To be opposite the supply side of the radiator.
12.	Piping Configuration: Supply: Bottom left. Return: Bottom right.
13.	Piping Configuration: Supply: Bottom right. Return: Bottom left.
14.	Vertical Covers: For straight vertical pipe between the radiator and floor. Field cut for heights other than 3 and 10 inches.
2.3	RESIDENTIAL HYDRONIC TOWEL RADIATORS
A.	Basis of Design: Flat-Tube Hydronic Towel Radiators:
1.	Model Series: Omnipanel: Low profile design available in five sizes. A large surface area maximizes radiant output, making it a heat source, towel warmer, and dryer.
2.	To be installed in a Closed Loop Forced Hot Water Heating Systems.
3.	Construction: Cold rolled welded steel one piece. Flattened water tubes welded to headers at each end.
4.	Finish: Gloss powder coat. Color: ________. Paint Thickness: 2 to 3 mils.
5.	Mounting: Wall. Method: Wall brackets.
a.	Drywall Construction: May require metal wall anchors.
b.	Solid Wood or Placement Directly onto Blocking: Requires No. 8 x 1-1/2 inch long screws.
6.	Piping Connections: Inlet and Outlet: 1/2 inch NPT. Vents: 1/8 inch NPT.
7.	Style: Runtal Omnipanel.
8.	Heat outputs at 180 degrees F AWT and 70 degrees F room temperature.
9.	Model: TW9. Height: 26.1 inches.
a.	Width: 16 inches. BTUH: 1600.
b.	Width: 20 inches. BTUH: 2000.
c.	Width: 24 inches. BTUH: 2400.
d.	Width: 30 inches. BTUH: 3000.
e.	Width: 36 inches. BTUH: 3600.
10.	Model: TW12. Height: 34.8 inches.
a.	Width: 16 inches. BTUH: 1920.
b.	Width: 20 inches. BTUH: 2400.
c.	Width: 24 inches. BTUH: 1880.
d.	Width: 30 inches. BTUH: 3600.
e.	Width: 36 inches. BTUH: 4320.
11.	Model: TW12. Height: 43.6 inches.
a.	Width: 16 inches. BTUH: 2400.
b.	Width: 20 inches. BTUH: 3000.
c.	Width: 24 inches. BTUH: 3600.
d.	Width: 30 inches. BTUH: 4500.
e.	Width: 36 inches. BTUH: 5400.
12.	Model: TW18. Height: 52.3 inches.
a.	Width: 16 inches. BTUH: 3040.
b.	Width: 20 inches. BTUH: 3800.
c.	Width: 24 inches. BTUH: 4560.
d.	Width: 30 inches. BTUH: 5700.
e.	Width: 36 inches. BTUH: 6840.
13.	Model: TW21. Height: 61.1 inches.
a.	Width: 16 inches. BTUH: 3520.
b.	Width: 20 inches. BTUH: 4400.
c.	Width: 24 inches. BTUH: 5280.
d.	Width: 30 inches. BTUH: 6600.
e.	Width: 36 inches. BTUH: 7920.
B.	Basis of Design: Round Tube Style: A large surface area to maximize radiant output, making it a heat source, towel warmer, and dryer.
1.	May be part of the closed loop hydronic heating system.
2.	Construction: Welded one piece. Round water tubes welded to headers.
3.	Material: Low carbon steel.
a.	Finish: Gloss powder coat. Color: ________. Paint Thickness: 2 to 3 mils.
b.	Finish: Chrome plated.
4.	Material: Stainless steel. Finish: Brushed stainless steel.
5.	Mounting: Wall. Method: Wall brackets.
a.	Drywall Construction: May require metal wall anchors.
b.	Solid Wood or Placement Directly onto Blocking: Requires No. 8 x 1-1/2 inch long screws.
6.	Piping Connections: Inlet and Outlet: 1/2 inch NPT. Vents: 1/8 inch NPT.
7.	Style: Runtal Omnipanel.
8.	Heat outputs at 180 degrees F AWT and 70 degrees F room temperature.
9.	Model: Runtal Neptune. Width: 19.5 inches. Depth: 4.2 inches.
a.	NTR-3320. Height: 33.1 inches.
1)	Painted Finish: 2228 BTUH.
2)	Chrome Finish and Stainless Steel: 1782 BTUH.
b.	NTR-4620. Height: 45.7 inches.
1)	Painted Finish: 2706 BTUH.
2)	Chrome Finish and Stainless Steel: 2213 BTUH.
10.	Model: Runtal Radia. Depth: 3.6 inches.
a.	RTR-2924. Width: 23.6 inches. Height: 28.4 inches. BTUH 2136.
b.	RTR-4624. Width: 23.6 inches. Height: 45.4 inches. BTUH 3358.
c.	RTR-4630. Width: 29.5 inches. Height: 45.4 inches. BTUH 4150.
11.	Model: Runtal Versus.
a.	Width: 22.8 inches. Depth: 3.2 inches.
b.	VTR-5223. Height: 51.5 inches. BTUH 2656.
c.	VTR-6923. Height: 68.5 inches. BTUH 3494.
12.	Model: Runtal Solea.
a.	Width: 19.7 inches. Depth: 5.5 inches.
b.	STR-3420. Height: 33.8 inches. BTUH 2014.
c.	STR-5420. Height: 53.3 inches. BTUH 3108.
13.	Model: Runtal Fain.
a.	Width: 19.7 inches. Depth: 3.5 inches. Height: 33.1 inches.
b.	FTR-3320. BTUH: 984.
2.4	RESIDENTIAL ELECTRIC RADIATORS
A.	Basis of Design: Electric Baseboard - Even radiant heat and high output design.
1.	Model: EB3 Series. Mounting: Wall. Either end may be used for wiring.
2.	Model: EBP Series. Mounting: Floor, pedestal. Either end may be used for wiring.
3.	Compliance: cULus Listed.
4.	Height: 10.5 inches. Depth: 2.25 inches.
5.	Lengths: Available in 3 to 10 ft in 12 inch increments. Weight: 10 lbs per ft.
6.	Construction: Welded steel.
7.	Finish: Powder coat. Color: ________. Paint Thickness: 2 to 3 mils.
8.	Wiring: Multiple electric baseboards must be wired in parallel.
9.	Model: EB3-120D-(120 Volts).
10.	Model: EBP-120D-(120 Volts). Freestanding floor mounted option for curtain wall.
11.	Model: EB3-208D-(208 Volts).
12.	Model: EBP-208D-(208 Volts). Freestanding floor mounted option for curtain wall.
13.	Model: EB3-240D-(240 Volts).
14.	Model: EBP-240D-(240 Volts). Freestanding floor mounted option for curtain wall.
15.	Length: 36 inches. BTUH Output: 1500. Watt Output: 440.
16.	Length: 48 inches. BTUH Output: 2000. Watt Output: 586.
17.	Length: 60 inches. BTUH Output: 2500. Watt Output: 733.
18.	Length: 72 inches. BTUH Output: 3000. Watt Output: 879.
19.	Length: 84 inches. BTUH Output: 3500. Watt Output: 1026.
20.	Length: 96 inches. BTUH Output: 4000. Watt Output: 1172.
21.	Length: 108 inches. BTUH Output: 4500. Watt Output: 1319.
22.	Length: 120 inches. BTUH Output: 5000. Watt Output: 1466.
23.	Accessories:
a.	Floor pedestals.
b.	End caps.
c.	End trims.
d.	Center trims.
e.	Inside corner trims.
f.	Outside corner trims.
B.	Basis of Design: Electric Wall Panels - Model EWP:
1.	Compliance: cULus:
2.	Construction: Welded construction.
3.	Finish: Powder coat. Color: ________. Paint Thickness: 2 to 3 mils.
4.	Wiring: Multiple electric baseboards must be wired in parallel.
5.	Depth: 2-1/2 inches.
6.	Model: EWP-6-120D-(120 Volts). Height: 17-1/4 inch. Weight: 15 lbs per ft.
a.	Length: 24 inches. BTUH Output: 2013. Watt Output: 590. Amps: 4.9.
b.	Length: 36 inches. BTUH Output: 3003. Watt Output: 880. Amps: 7.3.
c.	Length: 48 inches. BTUH Output: 4026. Watt Output: 1180. Amps: 9.8.
7.	Model: EWP-6-208D-(208 Volts). Height: 17-1/4 inch. Weight: 15 lbs per ft.
a.	Length: 24 inches. BTUH Output: 2013. Watt Output: 590. Amps: 2.8.
b.	Length: 36 inches. BTUH Output: 3003. Watt Output: 880. Amps: 4.2.
c.	Length: 48 inches. BTUH Output: 4026. Watt Output: 1180. Amps: 5.7.
8.	Model: EWP-6-240D-(240 Volts). Height: 17-1/4 inch. Weight: 15 lbs per ft.
a.	Length: 24 inches. BTUH Output: 2013. Watt Output: 590. Amps: 2.5.
b.	Length: 36 inches. BTUH Output: 3003. Watt Output: 880. Amps: 3.7.
c.	Length: 48 inches. BTUH Output: 4026. Watt Output: 1180. Amps: 4.9.
9.	Model: EWP-8-120D-(120 Volts). Height: 23-1/8 inch. Weight: 15 lbs per ft.
a.	Length: 24 inches. BTUH Output: 2627. Watt Output: 770. Amps: 6.4.
b.	Length: 36 inches. BTUH Output: 3924. Watt Output: 1150. Amps: 9.6.
c.	Length: 48 inches. BTUH Output: 5220. Watt Output: 1530. Amps: 12.8.
10.	Model: EWP-8-208D-(208 Volts). 23-1/8 inch. Weight: 15 lbs per ft.
a.	Length: 24 inches. BTUH Output: 2627. Watt Output: 770. Amps: 3.7.
b.	Length: 36 inches. BTUH Output: 3924. Watt Output: 1150. Amps: 5.5.
c.	Length: 48 inches. BTUH Output: 5220. Watt Output: 1530. Amps: 7.4.
11.	Model: EWP-8-240D-(240 Volts). 23-1/8 inch. Weight: 15 lbs per ft.
a.	Length: 24 inches. BTUH Output: 2627. Watt Output: 770. Amps: 3.2.
b.	Length: 36 inches. BTUH Output: 3924. Watt Output: 1150. Amps: 4.8.
c.	Length: 48 inches. BTUH Output: 5220. Watt Output: 1530. Amps: 6.4.
2.5	RESIDENTIAL ELECTRIC TOWEL RADIATORS:
A.	Basis of Design: Flat Tube Style: Runtal Omnipanel ll.
1.	Compliance: cULus.
2.	Controls: Built-in toggle switch. Operates without further accessories or connected to a timer or thermostat.
3.	Controls: No unit controls for when building codes won't permit unit mounted controls on specific placements, such as above a tub.
a.	Must be connected to a switching device, thermostat, relay switch, etc.
4.	Wiring Procedures and Connections: In accordance with the National Electric Code (NEC) and local codes.
5.	Finish: Gloss powder coat. Color: ________. Paint Thickness: 2 to 3 mils.
6.	Finish: Chrome plated.
7.	Finish: Brushed stainless steel.
8.	Mounting: Wall. Mounting brackets supplied.
9.	Model: OPII 9. Width: 24.0 inches. Depth: 3.8 inches. Height: 26.1 inches.
a.	BTUH Output: 1450. Watt Output: 425.
b.	Voltage: 120. Amp Draw: 3.5.
c.	Voltage: 208. Amp Draw: 2.0.
d.	Voltage: 240 Amp Draw: 1.9.
10.	Model: OPII 12. Width: 24.0 inches. Depth: 3.8 inches. Height: 34.8 inches.
a.	BTUH Output: 2400. Watt Output: 700.
b.	Voltage: 120. Amp Draw: 5.8.
c.	Voltage: 208. Amp Draw: 3.4.
d.	Voltage: 240 Amp Draw: 2.9.
11.	Model: OPII 15. Width: 24.0 inches. Depth: 3.8 inches. Height: 43.6 inches.
a.	BTUH Output: 2400. Watt Output: 700.
b.	Voltage: 120. Amp Draw: 5.8.
c.	Voltage: 208. Amp Draw: 3.4.
d.	Voltage: 240 Amp Draw: 2.9.
B.	Basis of Design: Round Tube Style: Five round tube towel radiators.
1.	Wiring: Direct wire.
2.	Wiring: Plug-in.
3.	Digital Controls: Soft-touch. Five settings: Off, low, med. High, High timer for 3 hours.
4.	Finish: Powder coat. Color: ________.
5.	Finish: Chrome plated.
6.	Finish: Brushed stainless steel.
7.	Mounting: Wall. Mounting brackets supplied.
8.	Style: Runtal Neptune.
a.	Model: NTRE-3320 (WxDxH). 19.5 x 4.2 x 37.4 inches.
1)	BTUH Output: 1536. Watt Output: 450. Amp Draw at 120 V: 4.1.
b.	Model: NTRE-3320C/S (WxDxH). 19.5 x 4.2 x 37.4 inches.
1)	BTUH Output: 1024. Watt Output: 300. Amp Draw at 120 V: 2.7.
c.	Model: NTRE-4620 (WxDxH). 19.5 x 4.2 x 50.0 inches.
1)	BTUH Output: 2048. Watt Output: 600. Amp Draw at 120 V: 5.5.
d.	Model: NTRE-4620C/S (WxDxH). 19.5 x 4.2 x 50.0 inches.
1)	BTUH Output: 1536. Watt Output: 450. Amp Draw at 120 V: 4.1.
9.	Style: Runtal Radia.
a.	Model: RTRE-2924 (WxDxH). 23.6 x 3.6 x 32.7 inches.
1)	BTUH Output: 1536. Watt Output: 450. Amp Draw at 120 V: 4.1.
b.	Model: RTRE-4624 (WxDxH). 23.6 x 3.6 x 49.7 inches.
1)	BTUH Output: 2048. Watt Output: 600. Amp Draw at 120 V: 5.5.
c.	Model: RTRE-4630 (WxDxH). 29.5 x 3.6 x 49.7 inches.
1)	BTUH Output: 3072. Watt Output: 900. Amp Draw at 120 V: 8.2.
10.	Style: Runtal Solea. A curved profile allowing towels to be hung on top of each other.
a.	Model: STRE-3420 (WxDxH). 19.7 x 5.5 x 38.1 inches.
1)	BTUH Output: 1536. Watt Output: 450. Amp Draw at 120 V: 4.1.
b.	Model: STRE-5420 (WxDxH). 19.7 x 5.5 x 57.6 inches.
1)	BTUH Output: 3072. Watt Output: 900. Amp Draw at 120 V: 8.2.
2.6	RESIDENTIAL STEAM RADIATORS
A.	Basis of Design: Steamview. Made for one and two pipe steam systems.
1.	Construction: Cast steel.
2.	Two-Pipe Steam System:
a.	Left hand steam supply. Top input.
b.	Left hand steam supply. Bottom input.
c.	Right hand steam supply. Top input.
d.	Right hand steam supply. Bottom input.
e.	A 1 inch NPT tapping is built into each corner of the radiator.
1)	Two 1 inch plugs are provided to plug the two unused radiator tappings.
2)	A 1 inch plug with a 1/8 inch vent tapping.
3)	Pipe dope should be applied to the plugs.
f.	Proper Size Reducing Bushing for the Steam Trap: Supplied by the installer.
3.	Single-Pipe Steam System:
a.	Left hand steam supply. Bottom input.
b.	Right hand steam supply. Bottom input.
c.	A 1 inch NPT tapping is built into each corner of the radiator.
1)	Two 1 inch plugs are provided to plug the two unused radiator tappings.
2)	A 1 inch plug with a 1/8 inch vent tapping.
3)	Pipe dope should be applied to the plugs.
d.	A one pipe steam air vent or control valve in the mounted in the 1/8 inch vent tapping. Supplied by the installer.
4.	Mounting:
a.	Wall Mounting Brackets: To be secured to load-bearing wall members; wall stud or solid backing, capable of handling the radiator's weight.
b.	Orientation: Radiator is to be tilted a minimum of 1/16 inch per ft toward the condensate return.
5.	Finish: Powder coat. Color: ________.
6.	Model: SV16-24 (HxDxL): 16 x 2.5-3.0 x 24 inches. Weight: 10 lbs. BTUH: 2564.
7.	Model: SV16-36 (HxDxL): 16 x 2.5-3.0 x 36 inches. Weight: 15 lbs. BTUH: 3763.
8.	Model: SV16-48 (HxDxL): 16 x 2.5-3.0 x 48 inches. Weight: 22 lbs. BTUH: 5104.
9.	Model: SV16-60 (HxDxL): 16 x 2.5-3.0 x 60 inches. Weight: 27 lbs. BTUH: 6306.
10.	Model: SV16-72 (HxDxL): 16 x 2.5-3.0 x 72 inches. Weight: 33 lbs. BTUH: 7646.
11.	Model: SV24-24 (HxDxL): 24 x 2.5-3.0 x 24 inches. Weight: 14 lbs. BTUH: 3553.
12.	Model: SV24-36 (HxDxL): 24 x 2.5-3.0 x 36 inches. Weight: 21 lbs. BTUH: 5225.
13.	Model: SV24-48 (HxDxL): 24 x 2.5-3.0 x 48 inches. Weight: 30 lbs. BTUH: 7106.
14.	Model: SV24-60 (HxDxL): 24 x 2.5-3.0 x 60 inches. Weight: 37 lbs. BTUH: 8778.
15.	Model: SV24-72 (HxDxL): 24 x 2.5-3.0 x 72 inches. Weight: 46 lbs. BTUH: 10659.
B.	Basis of Design: Charleston Pro: Made for one and two pipe steam systems.
1.	Construction: All-welded steel.
2.	2-Pipe Steam System:
a.	Left hand steam supply. Top input.
b.	Left hand steam supply. Bottom input.
c.	Right hand steam supply. Top input.
d.	Right hand steam supply. Bottom input.
e.	A 1 inch NPT tapping is built into each corner of the radiator.
1)	Two 1 inch plugs are provided to plug the two unused radiator tappings.
2)	A 1 inch plug with a 1/8 inch vent tapping.
3)	Pipe dope should be applied to the plugs.
f.	Proper Size Reducing Bushing for the Steam Trap: Supplied by the installer.
3.	1-Pipe Steam System:
a.	Left hand steam supply. Bottom input.
b.	Right hand steam supply. Bottom input.
c.	A 1 inch NPT tapping is built into each corner of the radiator.
1)	Two 1 inch plugs are provided to plug the two unused radiator tappings.
2)	A 1 inch plug with a 1/8 inch vent tapping.
3)	Pipe dope should be applied to the plugs.
d.	A one pipe steam air vent or control valve in the mounted in the 1/8 inch vent tapping. Supplied by the installer.
4.	Mounting:
a.	Wall Mounting Brackets: To be secured to load-bearing wall members; wall stud or solid backing, capable of handling the radiator's weight.
b.	Orientation: Radiator is to be tilted a minimum of 1/16 inch per ft toward the condensate return.
5.	Finish: Powder coat. Color: ________.
6.	Model: SV16-24 (HxDxL): 16 x 4 x 24 inches. Weight: 21 lbs. BTUH: 2990.
7.	Model: SV16-36 (HxDxL): 16 x 4 x 36 inches. Weight: 30.3 lbs. BTUH: 4370.
8.	Model: SV16-48 (HxDxL): 16 x 4 x 48 inches. Weight: 40.5 lbs. BTUH: 5980.
9.	Model: SV16-60 (HxDxL): 16 x 4 x 60 inches. Weight: 51.3 lbs. BTUH: 7590.
10.	Model: SV16-72 (HxDxL): 16 x 4 x 72 inches. Weight: 60.5 lbs. BTUH: 8970.
11.	Model: SV24-24 (HxDxL): 24 x 4 x 24 inches. Weight: 29.2 lbs. BTUH: 4654.
12.	Model: SV24-36 (HxDxL): 24 x 4 x 36 inches. Weight: 42.4 lbs. BTUH: 6820.
13.	Model: SV24-48 (HxDxL): 24 x 4 x 48 inches. Weight: 57.8 lbs. BTUH: 9308.
14.	Model: SV24-60 (HxDxL): 24 x 4 x 60 inches. Weight: 73.2 lbs. BTUH: 11814.
15.	Model: SV24-72 (HxDxL): 24 x 4 x 72 inches. Weight: 86.4 lbs. BTUH: 13962.
C.	Basis of Design: Steam Radiators - Steam Flow Form: Fins arranged in a spiral around the heating tube radiate heat efficiently throughout the room.
1.	For two-pipe steam systems only.
2.	Construction: Stainless steel.
3.	Mounting: Floor. Pedestals. Tilt Toward Condensate Return: 1/16 inch per foot.
4.	Height: 7.65 inches. Diameter: 5.5 inches.
5.	Supply Side: Control Valve. 1 inch NPT.
6.	Return Side: Steam trap. 1/2 inch NPT.
7.	Model XSFF 91.44: Length: 36 inches. BTUH: 3000.
8.	Model XSFF 182.88: Length: 72 inches. BTUH: 6230.
2.7	SPECIALTY AND MADE-TO-ORDER RESIDENTIAL RADIATORS
A.	Basis of Design: Made-to-Order Radiant Baseboard. Model VLX. 5-year limited warranty.
1.	Built to order. Length: 20 inches to 29.5 ft in 2 inch increments.
2.	Construction: Cold rolled welded steel one piece. Flattened water tubes welded to headers at each end.
a.	Top Grille: 0.09 inch thick minimum, all-welded perforated.
3.	Finish: Gloss powder coat. Color: ________. Paint Thickness: 2 to 3 mils.
4.	Mounting: Free standing. Floor posts required.
5.	Panel Thermal Expansion: Not to exceed 1/64 inch per ft at 215 degrees F AWT.
6.	Piping Connections: Inlet and Outlet: 1/2 inch NPT. Vents: 1/8 inch NPT.
7.	Pressure Rating, Standard: 56 psi max. Test Pressure: 74 psi max.
a.	Minimum Wall Thickness: 0.048 inch.
8.	Pressure Rating, High: 128 psi max. Test Pressure: 184 psi max.
a.	Minimum Wall Thickness: 0.078 inch.
9.	Ribbed pipe cover trims, finished to match the radiators, provided with the radiation.
10.	Combination shutoff valve/union fitting of less than two inches in width for the supply and return to each panel radiator, to be field installed by others.
11.	Runtal-Flex Connectors: To be used where appropriate to provide expansion compensation for the radiators.
12.	Avg Water Temp of 180 degrees F. BTUH/ft at 65 degrees F, EAT.
13.	Model with Fins: VLX 7/7. Height: 2.8 inches Depth: 2 inches. BTUH/ft: 380.
14.	Model with Fins: VLX 14/14. Height: 5.8 inches Depth: 2 inches. BTUH/ft: 610.
15.	Model with Fins: VLX 21/21. Height: 8.6 inches Depth: 2 inches. BTUH/ft: 790.
16.	Model with Fins: VLX 28/28. Height: 11.5 inches Depth: 2 inches. BTUH/ft: 950.
17.	Model without Fins: VX 7. Height: 2.8 inches Depth: 2 inches. BTUH/ft: 160.
18.	Model without Fins: VX 14. Height: 5.8 inches Depth: 2 inches. BTUH/ft: 290.
19.	Model without Fins: VX 21. Height: 8.6 inches Depth: 2 inches. BTUH/ft: 430.
20.	Model without Fins: VX 28. Height: 11.5 inches Depth: 2 inches. BTUH/ft: 570.
B.	Basis of Design: Made-to-Order Wall Panels.
1.	Construction: Heavy gauge fully welded steel.
2.	Finish: Electrostatically applied, baked on powder coat paint. Color: ________.
3.	Available Lengths: 20 inches to 354 inches in increments of 2 inches.
4.	Mounting: Wall. Hardware included. 1 to 3 inches from floor.
5.	Uniform Pipe Fittings: 1/2 inch NPT. Vent Fittings: 1/8 inch. Vent included.
6.	Air Vent: To be opposite the supply side of the radiator.
7.	Multiple piping configurations.
8.	Vertical Covers: For straight vertical pipe between the radiator and floor. Field cut for heights other than 3 and 10 inches.
9.	Horizontal Covers: Standard trims simply snap into place. Require a 2 inch overlap on the radiator for proper fit.
a.	Straight Trims: 12 inches long. Used as end and center trims.
b.	Inside Corners: 12 x 12 inch.
c.	Right End Cap: 6 x 2 inch.
d.	Left End Cap: 2 x 6 inch.
e.	Outside Corner Trims and Special Trims: Available by request.
10.	Average Water Temperature: 180 degrees F.
11.	Model with Fins: VLX 35/35. Height: 14.4 inches. Depth: 2 inches. BTUH: 1260.
12.	Model with Fins: VLX 42/42. Height: 17.2 inches. Depth: 2 inches. BTUH: 1460.
13.	Model with Fins: VLX 49/49. Height: 20.2 inches. Depth: 2 inches. BTUH: 1650.
14.	Model with Fins: VLX 56/56. Height: 23.1 inches. Depth: 2 inches. BTUH: 1840.
15.	Model with Fins: VLX 63/56. Height: 26.1 inches. Depth: 2 inches. BTUH: 1950.
16.	Model with Fins: VLX 70/56. Height: 29.0 inches. Depth: 2 inches. BTUH: 2050.
17.	Model without Fins: VX 35. Height: 14.4 inches. Depth: 2 inches. BTUH: 710.
18.	Model without Fins: VX 42. Height: 17.2 inches. Depth: 2 inches. BTUH: 860.
19.	Model without Fins: VX 49. Height: 20.2 inches. Depth: 2 inches. BTUH: 1010.
20.	Model without Fins: VX 56. Height: 23.1 inches. Depth: 2 inches. BTUH: 1150.
21.	Model without Fins: VX 63. Height: 26.1 inches. Depth: 2 inches. BTUH: 1300.
22.	Model without Fins: VX 70. Height: 29.0 inches. Depth: 2 inches. BTUH: 1450.
C.	Basis of Design: Made-to-Order Vertical Steel Panel Radiators: Model HX.
1.	Tubes running vertically from floor to ceiling. Can be recessed into the wall.
2.	Built to order. Length: 20 inches to 29.5 ft in 2 inch increments without splicing. Wall to wall applications for perimeter heating.
3.	Construction: Cold rolled low carbon welded steel, one piece. A pair of flattened water tube panels welded to headers at each end.
a.	Side Grille: 0.09 inch thick minimum, all-welded perforated. On both sides.
4.	Finish: Powder coat. Color: ________. Paint Thickness: 2 to 3 mils.
5.	Mounting: Wall. Support blocking for radiator mounting to be by others.
6.	Mounting: Free standing. Floor posts required.
7.	Panel Thermal Expansion: Not to exceed 1/64 inch per ft at 215 degrees F AWT.
a.	Expansion Compensation: Provided in the piping as required, by others.
8.	Header Pipes: Square 0.109 inches minimum wall thickness. Include necessary supply, return, and air vent connections. Internal baffling as required.
9.	Uniform Pipe Fittings: 1/2 inch NPT. Vent Fittings: 1/8 inch. Vent included.
10.	Air Vent: To be opposite the supply side of the radiator.
11.	Multiple piping configurations.
12.	Pressure Rating, Standard: 56 psi max. Test Pressure: 74 psi max.
a.	Minimum Wall Thickness: 0.048 inch.
13.	Pressure Rating, High: 128 psi max. Test Pressure: 184 psi max.
a.	Minimum Wall Thickness: 0.078 inch.
14.	Ribbed pipe cover trims, finished to match the radiators, provided with the radiation.
15.	Combination shutoff valve/union fitting of less than two inches in width for the supply and return to each panel radiator, to be field installed by others.
16.	Runtal-Flex Connectors: To be used where appropriate to provide expansion compensation for the radiators.
17.	Avg Water Temp: 180 degrees F.
18.	Model: HX7. Width: 2.7 inches. Depth: 2 inches. BTUH/ft: 140.
19.	Model: HX14. Width: 5.7 inches. Depth: 2 inches. BTUH/ft: 280.
20.	Model: HX21. Width: 8.6 inches. Depth: 2 inches. BTUH/ft: 420.
21.	Model: HX28. Width: 11.5 inches. Depth: 2 inches. BTUH/ft: 560.
22.	Model: HX35. Width: 14.3 inches. Depth: 2 inches. BTUH/ft: 700.
23.	Model: HX42. Width: 17.3 inches. Depth: 2 inches. BTUH/ft: 840.
24.	Model: HX49. Width: 20.3 inches. Depth: 2 inches. BTUH/ft: 980.
25.	Model: HX56. Width: 23.1 inches. Depth: 2 inches. BTUH/ft: 1120.
26.	Model: HX63. Width: 26.1 inches. Depth: 2 inches. BTUH/ft: 1260.
27.	Model: HX70. Width: 29.0 inches. Depth: 2 inches. BTUH/ft: 1400.
D.	Basis of Design: Made-to-Order Steel Panel Column Radiators: Model R Series. Evenly spaced, vertical flat tubing. Allows light to pass through. Dual function as full-height room dividers, balustrades, or knee walls. Higher BTU output than flat-orientation radiators.
1.	Tubes running vertically from floor to ceiling. Can be recessed into the wall to clear door swings.
2.	Built to order. Length: 6 inches to 20 ft.
3.	Construction: Cold rolled low carbon welded steel, one piece. A pair of flattened water tube panels welded to headers at each end.
4.	Finish: Gloss powder coat. Color: ________. Paint Thickness: 2 to 3 mils.
5.	Mounting: Wall. Support blocking for radiator mounting to be by others.
6.	Mounting: Free standing. Floor posts required.
7.	Panel Thermal Expansion: Not to exceed 1/64 inch per ft at 215 degrees F AWT.
a.	Expansion Compensation: Provided in the piping as required, by others.
8.	Header Pipes: Round 0.072 inches minimum wall thickness. Include necessary supply, return, and air vent connections. Internal baffling as required.
9.	Piping Connections: Inlet and Outlet: 1/2 inch NPT. Vents: 1/8 inch NPT.
10.	Pressure Rating, Standard: 56 psi max. Test Pressure: 74 psi max.
a.	Minimum Wall Thickness: 0.048 inch.
11.	Pressure Rating, High: 128 psi max. Test Pressure: 184 psi max.
a.	Minimum Wall Thickness: 0.078 inch.
12.	Combination shutoff valve/union fitting of less than two inches in width for the supply and return to each panel radiator, to be field installed by others.
13.	Runtal-Flex Connectors: To be used where appropriate to provide expansion compensation for the radiators.
14.	Model: R1040-2. Height: 15.9 inches. Depth: 4 inches. BTUH/ft: 960.
15.	Model: R1060-2. Height: 23.6 inches. Depth: 4 inches. BTUH/ft: 1320.
16.	Model: R1075-2. Height: 29.5 inches. Depth: 4 inches. BTUH/ft: 1620.
17.	Model: R1090-2. Height: 35.6 inches. Depth: 4 inches. BTUH/ft: 1860.
18.	Model: R1200-2. Height: 78.8 inches. Depth: 4 inches. BTUH/ft: 4380.
19.	Model: R1215-2. Height: 84.6 inches. Depth: 4 inches. BTUH/ft: 4740.
E.	Basis of Design: Made-to-Order Curved and Segmented Single Panel Radiators. To follow architectural walls.
1.	Radiator length must be ordered by arc length.
2.	Mounting: Clip or Strap.
3.	Factory Curved: Concave and convex curves.
a.	Non-Finned Models: Min Radius: 5 ft. Max Length: 20 ft.
b.	Finned Models: Min Radius: 10 ft. Max Length: 16 ft.
4.	Field Curved: Concave and convex curves. Suit larger curvatures.
a.	Minimum Radius: 15 ft. Minimum Length: 15 ft.
F.	Basis of Design: Made-to-Order High Output Radiators. Model VLX-2. 5-year limited warranty.
1.	Built to order. Length: 2 to 29.5 ft in 2 inch increments.
2.	Construction: Cold rolled welded steel one piece. Flattened water tubes welded to headers at each end.
a.	Top Grille: 0.09 inch thick minimum, all-welded perforated.
3.	Finish: Gloss powder coat. Color: ________. Paint Thickness: 2 to 3 mils.
4.	Mounting: Wall. Support blocking for radiator mounting to be by others.
5.	Mounting: Free standing. Floor posts required.
6.	Panel Thermal Expansion: Not to exceed 1/64 inch per ft at 215 degrees F AWT.
7.	Piping Connections: Inlet and Outlet: 1/2 inch NPT. Vents: 1/8 inch NPT.
8.	Pressure Rating, Standard: 56 psi max. Test Pressure: 74 psi max.
a.	Minimum Wall Thickness: 0.048 inch.
9.	Pressure Rating, High: 128 psi max. Test Pressure: 184 psi max.
a.	Minimum Wall Thickness: 0.078 inch.
10.	Ribbed pipe cover trims, finished to match the radiators, provided with the radiation.
11.	Combination shutoff valve/union fitting of less than two inches in width for the supply and return to each panel radiator, to be field installed by others.
12.	Runtal-Flex Connectors: To be used where appropriate to provide expansion compensation for the radiators.
13.	Model with Fins: VLX 7/7-2. Height: 2.8 inches Depth: 4.8 inches.
a.	Avg Water Temp of 215 degrees F: BTUH/ft at 65 degrees F, EAT: 1300.
b.	Avg Water Temp of 180 degrees F: BTUH/ft at 65 degrees F, EAT: 920.
c.	Avg Water Temp of 140 degrees F: BTUH/ft at 65 degrees F, EAT: 530.
14.	Model with Fins: VLX 14/14-2. Height: 5.7 inches Depth: 4.8 inches.
a.	Avg Water Temp of 215 degrees F: BTUH/ft at 65 degrees F, EAT: 2020.
b.	Avg Water Temp of 180 degrees F: BTUH/ft at 65 degrees F, EAT: 1420.
c.	Avg Water Temp of 140 degrees F: BTUH/ft at 65 degrees F, EAT: 820.
15.	Model with Fins: VLX 21/21-2. Height: 8.6 inches Depth: 52 inches.
a.	Avg Water Temp of 215 degrees F: BTUH/ft at 65 degrees F, EAT: 2580.
b.	Avg Water Temp of 180 degrees F: BTUH/ft at 65 degrees F, EAT: 1810.
c.	Avg Water Temp of 140 degrees F: BTUH/ft at 65 degrees F, EAT: 1040.
16.	Model with Fins: VLX 28/28-2. Height: 11.5 inches Depth: 2 inches.
a.	Avg Water Temp of 215 degrees F: BTUH/ft at 65 degrees F, EAT: 3090.
b.	Avg Water Temp of 180 degrees F: BTUH/ft at 65 degrees F, EAT: 2170.
c.	Avg Water Temp of 140 degrees F: BTUH/ft at 65 degrees F, EAT: 1250.
17.	Model with Fins: VLX 35/35-2. Height: 14.4 inches Depth: 2 inches.
a.	Avg Water Temp of 215 degrees F: BTUH/ft at 65 degrees F, EAT: 3790.
b.	Avg Water Temp of 180 degrees F: BTUH/ft at 65 degrees F, EAT: 2670.
c.	Avg Water Temp of 140 degrees F: BTUH/ft at 65 degrees F, EAT: 1530.
18.	Model with Fins: VLX 42/42-2. Height: 17.2 inches Depth: 2 inches.
a.	Avg Water Temp of 215 degrees F: BTUH/ft at 65 degrees F, EAT: 4270.
b.	Avg Water Temp of 180 degrees F: BTUH/ft at 65 degrees F, EAT: 3000.
c.	Avg Water Temp of 140 degrees F: BTUH/ft at 65 degrees F, EAT: 1720.
19.	Model with Fins: VLX 49/49-2. Height: 20.2 inches Depth: 2 inches.
a.	Avg Water Temp of 215 degrees F: BTUH/ft at 65 degrees F, EAT: 4738.
b.	Avg Water Temp of 180 degrees F: BTUH/ft at 65 degrees F, EAT: 3335.
c.	Avg Water Temp of 140 degrees F: BTUH/ft at 65 degrees F, EAT: 1909.
20.	Model with Fins: VLX 56/56-2. Height: 23.1 inches Depth: 2 inches.
a.	Avg Water Temp of 215 degrees F: BTUH/ft at 65 degrees F, EAT: 5200.
b.	Avg Water Temp of 180 degrees F: BTUH/ft at 65 degrees F, EAT: 3660.
c.	Avg Water Temp of 140 degrees F: BTUH/ft at 65 degrees F, EAT: 2095.
21.	Model with Fins: VLX 63/56-2. Height: 26.1 inches Depth: 2 inches.
a.	Avg Water Temp of 215 degrees F: BTUH/ft at 65 degrees F, EAT: 5451.
b.	Avg Water Temp of 180 degrees F: BTUH/ft at 65 degrees F, EAT: 3836.
c.	Avg Water Temp of 140 degrees F: BTUH/ft at 65 degrees F, EAT: 2196.
22.	Model with Fins: VLX 70/56-2. Height: 29.0 inches Depth: 2 inches.
a.	Avg Water Temp of 215 degrees F: BTUH/ft at 65 degrees F, EAT: 5691.
b.	Avg Water Temp of 180 degrees F: BTUH/ft at 65 degrees F, EAT: 4005.
c.	Avg Water Temp of 140 degrees F: BTUH/ft at 65 degrees F, EAT: 2293.
G.	Basis of Design: Made-to-Order Hot Spring. Vertical installation only.
1.	For closed loop systems only. Not for use with domestic hot water systems.
2.	Working Pressure: 100 psi maximum.
3.	Working Temperature: 200 degrees F Maximum.
4.	Model: HOT 60. Height: 25.6 inch. Dia: 7.8 inch. Depth: 11.00 inch. BTUH: 1975.
5.	Model: HOT 180. Height: 72.8 inch. Dia: 7.8 inch. Depth: 11.00 inch. BTUH: 6681.
6.	Finish: Painted. 16 to 156 inches in 2 inch increments. Color: White.
7.	Finish: Painted. 16 to 156 inches in 2 inch increments. Color: Metallica.
8.	Finish: Chrome. 16 to 80 inches in 2 inch increments.
a.	Chrome finish reduces radiator output by 20 percent.
H.	Basis of Design: Made-to-Order Steam Flow Form. Fins arranged in a spiral around the heating tube radiate heat efficiently throughout the room.
1.	For two-pipe steam systems only.
2.	Construction: Stainless steel.
3.	Finish: Chrome Plated. Chrome plating will drop BTUH by 12 percent.
4.	Mounting: Floor. Pedestals. Tilt Toward Condensate Return: 1/16 inch per foot.
5.	Average Supply Hydronic Water Temperature: 180 degrees F.
6.	Height: 7.5 inches. Diameter: 5.2 inches.
7.	Supply Side: Control Valve. 1 inch NPT.
8.	Return Side: Steam trap. 1/2 inch NPT.
9.	Model XFF 100: Length: 39.4 inches. BTUH: 2553.
10.	Model XFF 150: Length: 59.1 inches. BTUH: 3920.
11.	Model XFF 200: Length: 78.8 inches. BTUH: 5288.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until the substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
B.	Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
3.5	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturer's recommendations.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION