SECTION 32 31 23 - Plastic Fences and Gates

VINYL FENCING AND GATES

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2017 -  2025 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Vinyl Fencing:
1.	Picket fence systems.
2.	Yard fence systems.
3.	Privacy fence systems.
4.	Post and rail fence systems.
B.	Post caps.
C.	Pergolas.
1.2	RELATED SECTIONS
A.	Section 02 20 00 - Assessment.
B.	Section 03 30 00 - Cast-in-Place Concrete.
1.3	REFERENCES
A.	ASTM D 1784 - Standard Specification for Rigid Poly(Vinyl Chloride) (PVC) Compounds and Chlorinated Poly (Vinyl Chloride) (CPVC) Compounds.
1.4	DESIGN / PERFORMANCE REQUIREMENTS
A.	Provide pool fencing to meet applicable code requirements.
1.5	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings: Submit shop drawings for each product and accessory required. Include information not fully detailed in manufacturer's standard product data.
D.	Selection Samples: For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.
E.	Verification Samples: For each finish product specified, two samples, minimum size 3 inches (76 mm) square, representing actual product, color, and patterns.
F.	Manufacturer's Certificates: Certify products meet or exceed specified requirements.
G.	Closeout Submittals: Provide manufacturer's maintenance instructions that include recommendations for periodic cleaning and maintenance of all components.
1.6	QUALITY ASSURANCE
A.	Manufacturer Qualifications: A firm engaged in the manufacture of vinyl fence and gates of types and sizes specified, and whose products have been in satisfactory use in similar service for a minimum of five years.
B.	Installer Qualifications: A firm with a minimum of two years of successful installation experience with projects utilizing vinyl fence and gates similar in type and scope to that required for this Project.
C.	Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
1.	Finish areas designated by Architect.
2.	Do not proceed with the remaining work until workmanship, color, and sheen are approved by Architect.
3.	Refinish mock-up area as required to produce acceptable Work.
4.	Accepted mock-ups shall be a comparison standard for remaining Work.
D.	Pre-Installation Conference: Conduct pre-installation conference in accordance with Section 01 20 00 - Price and Payment Procedures. The date and time of the pre-installation conference shall be acceptable to the Owner and the Architect.
1.	Prior to commencing the installation, meet at the Project site to review the material selections, installation procedures, and coordination with other trades.
2.	Mock-ups are to be reviewed during the pre-installation conference.
3.	Pre-installation conference shall include the Contractor, the Installer, and any trade that requires coordination with the work.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Deliver materials to the Project site in manufacturer's original wrappings and containers, labeled with supplier's or manufacturer's name, material or product brand name, and lot number, if any.
B.	Store materials in their original, undamaged packages and containers, inside a well-ventilated area protected from weather, moisture, soiling, extreme temperatures, and humidity.
1.8	SEQUENCING
A.	Ensure that locating templates and other information required for installation of products of this section are furnished to affected trades in time to prevent interruption of construction progress.
B.	Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
1.9	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
1.10	WARRANTY
A.	Lifetime Limited, Non-Prorated Warranty on Material and 5 Year Prorated Labor Warranty.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Superior Outdoor Products, which is located at:<BR />260 Jalyn Dr.<BR />New Holland, PA 17557<BR />Toll Free Tel: 800-633-7093<BR />Tel: 717-355-7100<BR />Fax: 717-355-7129<BR />Email: request info (info@superioroutdoors.com);Web: https://superioroutdoors.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with the provisions of Section 01 60 00 - Product Requirements.
2.2	MATERIALS
A.	PVC: Poly Vinyl Chloride (PVC) formulated to resist impact and for Ultraviolet (UV) stabilization. Extruded products meet or exceed ASTM D I784.
2.3	PICKET FENCE SYSTEMS
A.	Style: Classic. 1-1/2 inch (38 mm) picket fence.
1.	Style: Straight.
2.	Style: Concave.
3.	Height: 36 inch (914 mm).
4.	Height: 48 inch (1219 mm).
5.	Height: 57 inch (1448 mm). Pool.
6.	Notched Pickets: 7/8 x 1-1/2 inch (22 x 38 mm). Max Spacing: 2-1/8 inch (54 mm).
7.	Rails: 1-3/4 by 3-1/2 inch (44 x 89 mm). Routed.
8.	Rail Section: 6 foot (1829 mm).
9.	Rail Section: 8 foot (2436 mm).
10.	Posts: 4 inch (101 mm).
11.	Post Caps: 4 inch (101 mm). Flat.
12.	Post Caps: 4 inch (101 mm) Spade.
13.	Gates and Posts: Match fence style.
14.	Color: White.
15.	Color: Almond.
16.	Color: Clay.
17.	Color: Black.
B.	Style: Classic. 3 inch picket fence.
1.	Style: Straight.
2.	Style: Concave.
3.	Height: 36 inch (914 mm).
4.	Height: 48 inch (1219 mm).
5.	Height: 57 inch (1448 mm). Pool.
6.	Notched Pickets: 7/8 x 3 inch (22 x 76 mm). Max Spacing: 3-1/4 inch (83 mm).
7.	Rails: 1-3/4 by 3-1/4 inch (44 x 83 mm). Routed.
8.	Rail Section: 6 foot (1829 mm).
9.	Rail Section: 8 foot (2436 mm).
10.	Posts: 4 inch (101 mm).
11.	Post Caps: 4 inch (101 mm). Flat.
12.	Post Caps: 4 inch (101 mm). Spade.
13.	Gates and Posts: Match fence style.
14.	Color: White.
15.	Color: Almond.
16.	Color: Clay.
17.	Color: Black.
C.	Style: Columbia picket fence.
1.	Style: Straight.
2.	Style: Concave.
3.	Height: 36 inch (914 mm).
4.	Height: 48 inch (1219 mm).
5.	Height: 57 inch (1448 mm). Pool.
6.	Notched Pickets: 7/8 x 3 inch (22 x 76 mm). Max Spacing: 3-1/4 inch (83 mm).
7.	Rails: 1-3/4 by 3-1/2 inch (44 x 89 mm). Routed.
8.	Rail Section: 6 foot (1829 mm).
9.	Rail Section: 8 foot (2436 mm).
10.	Posts: 4 inch (101 mm).
11.	Post Caps: 4 inch (101 mm). Flat.
12.	Post Caps: 4 inch (101 mm). Spade.
13.	Gates and Posts: Match fence style.
14.	Color: White.
15.	Color: Almond.
16.	Color: Clay.
17.	Color: Black.
D.	Style: New England. 1-1/2 inch (38 mm) picket fence.
1.	Style: Straight.
2.	Style: Concave.
3.	Height: 36 inch (914 mm).
4.	Height: 48 inch (1219 mm).
5.	Notched Pickets: 1-1/2 inch (38 mm) square. Max Spacing: 1-3/4 inch (44 mm).
6.	Rails:
a.	Top Rail: 2 by 4 inch (51 x 102 mm). Routed.
b.	Bottom Rail: 2 by 6 inch (51 x 152 mm), routed.
7.	Rail Section: 6 foot (1829 mm).
8.	Rail Section: 8 foot (2436 mm).
9.	Posts: 5 inch (127 mm).
10.	Post Caps: 5 inch (127 mm) Flat.
11.	Post Caps: 5 inch (127 mm). New England.
12.	Gates and Posts: Matching fence style.
13.	Color: White.
14.	Color: Almond.
15.	Color: Clay.
2.4	YARD FENCE SYSTEMS
A.	Style: Baron Yard Fence.
1.	Height: 36 inch (914 mm).
2.	Height: 48 inch (1219 mm). Pool.
3.	Height: 60 inch (1524 mm). Pool. Midrail required.
4.	Height: 72 inch (1829 mm). Pool. Midrail required.
5.	Rail Section: 6 foot (1829 mm).
6.	Rail Section: 8 foot (2436 mm).
7.	Notched Pickets: 7/8 inch 3 inch (22 x 76 mm) maximum spacing 3-1/4 inch (83
8.	mm).
9.	Rails: 1-3/4 by 3-1/2 inch (44 x 89 mm) routed.
10.	Posts: 4 inch (101 mm).
11.	Post Caps: 4 inch (101 mm). Flat.
12.	Post Caps: 4 inch (101 mm.) New England.
13.	Gates: Match fence style.
14.	Color: White.
15.	Color: Almond.
16.	Color: Clay.
B.	Style: Imperial Yard Fence.
1.	Height: 36 inch (914 mm). Posts: 4 inch (101 mm).
2.	Height: 48 inch (1219 mm). Pool. Posts: 4 inch (101 mm).
3.	Height: 60 inch (1524 mm). Pool. Posts: 5 inch (127 mm). Midrail required.
4.	Height: 72 inch (1829 mm) Pool. Posts: 5 inch (127 mm). Midrail required.
5.	Rail Section: 6 foot (1829 mm).
6.	Rail Section: 8 foot (2436 mm).
7.	Pickets: 7/8 by 3 inch (22 by 76 mm). Max Spacing: 11/16 inch (17 mm).
8.	Picket Orientation: Vertical.
9.	Picket Orientation: Horizontal.
10.	Rails: 1-3/4 by 3-1/2 inch (44 x 89 mm) routed.
11.	Post Caps: 4 inch (101 mm). Flat.
12.	Post Caps: 4 inch (101 mm). New England.
13.	Post Caps: 5 inch (127 mm). Flat.
14.	Post Caps: 5 inch (127 mm). New England.
15.	Gates: Match fence style.
16.	Color: White.
17.	Color: Almond.
18.	Color: Clay.
19.	Color: Black.
20.	Color: Slate.
21.	Color: White / Slate.
22.	Color: Clay / Almond.
23.	Color: Black / Slate.
24.	Color: Almond / White.
25.	Color: Black / White.
C.	Style: Model Yard Fence.
1.	Height: 48 inch (1219 mm). Pool.
2.	Rail Section: 6 foot (1829 mm).
3.	Rail Section: 8 foot (2436 mm).
4.	Rails: 1-3/4 by 3-1/2 inch (44 x 89 mm) routed.
5.	Posts: 4 inch (101 mm).
6.	Post Caps: 4 inch (101 mm). Flat.
7.	Post Caps: 4 inch (101 mm) New England.
8.	Gates: Match fence style.
9.	Color: White.
10.	Color: Almond.
11.	Color: Clay.
12.	Color: Black.
2.5	PRIVACY FENCE SYSTEMS
A.	Style: Boston Privacy Fence.
1.	Height: 48 inch (1219 mm).
2.	Height: 60 inch (1524 mm). Pool.
3.	Height: 60 inch (1524 mm) with Lattice. Pool.
4.	Height: 66 inch (16766 mm) with New England Accent. Pool.
5.	Height: 72 inch (1829 mm). Pool.
6.	Height: 72 inch (1829 mm) with Lattice. Pool.
7.	Height: 84 inch (2134 mm). Pool. Midrail required.
8.	Height: 84 inch (2134 mm) with Lattice. Pool. Midrail required.
9.	Height: 96 inch (2438 mm). Pool. Midrail required.
10.	Height: 96 inch (2438 mm) with Lattice. Pool. Midrail required.
11.	Rail Section: 6 foot (1829 mm).
12.	Rail Section: 8 foot (2436 mm).
13.	Deco Rails: 2 by 6-1/2 inch (51 by 165 mm).
14.	Tongue and Groove Panels: 7/8 by 8-1/2 inch (22 by 216 mm) with 4 inch (102 mm) appearance.
15.	Posts: 5 inch (127 mm).
16.	Post Caps: 5 inch (127 mm). Flat.
17.	Post Caps: 5 inch (127 mm). New England.
18.	Gates and Posts: Matching fence style.
19.	Color: White.
20.	Color: Almond.
21.	Color: Clay.
B.	Style: Cambridge Privacy Fence. Smooth.
1.	Height: 46 inch (1168 mm).
2.	Height: 48 inch (1219 mm).
3.	Height: 54-1/2 inch (1384 mm). Pool.
4.	Height: 56-1/2 inch (1435 mm). Pool.
5.	Height: 60 inch (1524 mm). Pool.
6.	Height: 70 inch (1778 mm). Pool.
7.	Height: 70 inch (1778 mm) with Lattice. Pool.
8.	Height: 72 inch (1829 mm). Pool.
9.	Height: 72 inch (1829 mm) with Lattice. Pool.
10.	Height: 84 inch (2134 mm). Pool.
11.	Height: 96 inch )2438 mm). Pool.
12.	Rail Section: 8 foot (2436 mm).
13.	Rails: Top and Bottom Horizontals: 1-1/2 by 5-1/2 inch (38 by 140 mm).
a.	Height: 46 inch (1168 mm).
b.	Height: 54-1/2 inch (1384 mm).
c.	Height: 70 inch (1778 mm).
14.	Rails: Top and Bottom Horizontal: 2 by 6-1/2 inch (51 x 165 mm).
a.	Height: 48 inch (1219 mm).
b.	Height: 60 inch (1524 mm).
c.	Height: 72 inch (1829 mm).
15.	Rails: Top and Bottom Horizontal Deco: 2 by 7 inch (51 x 178 mm).
a.	Height: 48 inch (1219 mm).
b.	Height: 56-1/2 inch (1435 mm).
c.	Height: 72 inch (1829 mm).
d.	Height: 84 inch. Midrail required.
e.	Height: 96 inch. Midrail required.
16.	Vertical Panels: 3/4 by 10 inch 19 x 254 mm) interlocking.
17.	Posts: 5 inch (127 mm).
18.	Post Caps: 5 inch (127 mm). Flat.
19.	Post Caps: 5 inch (127 mm). New England.
20.	Gates and Posts: Match fence style.
21.	Color: White.
22.	Color: Almond.
23.	Color: Clay.
24.	Color: Black.
25.	Color: Slate.
26.	Color: White / Slate.
27.	Color: Clay / Almond.
28.	Color: Black / Slate.
29.	Color: Almond / White.
30.	Color: Black / White.
2.6	POST AND RAIL FENCE SYSTEMS
A.	Style: Post and Rail Sections.
1.	Height: 34-1/2 inch (876 mm).
2.	Height: 48 inch (1219 mm).
3.	Height: 57 inch (1448 mm).
4.	Rail Count: 2.
5.	Rail Count: 3.
6.	Rail Count: 4.
7.	Section width: 8 foot (2436 mm).
8.	Rail: 1-1/2 by 5-1/2 inch (38 x 140 mm).
a.	Fence Color: White.
b.	Fence Color: Almond.
9.	Rail: 2 by 6 inch (51 by 152 mm).
a.	Fence Color: Clay.
b.	Fence Color: Black.
c.	Fence Color: Slate.
10.	Posts: 5 inch (127 mm).
11.	Post Caps: 5 inch (127 mm). Flat.
12.	Post Caps: 5 inch (127 mm). New England.
13.	Gates: Match fence style.
2.7	POST CAPS
A.	Vinyl Post Caps:
1.	Style: 4 inch (101 mm) Flat. Color: White.
2.	Style: 4 inch (101 mm) Flat. Color: Almond.
3.	Style: 4 inch (101 mm) Flat. Color: Clay.
4.	Style: 4 inch (101 mm) Flat. Color: Black.
5.	Style: 4 inch (101 mm) New England. Color: White.
6.	Style: 4 inch (101 mm) New England. Color: Almond.
7.	Style: 4 inch (101 mm) New England. Color: Clay.
8.	Style: 4 inch (101 mm) New England. Color: Black.
9.	Style: 4 inch (101 mm) New York. Color: White.
10.	Style: 4 inch (101 mm) New York. Color: Almond.
11.	Style: 4 inch (101 mm) New York. Color: Clay.
12.	Style: 4 inch (101 mm) Spade. Color: White.
13.	Style: 4 inch (101 mm) Spade. Color: Almond.
14.	Style: 4 inch (101 mm) Spade. Color: Clay.
15.	Style: 4 inch (101 mm) Spade. Color: Black.
16.	Style: 4 inch (101 mm) Ball. Color: White.
17.	Style: 4 inch (101 mm) Ball. Color: Almond.
18.	Style: 4 inch (101 mm) Ball. Color: Clay.
19.	Style: 4 inch (101 mm) Queen. Color: White.
20.	Style: 4 inch (101 mm) Queen. Color: Almond.
21.	Style: 4 inch (101 mm) Queen. Color: Clay.
22.	Style: 4 inch (101 mm) King. Color: White.
23.	Style: 4 inch (101 mm) King. Color: Almond.
24.	Style: 4 inch (101 mm) King. Color: Clay.
25.	Style: 5 inch (127 mm) Flat. Color: White.
26.	Style: 5 inch (127 mm) Flat. Color: Almond.
27.	Style: 5 inch (127 mm) Flat. Color: Clay.
28.	Style: 5 inch (127 mm) Flat. Color: Black.
29.	Style: 5 inch (127 mm) New England. Color: White.
30.	Style: 5 inch (127 mm) New England. Color: Almond.
31.	Style: 5 inch (127 mm) New England. Color: Clay.
32.	Style: 5 inch (127 mm) Spade. Color: White.
33.	Style: 5 inch (127 mm) Spade. Color: Almond.
34.	Style: 5 inch (127 mm) Spade. Color: Clay.
35.	Style: 5 inch (127 mm) Ball. Color: White.
36.	Style: 5 inch (127 mm) Ball. Color: Almond.
37.	Style: 5 inch (127 mm) Ball. Color: Clay.
2.8	PERGOLAS
A.	Vinyl Pergolas:
1.	Size: 8 by 12 foot (2438 x 3658 mm).
2.	Size: 8 by 16 foot (2438 x 4877 mm).
3.	Size: 8 by 20 foot (2438 x 6096 mm).
4.	Size: 10 by 10 foot (3048 x 3048 mm).
5.	Size: 10 by 12 foot (3048 x 3658 mm).
6.	Size: 10 by 16 foot (3048 x 4877 mm).
7.	Size: 10 by 20 foot (3048 x 6096 mm).
8.	Size: 12 by 12 foot (3658 x 3658 mm).
9.	Size: 12 by 16 foot (3658 x 4877 mm).
10.	Size: 12 by 20 foot (3658 x 6096 mm).
11.	Size: 16 by 16 foot (4877 x 4877 mm).
12.	Size: 16 by 20 foot (4877 x 6096 mm).
13.	Support Column: Square Pergola Column: 6 inch (152 mm).
14.	Support Column: Tapered Round Column: 8 inch (203 mm).
15.	Support Column: Tapered Round Column: 10 inch (254 mm).
16.	Support Column: 8 inch (203 mm) Square Column: 8 inch (203 mm).
17.	Support Column: 8 inch (203 mm) Savannah Column: 8 inch (203 mm).
18.	Roof Style: Straight Rafters.
19.	Shade Cover Type: Square 1-1/2 inch (38 mm).
20.	Shade Cover Type: Square 1-3/4 inch (44 mm).
21.	Shade Cover Type: Lattice.
22.	Shade Cover Type: Louvered. 7/8 by 3 inch (22 x 76 mm).
23.	Color: White.
24.	Color: Almond.
25.	Color: Clay.
26.	Color: Black.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until conditions have been properly prepared.
B.	Verification of Conditions: Examine locations where fencing is to be installed for any conditions detrimental to the proper and timely completion of the work.
C.	If preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare the grade and remove surface irregularities, if any, which may cause interference with the installation of the fence.
C.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions.
B.	Set posts and gate posts for gate openings as indicated on the Drawings.
C.	Center and align posts, place concrete around posts and vibrate or tamp for consolidation. Recheck vertical and top alignment of posts and make necessary corrections.
D.	Install gates plumb, level, and secure for full opening without interference. For double gates, install a drop rod. Adjust hardware for smooth operation.
3.4	CLEANING
A.	Touch-up, repair, or replace damaged products before Substantial Completion.
B.	Clean the work according to the manufacturer's written instructions. Post hole excavations shall be scattered uniformly away from the posts. Clean fence with mild household detergent and rinse well with clean water. Remove mortar from exposed posts using a 10 percent solution of muriatic acid followed immediately by several rinses with clean water.
3.5	PROTECTION
A.	Protect installed products until completion of the project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION