SECTION 12 20 00

WINDOW TREATMENTS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2012 -  2014 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Interior Solar Shading Systems: 
1.	Manual solar shades. (SWFcontract)
2.	Manual shade system. (Pro Series)
3.	Motorized solar shades. (SWFcontract)
B.	Interior Window Coverings: 
1.	Aluminum horizontal mini blinds. (Bali S3000 1 inch)
2.	Aluminum horizontal mini blinds. (Bali Classics 1 inch)
3.	Aluminum horizontal mini blinds. (Bali CustoMiser 1 inch)
4.	Aluminum horizontal mini blinds. (Bali Apartment)
5.	Aluminum horizontal micro blinds. (Bali S4000)
6.	Aluminum horizontal micro blinds. (Bali)
7.	Aluminum horizontal blinds. (Bali Heritage 2 inch)
8.	Aluminum horizontal school blinds. (Bali 2 inch School)
9.	Designer vinyl blinds. (Graber 2 inch)
10.	Wood horizontal blinds. (Graber Elite Woods 2 inch)
11.	Wood horizontal blinds. (Graber Traditions 1 inch)
12.	Wood horizontal blinds. (Graber Traditions 2 inch)
13.	Faux wood blinds. (Graber Lake Forest)
14.	Vertical blinds. (SWFcontract G-98 Ultra-Vue Vertical Blinds)
15.	Vertical blinds. (SWFcontract G-71 Super-Vue Vertical Blinds)
16.	Vertical blinds. (SWFcontract G-85 Dura-Vue Vertical Blinds)
17.	Cellular shades. (SWFcontract CrystalPleat 3/8 inch Double Cell)
18.	Cellular shades. (SWFcontract CrystalPleat 3/8 inch Single Cell)
19.	Cellular shades. (SWFcontract CrystalPleat 3/4 inch Single Cell)
20.	Pleated shades. (SWFcontract EvenPleat)
21.	Pleated shades. (SWFcontract FashionPleat)
1.2	RELATED SECTIONS
A.	Section 06 10 00 - Rough Carpentry.
B.	Section 09 21 16.23 - Gypsum Board Shaft Wall Assemblies.
C.	Section 09 51 23 - Acoustical Tile Ceilings.
D.	Section 09 90 00 - Painting and Coating.
E.	Division 16 - Electrical.
1.3	REFERENCES
A.	ASTM International (ASTM):
1.	ASTM E 21 - Standard Test Method for Elevated Temperature Tension Tests of Metallic Materials.
2.	ASTM E 22 - Recommended Practice for Conducting Long Time High Temperature Tension Test of Metallic Materials.
3.	ASTM G 21 - Standard Practice for Determining Resistance of Synthetic Polymeric Materials to Fungi. 
4.	ASTM G 22 - Standard Practice for Determining Resistance of Plastics to Bacteria. 
B.	National Fire Protection Association (NFPA):
1.	NFPA 70 - National Electrical Code.
2.	NFPA 701 - Fire Tests for Flame-Resistant Textiles and Films.
C.	Underwriters Laboratories Inc. (UL). 
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data:  Submit manufacturer's product data sheets, including installation details, styles, material descriptions, profiles, features, finishes and operating instructions.
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Mounting details and Installation methods.
4.	Typical wiring diagrams if applicable.
C.	Shop Drawings: Submit manufacturer's shop drawings, including plans, elevations, sections, product details and finishes, installation details, operational clearances, wiring diagrams if applicable, and relationship to adjacent work.
D.	Window Treatment Schedule: Submit a schedule with same room designations indicated on the Drawings; including but not limited to opening sizes and key to typical mounting details.
E.	Maintenance Data: Submit instructions and precautions for cleaning and maintenance, operating hardware and controls as applicable.
F.	Selection Samples: 
1.	Frame and Component Finishes:  Submit 2 sets of samples, representing manufacturerï¿½s standard range of finishes specified for aluminum. 
2.	Fabric:  Submit 2 sets of samples, representing manufacturerï¿½s standard range of options for shade cloth.
3.	Aluminum Slats:  Submit 2 sets of samples, 6 inches long, representing manufacturerï¿½s standard range of finishes specified for aluminum slats.
G.	Verification Samples: 
1.	Frame and Component Finishes:  Submit 2 samples, representing actual finishes specified for aluminum. 
2.	Fabric:  Submit 2 samples, representing actual products specified for shade cloth.
3.	Aluminum Slats:  Submit 2 sets of samples, 6 inches long, representing actual finishes specified for aluminum slats.
1.5	QUALITY ASSURANCE
A.	Manufacturer's Qualifications:  Engaged in manufacturing of products of similar type to that specified, with a minimum of 10 years successful experience.
B.	Installer Qualifications: Minimum 2 years successful experience installing similar products.
C.	Single Source Requirements: To the greatest extent possible, provide products specified in this section from a single manufacturer.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Delivery: Deliver materials to site protected from damage.
B.	Storage: Store materials in clean, dry area indoors in manufacturer's unopened packaging until ready for installation and in accordance with manufacturer's instructions. Store in a clean, dry area, laid flat to prevent sagging and twisting of packaging.
C.	Handling: Protect materials and finish from damage during handling and installation.
1.7	PROJECT CONDITIONS, COORDINATION AND SEQUENCING
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.	Building shall be enclosed; windows, frames and sills shall be installed and glazed.
2.	Wet work shall be complete and dry.
3.	Ceilings, window pockets, electrical and mechanical work above window covering shall be complete.
B.	Conference: Convene a pre-installation conference to establish procedures to maintain optimum working conditions and to coordinate this work with related and adjacent work.
1.8	TYPE OF WARRANTY
A.	Manufacturer's Warranty:
1.	Provide Limited lifetime warranty on all Baliï¿½, Graberï¿½ and SWFcontractï¿½ products sold by SWF or by an authorized dealer, other than the products listed below, which have the limited warranty periods as indicated:
2.	2" vinyl and acrylic slats: Three years
3.	Drapery hardware: Three years
4.	FashionPleat pleated shade fabrics: Three years
5.	Vertical louvers (vanes): Three years
6.	Motorization components & accessories (batteries not included): Five years
1.9	EXTRA MATERIALS
A.	Attic Stock: Provide two extra blinds of primary size used for Owner's replacement stock.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: SWFcontract, which is located at:<BR />7549 Graber Rd.<BR />Middleton, WI  53562-1096 <BR />Toll Free Tel: 800-327-9798<BR />Email: request info (architectsolutions@swfcontract.com);Web: https://www.swfcontract.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	SHADING SYSTEMS - GENERAL 
A.	Shade Configuration:  As scheduled and indicated on Drawings. 
B.	Shade Configuration:  Single shades as scheduled and indicated on Drawings. 
C.	Shade Configuration:  Dual shades as scheduled and indicated on Drawings. 
D.	Shade Configuration:  Coupled shades as scheduled and indicated on Drawings.
2.3	MANUALLY OPERATED SOLAR SHADING SYSTEMS
A.	Shading Systems: SWFcontract Manual Solar Shades as manufactured by SWFcontract.
B.	Fabric:  Flame retardant, fade and stain resistant, anti-microbial.
1.	Style: ____________.
2.	Color Name: ____________.
3.	Color Number: ____________.
4.	Fabric Style, Color Name, Color Number:  As scheduled and indicated on Drawings.
5.	Fabric Style, Color Name, Color Number:  As selected by Architect from manufacturerï¿½s standard fabric range.
C.	Components: Fabricate such that shade hangs flat without buckling or distortion.
1.	TruePerformance Clutch Systems:
a.	Clutch System: TruePerformance Clutch System from SWFcontract consisting of fiberglass filled nylon for wear resistance, smooth operation and corrosion resistance. The clutch is comprised Velvetrol internal spring arrangement for a smooth pulling force that locks the shade in any position when operating the control loop. The clutch mechanism is bi-directional and does not require adjustment or lubrication. Clutch to be factory installed in roller tube at manufacturing. Clutch size to be selected by manufacturer based on fabric selection and shade size.
2.	Control Loops: Bead stops attached to the chain protect shade from over rotation.
a.	Materials: Standard, No. 10 stainless steel bead chain. 
b.	Materials:  Provide optional plastic bead chain, color ____________.
3.	Roller Tubes: Extruded-aluminum tubes engineered with a chamfered channel to accept fabric spline and allow fabric to lay across the tube without adding crease lines. The diameter and wall thickness to be determined by manufacturer based on fabric selection and shade size to provide minimal deflection and optimal performance.
4.	Idler Ends:  high strength, fiberglass-filled nylon with spring-loaded pin-end technology
5.	Lift Assist Systems: Heavy-duty torsion spring located inside the roller tube. The mechanism reduces the pull force allowing easy lifting of larger shades. 
6.	Spline Systems:  Consist of PVC spline heat-welded to the shade fabric and inserted into a channel on the roller tube. Tape and other methods of attachment are not acceptable.
7.	Hem Bars:  Standard, aluminum extrusion enclosed in a fabric hem pocket with heat-welded seams and ends, to coordinate with shade cloth selection.
8.	Hem Bars:  Provide optional fabric wrapped hem bar, to coordinate with shade cloth selection.
D.	Accessories:
1.	Fascia Panels: None.
2.	Fascia Panels:  Standard 3 inches (76 mm).
3.	Fascia Panels:  Standard 4 inches (102 mm). 
4.	Fascia Panels:  Back. 
5.	Fascia Panels: Dual shade snap-on design.
a.	Materials:  1/16 inches (1.6 mm) thick extruded 6063 T-5 aluminum alloy.
b.	Finish: White.
c.	Finish: Vanilla.
d.	Finish: Clear Anodized. 
e.	Finish: Bronze. 
f.	Finish: Black. 
g.	Size:  3 inches (76 mm). 
h.	Size:  4 inches (102 mm). 
i.	Size: 7-5/8 inches (194 mm).
6.	Shade Pockets: Manufacturer shall provide appropriate dimensional pocket as necessary to enclose roller tube and fabric. 
a.	Type: 4-3/4 inches (121 mm) x 5 inch (127 mm) extruded aluminum 6065 alloy.
b.	Finish:  White.
c.	Finish:  Clear Anodized.
d.	Finish:  Bronze Anodized.
e.	Type:  7-1/2 inches (191 mm) x 8 inches (203 mm) white powder coated steel.
7.	Closure Plates: Exposed, flush mounted, powder-coated extruded 6065-aluminum alloy designed to provide access to shades when recessed in ceiling. 
a.	Closure Mounts:  With a lip.
b.	Closure Mounts:  Without a lip.
c.	Plate Size: 2 inches (51 mm).
d.	Plate Size: 3 inches (76 mm).
e.	Plate Size: 5 inches (127 mm).
f.	Finish:  White.
g.	Finish:  Clear Anodized.
h.	Finish:  Bronze Anodized.
8.	Side, Sill, Center Channels: 2-piece design.
a.	Materials: Extruded 6065-aluminum.
b.	Size:  2 inch (51 mm) x 1 inch (25 mm), and 4 inch (102 mm) x 1 inch (25 mm) center channel is provided for coupled shades.
c.	Finish:  To Match Fascia Finish.
2.4	MANUAL SHADE SYSTEM 
A.	Shading Systems: Pro Series Manual Solar Shades as manufactured by SWFcontract. 
B.	Fabric:  Flame retardant, fade and stain resistant, anti-microbial. 
1.	Style: ____________. 
2.	Color Name: ____________. 
3.	Color Number: ____________. 
4.	Fabric Style, Color Name, Color Number:  As scheduled and indicated on Drawings. 
5.	Fabric Style, Color Name, Color Number:  As selected by Architect from manufacturer's standard fabric range. 
C.	Components: Fabricate such that shade hangs flat without buckling or distortion. 
1.	Features: 
a.	Smooth, quiet and consistent operation. 
b.	Built for commercial applications. 
c.	Works with large and coupled shades without motorization. 
d.	Overrunning-clutch-drive system. 
2.	Components: 
a.	Pro Series Clutch System:  High performance Acetal plastic components mounted on a heavy duty 1/8 inch (3 mm) thick steel stamping. 
1)	Universal Clutch Mechanism: 
a)	Shared between the drive end brackets of system comprises an internal heavy duty wrap spring and an actuator for a smooth pulling force that locks shade in any position when operating control loop. 
b)	Bidirectional and does not require adjustment or lubrication.   
b.	Idle End Bracket:  High-performance Acetal plastic components mounted on a heavy duty 1/8 inch (3 mm) thick steel stamping. 
1)	Intermediate Brackets:  High-performance Acetal plastic components mounted on a heavy duty 1/8 inch (3 mm) thick steel stamping providing support to coupled bands connected with an intermediate bracket mechanism. 
a)	The intermediate bracket mechanism for certain tube sizes shall have adjustability for shade bands alignment. 
c.	Roller Tube:  Extruded tempered aluminum alloy. Removable/replaceable "snap-on, snap-off" spline mounting. 
1)	Diameter and Wall Thickness:  Determined by manufacturer, based on fabric selection and shade size providing minimal deflection and optimal performance. 
d.	Drive Chain:  Special stainless steel bead chain. Bead stops attached to chain to protect shade from over-rotation. 
e.	Lift Assist System:  Heavy-duty torsion spring located inside roller tube. Mechanism reduces pull force, allowing easy lifting of larger shades. 
f.	Removable Spline System:  Co-extruded PVC spline, heat-sealed to shade fabric and inserted into an engineered "snap-on, snap-off" spline mounting.  
1)	Allows for adjustability on-site and ease in changing fabric bands in field. 
g.	Hem Bar:  Extruded aluminum. Sufficient weight for proper shade operation.  
1)	Exposed:  Finish:  As determined by Architect from manufacturer's range. 
2)	Enclosed:  In heat sealed pocket of fabric band material. 
3.	Options: 
a.	Dual Shades:  Hold two shades in one bracket assembly. 
b.	Coupled shades. 
c.	Bracket end covers to match appropriate fascia In size and color. 
d.	Side channels. 
e.	Sill channels. 
f.	Center channels. 
g.	Pockets:  4-3/4 inch (121 mm). 
h.	Pockets:  7-1/2 inch (191 mm). 
i.	Closure plate:  2 inch (51 mm). 
j.	Closure plate:  3 inch (76 mm). 
k.	Closure plate:  5 inch (127m). 
l.	Fascia:  Square. 
m.	Fascia:  Square extended. 
n.	Fascia:  Square dual. 
o.	Fascia:  Back. 
p.	Fascia:  Reverse roll.
2.5	MOTORIZED SOLAR SHADING SYSTEMS
A.	Shading Systems: Motorized Solar Shades as manufactured by SWFcontract.
1.	Configuration:  As scheduled or indicated by Drawings. 
2.	Configuration:  Individual shades. 
3.	Configuration:  Dual shades. 
4.	Configuration:  Group shades, as indicated on Drawings. 
B.	Fabric: Flame retardant, fade and stain resistant, anti-static, anti-microbial.
1.	Style: ____________.
2.	Color Name: ____________.
3.	Color Number: ____________.
4.	Fabric Style, Color Name, Color Number:  As scheduled and indicated on Drawings.
5.	Fabric Style, Color Name, Color Number: As selected by Architect from manufacturer's standard fabric range.
C.	Components: Fabricate such that shade hangs flat without buckling or distortion.
1.	Motors:  Enclosed tubular motors, quick-disconnect plugs standard.
a.	Description: Asynchronous, maintenance free with built in reversible capacitor and line voltage power supply.
b.	Compliance: Temperature Class A, thermally protected.
c.	Motor Type:  Low volt wired.
d.	Motor Type:  Low voltage wireless.
e.	Motor Type:  Line voltage wired.
f.	Motor Type:  Line voltage wireless.
g.	Motor Type:  Line voltage intelligent.
h.	Motors:  Concealed inside roller tubes. 
i.	Motor Size: To be determined by shade manufacturer to insure proper operation based on window size and fabric selection and not to exceed 80 percent of the motor and tube assembly rated lift capacity. 
j.	Speed: Shades same room must have motors rated at same nominal speed. 
k.	Power Supply Type:  Low voltage wall plug.
l.	Power Supply Type:  Standard wall plug, 110V-120 VAC.
m.	Power Supply Type:  Standard hardwired, 110V-120 VAC.
2.	Controls:  Provide group controls.
3.	Controls:  Provide individual controls.
4.	Controls:  Automated Shading System: 
a.	Option: Sunlight sensors. 
b.	Option:  Timer 
5.	Building Automation:  Provide interface with building automation. 
6.	Roller Tubes: Extruded-aluminum tubes engineered with a chamfered channel to accept fabric spline and allow fabric to lay across the tube without adding crease lines. The diameter and wall thickness to be determined by manufacturer based on fabric selection and shade size to provide minimal deflection and optimal performance.
7.	Idle End Brackets: Galvanized steel, adjustable, allow shades to be leveled in place.
8.	Spline Systems:  Consist of PVC spline heat-welded to the shade fabric and inserted into a channel on the roller tube. Spline system allows for on-site adjustments and facilitates changing fabric panels in the field. Tape and other methods of attachment are not acceptable.
9.	Hem Bars: Standard, aluminum extrusion enclosed in a fabric hem pocket with heat-welded seams and ends, to match shade cloth selection.
10.	Hem Bars: Provide optional fabric wrapped hem bar, to match shade cloth selection.
D.	Accessories:
1.	Fascia Panels:  None.
2.	Fascia Panels:  Standard 4.25 inches (108 mm).
3.	Fascia Panels:  Standard 7.5 inches (190.5 mm). 
4.	Fascia Panels:  Back. 
5.	Fascia Panels:  Dual shade snap-on design.
a.	Materials:  1/16 inches (1.6 mm) thick extruded 6063 T-5 aluminum alloy with powder coated finish.
b.	Finish: White.
c.	Finish: Vanilla. 
d.	Finish: Clear Anodized. 
e.	Finish: Bronze.
f.	Finish: Black. 
g.	Size:  3 inches (76 mm). 
h.	Size:  4 inches (102 mm). 
i.	Size:  7-5/8 inches (194 mm). 
6.	Shade Pockets:  Manufacturer shall provide appropriate dimensional pocket as necessary to enclose roller tube and fabric. 
a.	Type:  4-3/4 inches (121 mm) x 5 inch (127 mm) extruded aluminum 6065 alloy. 
b.	Finish:  White. 
c.	Finish:  Clear Anodized. 
d.	Finish:  Bronze Anodized. 
e.	Type:  7-1/2 inches (191 mm) x 8 inches (203 mm) white powder coated steel. 
7.	Closure Plates: Exposed, flush mounted, powder-coated extruded 6065-aluminum alloy designed to provide access to shades when recessed in ceiling. 
a.	Closure Mounts:  With a lip. 
b.	Closure Mounts:  Without a lip. 
c.	Plate Size:  2 inches (51 mm). 
d.	Plate Size:  3 inches (76 mm). 
e.	Plate Size:  5 inches (127 mm). 
f.	Finish:  White. 
g.	Finish:  Clear Anodized. 
h.	Finish:  Bronze. 
8.	Side, Sill, Center Channels: 2-piece design.
a.	Materials: Extruded 6065-aluminum.
b.	Size:  2 inch (51 mm) x 1 inch (25 mm), and 4 inch (102 mm) x 1 inch (25 mm) center channel is provided for coupled shades.
c.	Finish:  To Match Fascia Finish
9.	Blackout Shades: Provide synthetic pile inserts to eliminate light leakage.
2.6	SOLAR SHADE FABRICS
A.	Fabrics: Flame retardant, fade and stain resistant, anti-static, anti-microbial.
1.	Compliance: Pass NFPA 701 FR and ASTM G 21 and ASTM G 22.
2.	Seams: Shades with railroaded fabric will have heat-welded seams.
3.	Style: ____________.
4.	Color Name: ____________.
5.	Color Number: ____________.
6.	Fabric Style, Color Name, Color Number:  As scheduled and indicated on Drawings.
7.	Fabric Style, Color Name, Color Number: As selected by Architect from manufacturer's standard fabric range.
8.	Collection:  As scheduled and indicated on Drawings.
9.	Collection:  Double-Take T100 (1 percent).
10.	Collection:  Double-Take T300 (3 percent).
11.	Collection:  Double-Take T500 (5 percent).
12.	Collection:  Crosshatch S Series S100 (1 percent).
13.	Collection:  Crosshatch S Series S300 (3 percent). 
14.	Collection:  Crosshatch S Series S500 (5 percent).
15.	Collection:  Crosshatch S Series S1000 (10 percent).
16.	Collection:  Crosshatch A Series A100 (1 percent).
17.	Collection:  Crosshatch A Series A300 (3 percent).
18.	Collection:  Crosshatch A Series A500 (5 percent).
19.	Collection: Crosshatch R Series R100 (1 percent).
20.	Collection: Crosshatch R Series R300 (3 percent).
21.	Collection: Crosshatch R Series R500 (5 percent)
22.	Collection: Latitude X100 (1 percent).
23.	Collection: Factor M1400 (14 percent).
24.	Collection: Aspect (4 percent).
25.	Collection: Zenith (4 percent).
26.	Collection: Vision (7 percent).
27.	Collection:  Sheer Lines Light-Filtering Fabric (14 percent). 
28.	Collection:  Compass Reversible Twill Light-Filtering Fabric Series C100 (1 Percent). 
29.	Collection:  Compass Reversible Twill Light-Filtering Fabric Series C300 (3 Percent). 
30.	Collection:  Compass Reversible Twill Light-Filtering Fabric Series C500 (5 Percent). 
31.	Collection: Summit U Series U100 (1 percent).
32.	Collection: Summit U Series U300 (3 percent).
33.	Collection: Summit U Series U500 (5 percent).
34.	Collection:  Eternity PVC Free E Series E100 (1 Percent). 
35.	Collection:  Eternity PVC Free E Series E300 (3 Percent). 
36.	Collection:  Conceal Blackout Fabric, Light-Blocking Fabric (0 percent). 
37.	Collection:  Parallel Blackout Fabric, Light-Blocking Fabric (0 percent).
38.	Collection: Enterprise Blackout (0 percent).
39.	Collection: Nightfall Blackout (0 percent).
2.7	HORIZONTAL BLINDS
A.	Window Coverings:  Bali S3000 1 inch Aluminum Horizontal Mini Blinds as manufactured by SWFcontract.
1.	Slats: 
a.	Materials:  5000 series cold-rolled aluminum.
b.	Nominal Width: 1 inch (25 mm).
c.	Finish:  Polyester baked enamel, with Advanced Finishing Technology (AFT) which delivers anti-static performance to repel dust.
d.	UL Greenguard Gold certified. 
e.	Type: Solid .006 inch (0.15 mm) thick (standard).
f.	Type: Solid .008 inch (0.20 mm) thick. 
g.	Type: Perforated, 8 percent openness.
h.	Type: Inverted
i.	Type:  Privacy, (No Cord Route Holes). 
j.	Slat Color Name: ________.
k.	Slat Color Number: ________.
2.	Braided Ladders: 100 percent polyester yarn incorporating two extra strength rungs per ladder for slat support. 
a.	Ladder Spacing:  18 mm (11.86 slats per foot). 
b.	Ladder Spacing:  21.5 mm (14.17 slats per foot), standard. 
c.	Ladder Spacing:  20 mm (15.24 slats per foot). 
d.	Ladder Spacing:  22.5 mm (13.54 slats per foot). 
3.	Components:
a.	Headrail: 
1)	Size: 1 inches (25 mm) high x 1-1/2 inches (38 mm) wide x .025 inch (0.64 mm) thick.
2)	Description: Steel valance-free design with curved front profile, rolled edges at the top and a light blocking lip at the lower back side.
3)	Finish: Includes phosphate treatment, a chrome-free sealer, a low HAP urethane primer and a topcoat with low HAP polyester baked enamel.
b.	Tilters: Injection-molded thermoplastics, incorporates clutch mechanism to prevent damage due to over tilting.
c.	Tilt Limiter: Limits slat operation between a select range of operation. 
1)	Degrees Up: ___.
2)	Degrees Down: ___.
d.	Tilt Rods: Electro-zinc coated solid steel measuring 1/4 inch (13 mm) square.
e.	Tilt Wands: Clear polycarbonate with hexagonal cross section measuring approximately 1/4 inch diameter, attached to tilter shaft by means of spring clip.
f.	Cord Locks: Metal, snap-in design with floating, shaft-type locking pin and crash proof safety feature that locks blind automatically upon release of cord.
1)	Operation: Standard.
2)	Operation: Top lock cord lock provides for only two blind positions; fully down or fully raised.
3)	Operation: Ring Pull, provide plated steel ring in lieu of tassels, nominal 4 inch cord.
g.	Drum and Cradles: Low-friction thermoplastic, provided for each ladder.
h.	Brackets: Concealed, top loading, zinc plated steel with snap-in design.
i.	Brackets: Box brackets.
j.	Brackets: Extension brackets.
k.	Brackets: Hold down brackets.
l.	Bottomrails: Enclosed tubular shape.
1)	Materials: Phosphate-treated steel, finished with a chrome-free sealer.
2)	Finish: Low HAP urethane primer and a topcoat of low HAP polyester baked enamel, .025 inch (0.64 mm) thick.
B.	Window Coverings: Bali Classics 1 inch Aluminum Horizontal Mini Blinds as manufactured by SWFcontract.
1.	Slats: 
a.	Materials:  5000 series cold-rolled aluminum.
b.	Nominal Width: 1 inch (25 mm).
c.	Finish:  Polyester baked enamel, with Advanced Finishing Technology (AFT) which delivers anti-static performance to repel dust.
d.	UL Greenguard Gold certified 
e.	Type: Solid .006 inch (0.15 mm) thick (standard).
f.	Type: Solid .008 inch (0.20 mm) thick.
g.	Type: Perforated, 8 percent openness.
h.	Type: Inverted. 
i.	Slat Color Name: ________.
j.	Slat Color Number: ________.
2.	Braided Ladders: 100 percent polyester yarn incorporating two extra strength rungs per ladder for slat support. 
a.	Ladder Spacing: 21.5 mm (14.17 slats per foot), standard.
b.	Ladder Spacing: 20 mm (15.24 slats per foot).
c.	Ladder Spacing: 22.5 mm (13.54 slats per foot).
3.	Components:
a.	Headrail: 
1)	Size: 1 inches (25 mm) high x 1-1/2 inches (38 mm) wide x .025 inch (0.64 mm) thick.
2)	Description: U-shaped steel.
3)	Finish: Includes phosphate treatment, a chrome-free sealer, a low HAP urethane primer and a topcoat with low HAP polyester baked enamel.
b.	Tilters: Injection-molded thermoplastics, incorporates clutch mechanism to prevent damage due to over tilting.
c.	Tilt Limiter: Limits slat operation between a select range of operation. 
1)	Degrees Up: ___.
2)	Degrees Down: ___.
d.	Tilt Rods: Electro-zinc coated solid steel measuring 1/4 inch (13 mm) square.
e.	Tilt Wands: Clear polycarbonate with hexagonal cross section measuring approximately 1/4 inch diameter, attached to tilter shaft by means of spring clip.
f.	Cord Locks: Metal, snap-in design with floating, shaft-type locking pin and crash proof safety feature that locks blind automatically upon release of cord.
1)	Operation: Standard.
2)	Operation: Top lock cord lock provides for only two blind positions; fully down or fully raised.
3)	Operation: Ring Pull, provide plated steel ring in lieu of tassels, nominal 4 inch cord.
g.	Drum and Cradles: Low-friction thermoplastic, provided for each ladder.
h.	Brackets:  Standard, box style.
i.	Brackets: Extension brackets.
j.	Brackets: Hold down brackets.
k.	Brackets: 2 piece pocket bracket.
l.	Valance: Standard. 
m.	Valance: Deluxe 2-Slat. 
n.	Bottomrails: Enclosed tubular shape.
1)	Materials: Phosphate-treated steel, finished with a chrome-free sealer.
2)	Finish: Low HAP urethane primer and a topcoat of low HAP polyester baked enamel, .025 inch (0.64 mm) thick.
3)	Turn Clips: For extruded pocket.
o.	Accent Channels: Provide side channels.
C.	Window Coverings: Bali CustoMiser 1 inch Aluminum Horizontal Mini Blinds as manufactured by SWFcontract.
1.	Slats: 
a.	Materials:  5000 series cold-rolled aluminum.
b.	Nominal Width: 1 inch (25 mm).
c.	Finish:  Polyester baked enamel, with Advanced Finishing Technology (AFT) which delivers anti-static performance to repel dust.
d.	UL Greenguard Gold certified 
e.	Type: Solid .006 inch (0.15 mm) thick (standard).
f.	Type: Solid .008 inch (0.20 mm) thick.
g.	Type: Perforated, 8 percent openness.
h.	Type: Inverted. 
i.	Slat Color Name: ________.
j.	Slat Color Number: ________.
2.	Braided Ladders: 100 percent polyester yarn incorporating two extra strength rungs per ladder for slat support.
a.	Ladder Spacing:  21.5 mm (14.17 slats per foot), standard.
b.	Ladder Spacing:  20 mm (15.24 slats per foot).
c.	Ladder Spacing:  22.5 mm (13.54 slats per foot).
3.	Components:
a.	Headrail: 
1)	Size: 1 inches (25 mm) high x 1 inches (25 mm) wide x .025 inch (0.64 mm) thick.
2)	Description: U-shaped steel.
3)	Finish: Includes phosphate treatment, a chrome-free sealer, a low HAP urethane primer and a topcoat with low HAP polyester baked enamel.
b.	Tilters: Injection-molded thermoplastics, incorporates clutch mechanism to prevent damage due to over tilting.
c.	Tilt Limiter: Limits slat operation between a select range of operation. 
1)	Degrees Up: ___.
2)	Degrees Down: ___.
d.	Tilt Rods: Electro-zinc coated solid steel measuring 1/4 inch (13 mm) square.
e.	Tilt Wands: Clear polycarbonate with hexagonal cross section measuring approximately 1/4 inch diameter, attached to tilter shaft by means of spring clip.
f.	Cord Locks: Metal, snap-in design with floating, shaft-type locking pin and crash proof safety feature that locks blind automatically upon release of cord.
1)	Operation: Standard.
2)	Operation: Top lock cord lock provides for only two blind positions; fully down or fully raised.
3)	Operation: Ring Pull, provide plated steel ring in lieu of tassels, nominal 4 inch cord.
g.	Drum and Cradles: Low-friction thermoplastic, provided for each ladder.
h.	Brackets:  Standard, box type.
i.	Brackets: Extension brackets.
j.	Brackets: Hold down brackets.
k.	Valance: Standard. 
l.	Valance: Deluxe 2-Slat. 
m.	Bottomrails: Enclosed tubular shape.
1)	Materials: Phosphate-treated steel, finished with a chrome-free sealer.
2)	Finish: Low HAP urethane primer and a topcoat of low HAP polyester baked enamel, .025 inch (0.64 mm) thick.
D.	Window Coverings: Bali Apartment Aluminum Horizontal Mini Blinds as manufactured by SWFcontract.
1.	Slats: 
a.	Materials:  5000 series cold-rolled aluminum.
b.	Nominal Width: 1 inch (25 mm).
c.	UL Greenguard Gold certified. 
d.	Finish:  White satin polyester baked enamel, with Advanced Finishing Technology (AFT) which delivers anti-static performance to repel dust.
e.	Finish:  Alabaster polyester baked enamel, with Advanced Finishing Technology (AFT) which delivers anti-static performance to repel dust.
f.	Type: Solid .006 inch (0.15 mm) thick (standard).
g.	Slat Color Name: ________.
h.	Slat Color Number: ________.
2.	Braided Ladders: 100 percent polyester yarn incorporating two extra strength rungs per ladder for slat support.
a.	Ladder Spacing:  21.5 mm (14.17 slats per foot), standard. 
b.	Ladder Spacing:  20 mm (15.24 slats per foot). 
c.	Ladder Spacing:  22.5 mm (13.54 slats per foot).
3.	Components:
a.	Headrail: 
1)	Size: 1 inches (25 mm) high x 1 inches (25 mm) wide x .025 inch (0.64 mm) thick.
2)	Description: U-shaped steel.
3)	Finish: Includes phosphate treatment, a chrome-free sealer, a low HAP urethane primer and a topcoat with low HAP polyester baked enamel.
b.	Tilters: Injection-molded thermoplastics, incorporates clutch mechanism to prevent damage due to over tilting.
c.	Tilt Rods: Electro-zinc coated solid steel measuring 1/4 inch (13 mm) square.
d.	Tilt Wands: Clear polycarbonate with hexagonal cross section measuring approximately 1/4 inch diameter, attached to tilter shaft by means of spring clip.
e.	Cord Locks: Metal, snap-in design with floating, shaft-type locking pin and crash proof safety feature that locks blind automatically upon release of cord.
f.	Drum and Cradles: Low-friction thermoplastic, provided for each ladder.
g.	Brackets:  Extension brackets.
h.	Brackets:  Hold down brackets.
i.	Valance: Standard. 
j.	Valance: Deluxe 2-Slat. 
k.	Bottomrails:  Enclosed tubular shape.
1)	Materials: Phosphate-treated steel, finished with a chrome-free sealer.
2)	Finish: Low HAP urethane primer and a topcoat of low HAP polyester baked enamel, .025 inch (0.64 mm) thick.
E.	Window Coverings: SWFcontract 2 inch Designer Vinyl Blinds.
1.	Slats: Straight cut edges.
a.	Materials: Rigid UV stabilized crowned PVC.
b.	Nominal Width: 2 inches.
c.	Thickness: .045 inch (1.1 mm) thick. 
d.	Compliance: NFPA 701.
e.	Slat Color Name: ________.
f.	Slat Color Number: ________.
2.	Components:
a.	Headrails: SureClose Headrail.
1)	Size: 1-5/8 inch (41 mm) high x 2-1/4 inch (57 mm) wide x .022 inch (0.56 mm) thick.
2)	Description: U-shaped steel with 1/8 inch (3.2 mm) light blocking lip on the bottom centerline. 
3)	Finishing: Phosphate treatment, chrome-free sealer, low HAP urethane primer and topcoat with low HAP polyester baked enamel.
b.	Tilters: Cord tilter, snap-in, low-friction thermoplastic worm and pulley design, nylon gear housing; secured to pulley and treated with wood tassels at tilt end.
c.	Tilters: Wand tilter.
d.	Tilters: Ring tilter.
e.	Cord Locks: Metal, snap-in design incorporating a floating, shaft-type locking pin. Cord lock shall incorporate a crash proof safety feature that will lock blind automatically upon release of cord. End of lift cords will be treated with tassels.
f.	Ladders: Braided ladder, 100 percent polyester incorporating two extra strength rungs per ladder to support slats. 
g.	Ladders: Fabric tape, nominal 1 inch (25 mm). 
h.	Ladders: Fabric tape, nominal 1-1/2 inches (38 mm). 
i.	Ladder Spacing: 44 mm.
j.	Valance: Standard. 
k.	Valance: Deluxe.
l.	Bottomrails: Extruded foam PVC 3/4 inch (19 mm) high x 2 inches (51 mm) wide and shall coordinate with slats. 
2.8	ALUMINUM HORIZONTAL MICRO BLINDS
A.	Window Coverings: Bali S4000 Aluminum Horizontal Micro blinds as manufactured by SWFcontract.
1.	Slats: 
a.	Materials:  5000 series cold-rolled aluminum.
b.	Nominal Width: 1/2 inch.
c.	Finish:  Polyester baked enamel, with Advanced Finishing Technology (AFT) which delivers anti-static performance to repel dust.
d.	UL Greenguard Gold certified 
e.	Type: Solid .006 inch (0.15 mm) thick (standard).
f.	Slat Color Name: ________.
g.	Slat Color Number: ________.
2.	Components:
a.	Headrail: 
1)	Size: 1 inches (25 mm) high x 1-1/2 inches (38 mm) wide x .025 inch (0.64 mm) thick.
2)	Description: Steel valance-free design with curved front profile, rolled edges at the top and a light blocking lip at the lower back side.
3)	Finish: Includes phosphate treatment, a chrome-free sealer, a low HAP urethane primer and a topcoat with low HAP polyester baked enamel.
b.	Tilters: Injection-molded thermoplastics, incorporates clutch mechanism to prevent damage due to over tilting.
c.	Tilt Limiter: Limits slat operation between a select range of operation. 
1)	Degrees Up: ___.
2)	Degrees Down: ___.
d.	Tilt Rods: Electro-zinc coated solid steel measuring 1/4 inch (13 mm) square.
e.	Tilt Wands: Clear polycarbonate with hexagonal cross section measuring approximately 1/4 inch diameter, attached to tilter shaft by means of spring clip.
f.	Cord Locks: Metal, snap-in design with floating, shaft-type locking pin and crash proof safety feature that locks blind automatically upon release of cord.
1)	Operation: Standard.
2)	Operation: Top lock cord lock provides for only two blind positions; fully down or fully raised.
3)	Operation: Ring Pull, provide plated steel ring in lieu of tassels, nominal 4 inch cord.
g.	Drum and Cradles: Low-friction thermoplastic, provided for each ladder.
h.	Brackets: Box brackets.
i.	Braided Ladders:  100 percent polyester yarn incorporating two extra strength rungs per ladder for slat support. Standard ladder spacing shall be 12.5 mm.
j.	Bottomrails: Enclosed tubular shape.
1)	Materials: Phosphate-treated steel, finished with a chrome-free sealer.
2)	Finish: Low HAP urethane primer and a topcoat of low HAP polyester baked enamel, .025 inch (0.64 mm) thick.
B.	Window Coverings: Bali Aluminum Horizontal Micro blinds as manufactured by SWFcontract.
1.	Slats: 
a.	Materials:  5000 series cold-rolled aluminum.
b.	Nominal Width: 1/2 inch.
c.	Finish:  Polyester baked enamel, with Advanced Finishing Technology (AFT) which delivers anti-static performance to repel dust.
d.	UL Greenguard Gold certified 
e.	Type: Solid .006 inch (0.15 mm) thick (standard).
f.	Slat Color Name: ________.
g.	Slat Color Number: ________.
2.	Components:
a.	Headrail: 
1)	Size: 1 inches (25 mm) high x 1 inches (25 mm) wide x .025 inch (0.64 mm) thick.
2)	Description: U-shaped steel.
3)	Finish: Includes phosphate treatment, a chrome-free sealer, a low HAP urethane primer and a topcoat with low HAP polyester baked enamel.
b.	Tilters: Injection-molded thermoplastics, incorporates clutch mechanism to prevent damage due to over tilting.
c.	Tilt Limiter: Limits slat operation between a select range of operation. 
1)	Degrees Up: ___.
2)	Degrees Down: ___.
d.	Tilt Rods: Electro-zinc coated solid steel measuring 1/4 inch (13 mm) square.
e.	Tilt Wands: Clear polycarbonate with hexagonal cross section measuring approximately 1/4 inch diameter, attached to tilter shaft by means of spring clip.
f.	Cord Locks: Metal, snap-in design with floating, shaft-type locking pin and crash proof safety feature that locks blind automatically upon release of cord.
1)	Operation: Standard.
2)	Operation: Top lock cord lock provides for only two blind positions; fully down or fully raised.
3)	Operation: Ring Pull, provide plated steel ring in lieu of tassels, nominal 4 inch cord.
g.	Drum and Cradles: Low-friction thermoplastic, provided for each ladder.
h.	Brackets: Box brackets.
i.	Valance: Standard. 
j.	Valance: Deluxe 2-Slat.
k.	Braided Ladders:  100 percent polyester yarn incorporating two extra strength rungs per ladder for slat support. Standard ladder spacing shall be 12.5 mm.
l.	Bottomrails: Enclosed tubular shape.
1)	Materials: Phosphate-treated steel, finished with a chrome-free sealer.
2)	Finish: Low HAP urethane primer and a topcoat of low HAP polyester baked enamel, .025 inch (0.64 mm) thick.
2.9	ALUMINUM HORIZONTAL BLINDS
A.	Window Coverings: Bali Heritage 2 inch Aluminum Horizontal Blinds as manufactured by SWFcontract.
1.	Slats:
a.	Materials:  5000 series cold-rolled aluminum.
b.	Nominal Width: 2 inches.
c.	Finish:  Polyester baked enamel, with Advanced Finishing Technology (AFT) which delivers anti-static performance to repel dust.
d.	UL Greenguard Gold certified 
e.	Type:  Solid .008 inch (0.20 mm) thick (standard).
f.	Type: Inverted. 
g.	Slat Color Name: ________.
h.	Slat Color Number: ________.
2.	Components:
a.	Headrail: SureClose Headrail.
1)	Size: 1-5/8 inch (41 mm) high x 2-1/4 inch (57 mm) wide x .022 inch (0.56 mm) thick.
2)	Description: U-shaped steel with 1/8 inch (3.2 mm) light blocking lip on the bottom centerline.
3)	Finish: Includes phosphate treatment, a chrome-free sealer, a low HAP urethane primer and a topcoat with low HAP polyester baked enamel.
b.	Motors: Tilt wirefree motor. Provides tilt control of 2ï¿½ horizontal blinds. 
1)	Description: Capable of precision tilting of blind slats 
2)	Motor type: Low voltage wired. 
3)	Motors: concealed inside headrail. 
4)	Motor size: To be determined by blind manufacturer to insure proper operation based on window size up to 7,200 square feet. 
5)	Speed: 5 rpms. 
6)	Power Supply Type: Low voltage battery 12 VDC 
7)	Power Supply Type: Low voltage wall plug, 110V-120V VAC. 
8)	Power Supply Type: Solar Recharge Kit 
9)	Power Supply Type: 5-10 motor Transformer Kit 
c.	Tilters: Cord tilter, snap-in component incorporating a worm and pulley of low-friction thermoplastic and a nylon gear; standard 1.8 mm in diameter.
d.	Tilters:  Wand tilter.
e.	Tilters:  Ring tilter.
f.	Cord Locks: Metal, snap-in design with floating, shaft-type locking pin and crash proof safety feature that locks blind automatically upon release of cord.
1)	Operation: Standard.
2)	Operation: Ring Pull, provide plated steel ring in lieu of tassels, nominal 4 inch cord.
g.	Ladders: 
1)	Type: Braided ladders. 
2)	Type:  Fabric tape.
h.	Bottomrails: C-shaped, enclosed with a dust cover slat.
1)	Size: 9/16 inch (14 mm) high x 2 inches (51 mm) wide x .040 inch (1 mm) thick.
2)	Materials: Anodized aluminum. 
3)	Finish: Polyester baked enamel to match headrail.
i.	Valance:  Standard
j.	Valance: Deluxe. 
B.	Window Coverings: Bali Heritage 2 inch School Aluminum Horizontal Blinds as manufactured by SWFcontract.
1.	Slats:
a.	Materials:  5000 series cold-rolled aluminum.
b.	Nominal Width: 2 inches.
c.	Finish:  Polyester baked enamel, with Advanced Finishing Technology (AFT) which delivers anti-static performance to repel dust.
d.	UL Greenguard Gold certified 
e.	Type:  Solid .008 inch (0.20 mm) thick (standard).
f.	Type: Inverted. 
g.	Slat Color Name: ________.
h.	Slat Color Number: ________.
2.	Components:
a.	Headrail: SureClose Headrail.
1)	Size: 1-5/8 inch (41 mm) high x 2-1/4 inch (57 mm) wide x .022 inch (0.56 mm) thick.
2)	Description: U-shaped steel with 1/8 inch (3.2 mm) light blocking lip on the bottom centerline.
3)	Finish: Includes phosphate treatment, a chrome-free sealer, a low HAP urethane primer and a topcoat with low HAP polyester baked enamel.
b.	Tilters: Cord tilter, snap-in component incorporating a worm and pulley of low-friction thermoplastic and a nylon gear; standard 2.2 mm in diameter.
c.	Tilters:  Wand tilter.
d.	Tilters:  Ring tilter.
e.	Cord Locks: Metal, snap-in design with floating, shaft-type locking pin and crash proof safety feature that locks blind automatically upon release of cord.
1)	Operation: Standard.
2)	Operation: Top lock cord lock provides for only two blind positions; fully down or fully raised.
3)	Operation: Ring Pull, provide plated steel ring in lieu of tassels, nominal 4 inch cord.
f.	Lift Cords: Braided polyester measuring 2.2 mm in diameter.
g.	Vinyl Ladder Tape: 1-1/2 inch wide reinforced vinyl. 
h.	Ladder Spacing: Standard, 42 mm. 
i.	Bottomrails: C-shaped, enclosed with a dust cover slat.
1)	Size: 9/16 inch (14 mm) high x 2 inches (51 mm) wide x .040 inch (1 mm) thick.
2)	Materials: Anodized aluminum. 
3)	Finish: Polyester baked enamel to match headrail.
j.	Valance: Standard.
k.	Valance:  Deluxe. 
2.10	WOOD HORIZONTAL BLINDS
A.	Window Coverings: SWFcontract Elite Woods 2 inch Wood Horizontal Blinds.
1.	Slats:
a.	Slat Type: Standard.
b.	Slat Type: NoHoles slats.
c.	Nominal Slat Width: 2 inches.
d.	Thickness: .115 inch (2.9 mm) thick.
e.	Materials: Lineal grained and smooth sanded 100 percent North American basswood, kilned dried to 6 - 10 percent moisture content to reduce warping.
f.	Finish: Painted, color ___________.
1)	Standard Slat Color Name: ________.
2)	Custom Slat Color Name: Colors by Choice color program, ________.
3)	Slat Color Number: ________.
g.	Finish: Stained and coated with clear satin lacquer, hand-rubbed appearance. 
h.	Finish: Stained and coated with high polish satin lacquer. 
i.	Beaded Slats: __________.
2.	Components:
a.	Headrails:  1-5/8 inch (41 mm) high x 2-3/8 inch (60 mm) wide x .025 inch (1.4 mm) thick U-shaped steel with 1/8" light-blocking lip
b.	Valance: Lineal grained, smooth sanded 100 percent North American basswood. 
c.	Motors: Tilt wirefree motor. Provides tilt control of 2" horizontal blinds.  
1)	Description: Capable of precision tilting of blind slats  
2)	Motor type: Low voltage wired.  
3)	Motors: Concealed inside headrail.  
4)	Motor size: To be determined by blind manufacturer to insure proper operation based on window size up to 7,200 square feet.  
5)	Speed: 5 rpms.  
6)	Power Supply Type: Low voltage battery 12 VDC  
7)	Power Supply Type: Low voltage wall plug, 110V-120V VAC.  
8)	Power Supply Type: Solar Recharge Kit.  
9)	Power Supply Type: 5-10 motor Transformer Kit.  
10)	Type: Four bead. 
11)	Type: Crown molded.
d.	Tilters: Cord operated, low-friction thermoplastic worm and pulley design, nylon gear housing.
e.	Tilters: Wood wand tilter.
f.	Tilters: Ring tilter.
g.	Tassels: Antique brass.
h.	Tassels: Wood tassels
i.	Cord Locks: Snap-in metal design, incorporating a floating, shaft-type locking pin and a crash proof safety feature that will lock blind automatically upon release of cord.
1)	Operation: Standard.
2)	Operation: Ring Pull, provide plated steel ring in lieu of tassels, nominal 4 inch cord.
3)	Operation:  Cordless. 
j.	Ladders: Nominal 2 inch. 
k.	Ladders: Nominal 2-1/2 inches. 
l.	Ladders:  COM fabric.
m.	Ladders: Braided ladder roll, secured around body of ladder with stainless steel wire loop, secured to the tilt rod to ensure tight closure of slats.
1)	Materials: Polyester Dacron yarn. 
n.	Ladder Spacing: Standard, 44 mm.
o.	Bottomrails: 
1)	Materials: Lineal grained and smooth sanded 100 percent North American basswood, kilned dried to 6 - 10 percent moisture content to reduce warping. 
2)	Description: Contour molded to a shape of 3/8 inch (9.5 mm) x 2 inches (51 mm) with 1/8 inch (3.2 mm) radius rounded edges.
p.	Decorative Trims:  As scheduled and indicated on Drawings.
B.	Window Coverings: SWFcontract Traditions 1 inch Wood Horizontal Blinds.
1.	Slats:
a.	Nominal Slat Width:  1 inch (25 mm).
b.	Materials: Lineal grained and smooth sanded 100 percent North American basswood, kilned dried to 6 - 10 percent moisture content to reduce warping.
c.	Finish: Painted, color ___________.
1)	Standard Slat Color:
a)	Color Name:  ________.
b)	Color Number:  ________.
2)	Custom Slat Color Name:  Colors by Choice color program, ________. 
d.	Finish: PureGrain finish. 
e.	Finish: Stained and coated with clear satin lacquer, hand-rubbed appearance. 
f.	Finish: Stained and coated with high polish satin lacquer. 
2.	Components:
a.	Headrails: 1 inch (25 mm) high x 1-1/2 inch (38 mm) wide x .025 inch (0.64 mm) thick U-shaped steel.
b.	Finishing: Phosphate treatment, chrome-free sealer, low HAP urethane primer and topcoat with low HAP polyester baked enamel.
c.	Operation:  Tilters, injection-molded thermoplastics for smooth low-friction operation and will incorporate a clutch mechanism to prevent damage due to over tilting. 
1)	Type: Wood wand tilter, standard.
2)	Type: Ring tilter.
d.	Cord Locks: Snap-in design incorporating a stainless steel wear guard over which cords pass. A floating, shaft-locking pin will lock blind at any position and shall be crash proof. 
e.	End of Lift Cords: Treated with wooden tassels. 
f.	End of Lift Cords: Ring pulls, plated steel ring in lieu of tassels with nominal 4 inch cord.
g.	Ladders: Braided ladders, 100 percent polyester incorporating two extra strength rungs per ladder to support slats.
h.	Bottomrails: 5/8 inch (16 mm) high x 1 inch (25 mm) wide wood and finished to coordinate with slat color. 
C.	Window Coverings: SWFcontract Traditions 2 inch Wood Horizontal Blinds.
1.	Slats:
a.	Slat Type: Standard.
b.	Slat Type: NoHoles slats.
c.	Nominal Slat Width: 2 inches.
d.	Nominal Slat Width: 2-1/2 inches Shutter style.
e.	Nominal Slat Width: 2-3/8 inches.
f.	Thickness: 1/8 inch (3.2 mm).
g.	Materials: Lineal grained and smooth sanded 100 percent North American basswood, kilned dried to 6 - 10 percent moisture content to reduce warping.
h.	Finish: Painted, color ___________.
1)	Standard Slat Color:
a)	Color Name:  ________.
b)	Color Number:  ________.
i.	Finish: PureGrain finish. 
j.	Finish: Stained and coated with clear satin lacquer, hand-rubbed appearance. 
k.	Finish: Stained and coated with high polish satin lacquer. 
2.	Components: 
a.	Headrails: SureClose Headrail.
1)	Size: 1-5/8 inch (41 mm) high x 2-1/4 inch (57 mm) wide x .022 inch (0.56 mm) thick.
2)	Description: U-shaped steel with 1/8 inch (3.2 mm) light blocking lip on the bottom centerline. 
3)	Finishing: Phosphate treatment, chrome-free sealer, low HAP urethane primer and topcoat with low HAP polyester baked enamel.
b.	Operation:  Cordless.
c.	Operation:  Tilters, cord tilter, snap-in, low-friction thermoplastic worm and pulley design, nylon gear housing; secured to pulley and treated with wood tassels at tilt end.
d.	Operation:  Tilters, wood wand tilter.
e.	Operation:  Tilters, ring tilter.
f.	Cord Locks: Snap-in design incorporating a stainless steel wear guard over which cords pass. A floating, shaft-locking pin will lock blind at any position and shall be crash proof. 
g.	End of Lift Cords: Treated with wooden tassels. 
h.	End of Lift Cords: Ring pulls, plated steel ring in lieu of tassels with nominal 4 inch cord.
i.	Ladders: Braided ladders, 100 percent polyester incorporating two extra strength rungs per ladder to support slats.
j.	Ladders: Fabric tapes.
k.	Ladder Spacing: 44 mm. 
l.	Bottomrails: 5/8 inch (16 mm) high x 2 inch (51 mm) wide wood in a trapezoid shape to improve closure and finished to coordinate with slats. 
2.11	FAUX WOOD BLINDS
A.	Window Coverings: 
1.	Blinds: SWFcontract Traditions Lake Forest Faux Wood Blinds.
a.	Surface Appearance: Printed slats mimic the look of real wood.
2.	Slats: Straight cut edges.
a.	Slat Width:  2 inches (51 mm).
b.	Slat Width:  2.5 inches (63 mm).
c.	Slat Type:  Standard.
d.	Slat Type: NoHoles slats.
e.	Materials: Rigid UV stabilized flat PVC 
f.	Nominal Width:  2 inches wide.
g.	Thickness: .10 inches thick. 
h.	Compliance: FR Rated and NFPA 701.
i.	Slat Color Name: ________.
j.	Slat Color Number: ________.
3.	Components:
a.	Headrails: SureClose Headrail.
1)	Size: 1-5/8 inch (41 mm) high x 2-1/4 inch (57 mm) wide x .022 inch (0.56 mm) thick.
2)	Description: U-shaped steel with 1/8 inch (3.2 mm) light blocking lip on the bottom centerline. 
3)	Finishing: Phosphate treatment, chrome-free sealer, low HAP urethane primer and topcoat with low HAP polyester baked enamel.
b.	Operation:  Cordless.
c.	Operation:  Tilters, cord tilter, snap-in, low-friction thermoplastic worm and pulley design, nylon gear housing; secured to pulley and treated with wood tassels at tilt end.
d.	Cord Locks: Metal, snap-in design incorporating a floating, shaft-type locking pin. Cord lock shall incorporate a crash proof safety feature that will lock blind automatically upon release of cord. End of lift cords will be treated with tassels.
e.	Ladders: Braided ladder, 100 percent polyester incorporating two extra strength rungs per ladder to support slats.
f.	Ladders:  Fabric tape.
g.	Ladder Spacing: 44 mm.
h.	Bottomrails: Extruded foam PVC 9/16 inch (14 mm) high x 2 inches (51 mm) wide, coordinates with slats. 
2.12	VERTICAL BLINDS
A.	Window Coverings: SWFcontract G-98 Ultra-Vue Vertical Blinds.
1.	Louvers: As selected by Architects from the Graber line of PVC offerings.
a.	Type: 3-1/2 inch PVC.
b.	Type: 2 inch PVC.
c.	Type: 3-1/2 inch Fabric.
d.	Louver Color Number: _________.
e.	Louver Color Name: _________.
f.	Channel Panel Insert for Fabric Louvers: 
1)	Insert Color Name: _________.
2)	Insert Color Number: _________.
2.	Components:
a.	Bottom Chain: Provide optional bottom chain.
b.	Headrails:
1)	Materials: Anodized aluminum alloy 6063-T5 with a bright dip finish.
2)	Size: 1-3/8 inches (35 mm) wide x 1-3/16 inches (30 mm) high.
3)	Average Wall Thickness: .050 inch (1.3 mm) 
c.	Carriers: Carriers shall be centrally located making the headrail reversible and are replaceable without demounting the headrail.
1)	Materials: Molded acetyl 5/16 inch (8 mm) wide, non-yellowing.
2)	Description: Traverses on self-lubricated wheels, standard stack release mechanism allows stack to be moved away from stack end access. 
d.	Rotation Control: Gear ratio of 6:1.
1)	Control Type: Standard, bead chain, No. 6 nickel-plated steel.
2)	Control Type: One Touch wand control, one way draw only, not available with 2 inch louvers.
3)	Rack and Pinion Gear System: Provides 180 degrees direct rotation. 
4)	Pinion Rods: Extruded aluminum 0.235 inch (6 mm) diameter.
e.	Traversing Control: Stainless steel spacer system for uniform louver spacing. 
f.	Traverse Cord: Danskord 1.8 mm diameter and is equipped with a tension pulley and cord clip. 
g.	Cord Clip: Anchored to the wall or window jamb in accordance with CPSC recommendations.
h.	Valances:  Provide optional valances. 
i.	UL Greenguard Gold certified
B.	Window Coverings: SWFcontract G-71 Super-Vue Vertical Blinds.
1.	Louvers: As selected by Architects from the Graber line of PVC offerings.
a.	Type: 3-1/2 inch PVC.
b.	Type: 2 inch PVC.
c.	Type: 3-1/2 inch Fabric.
d.	Louver Color Number: _________.
e.	Louver Color Name: _________.
f.	Channel Panel Insert for Fabric Louvers: 
1)	Insert Color Name: _________.
2)	Insert Color Number: _________.
2.	Components:
a.	Headrails:
1)	Materials: Anodized aluminum alloy 6063-T5 with a satin dip finish.
2)	Size: 1-15/16 inches (49 mm) wide x 1-3/8 inches (35 mm) high.
3)	Average Wall Thickness: .050 inch (1.3 mm) 
b.	Carriers: Carriers shall be centrally located making the headrail reversible; carriers and stems are replaceable without demounting the headrail.
1)	Materials: Molded acetyl.
2)	Description: Traverses on self-lubricated wheels.
3)	Stems: Clear, non-yellowing, UV-stabilized nylon; impact-resistant. 
c.	Traversing Control:  Wand.
d.	Traversing Control:  Cord.
1)	Traverse Cord: No. 3 braided polyester with a fiberglass core, 0.094 inch (2.4 mm) and is equipped with a tension cord weight and cord clip. 
2)	Cord Clip: Anchored to the wall or window jamb during installation in accordance with CPSC recommendations.
e.	Operation Mechanism:  As scheduled and indicated on Drawings. 
f.	Operation Mechanism:  Rotation control, bead chain, No. 10 nickel-plated steel. 
1)	E-Z Open feature automatically rotates louvers open when traverse cord is operated. 
2)	Dual Rack and Pinion Gear System:  Provides 180 degrees direct rotation.  
3)	Pinion Rods:  Extruded aluminum 0.30 inch (7.6 mm) diameter. 
g.	Operation Mechanism:  One Touch wand control, one way draw only, not available with 2 inch louvers. 
h.	UL Greenguard Gold certified
C.	Window Coverings: SWFcontract G-85 Dura-Vue Vertical Blinds.
1.	Louvers: As selected by Architects from the Graber line of PVC offerings.
a.	Type: 3-1/2 inch PVC.
b.	Type: 2 inch PVC.
c.	Type: 3-1/2 inch Fabric.
d.	Louver Color Number: _________.
e.	Louver Color Name: _________.
f.	Channel Panel Insert for Fabric Louvers: 
1)	Insert Color Name: _________.
2)	Insert Color Number: _________.
2.	Components:
a.	Headrails: Roll formed, phosphate-treated recycled steel.
1)	Size: 1-1/2 inches (38 mm) wide x 1-1/4 inches (32 mm) high.
2)	Thickness: .027 inches (0.7 mm).
3)	Finish: With baked enamel finish in Ivory Gloss. 
b.	Carriers: Carriers shall be centrally located making the headrail reversible; carriers and stems are replaceable without demounting the headrail.
1)	Description: Traverses on self-lubricated wheels.
2)	Detachable Stems: Clear, non-yellowing, UV-stabilized nylon; impact-resistant. 
c.	Rotation Controls: Standard, bead chain, No. 6 nickel-plated steel.
1)	Dual Rack and Pinion Gear System: Provides 180 degrees direct rotation. 
2)	Pinion Rods: Extruded aluminum 0.30 inch (7.6 mm) diameter.
3)	Control Type: Standard, bead chain, No. 6 nickel-plated steel.
4)	Control Type: One Touch wand control, one way draw only, not available with 2 inch louvers.
d.	Traversing Control: Nylon strap system.
1)	Traverse Cord: No. 3 braided polyester with a fiberglass core, 0.094 inch (2.4 mm) and is equipped with a tension cord weight and cord clip. 
2)	Cord Clip: Anchored to the wall or window jamb during installation in accordance with CPSC recommendations.
e.	Valances:  Provide optional valances.
f.	UL Greenguard Gold certified
2.13	CELLULAR SHADES
A.	Window Coverings: SWFcontract CrystalPleat 3/8 inch Double Cell Cellular Shades.
1.	Fabric:  Fade and stain resistant, anti-static, anti-microbial.
a.	Compliance:  ASTM G 21 and ASTM G 22.
b.	Description: 3/8 inch (9.5 mm) double cell construction selected from an assortment of non-woven spun-lace, point bond 100 percent polyester fabrics.
c.	Seams: Shades with railroaded fabric will have heat-welded seams.
d.	Style: ____________.
e.	Color Name: ____________.
f.	Color Number: ____________.
g.	Fabric Style, Color Name, Color Number:  As scheduled and indicated on Drawings.
h.	Fabric Style, Color Name, Color Number: As selected by Architect from manufacturer's standard fabric range.
2.	Lift System: Standard.
a.	Cord Locks: Snap-in design, injection-molded thermoplastic, incorporating a metal, free-floating, serrated cord-locking roller. 
b.	Lift Cords: 1.2 mm polyester and concealed. A snap tassel and joiner ball connect to a single Danskord for raising and lowering the shade. Cord, tassel and joiner ball are color coordinated with fabric.
c.	Headrails: 
1)	Size: 0.665 inch (17 mm) high x 1.540 inch (39 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
3.	Lift System: 
a.	Continuous Cord Loop Lift System: White cord loop controls lowering and raising shade.
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
c.	Bottomrails: 
1)	Size: 0.36 inch (0.9 mm) high x 1.54 inch (39 mm) deep. 
2)	Materials: Extruded aluminum.  
3)	Wall Thickness: 0.045 inch (1.14 mm).  
4)	Finish: Painted to coordinate with fabric color.
4.	Lift System: 
a.	Cordless Lift System: Lift and lowering operation without use of cord controls.
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
c.	Bottomrails: 
1)	Size: 0.36 inch (0.9 mm) high x 1.54 inch (39 mm) deep. 
2)	Materials: Extruded aluminum. 
3)	Wall Thickness: 0.045 inch (1.14 mm). 
4)	Finish: Painted to coordinate with fabric color.
5.	Lift System: 
a.	Motor Lift System: Lift and lowering operation with a wireless controller 
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep. 
2)	Materials: Extruded aluminum headrail. 
3)	Wall Thickness: 0.045 inch (1.1 mm). 
4)	Finish: Painted to coordinate with fabric color. 
c.	Bottomrails: 
1)	Size: 0.36 inch (0.9 mm) high x 1.54 inch (39 mm) deep. 
2)	Materials: Extruded aluminum. 
3)	Wall Thickness: 0.045 inch (1.14 mm). 
4)	Finish: Painted to coordinate with fabric color. 
d.	Motors:
1)	Motor type: Low voltage wired.  
2)	Motors: concealed inside headrail  
3)	Power Supply Type: Low voltage battery 12 VDC  
4)	Power Supply Type: Low voltage wall plug, 110V-120V VAC.  
5)	Power Supply Type: Solar Recharge Kit  
6)	Power Supply Type: 5-10 motor Transformer Kit  
B.	Window Coverings: SWFcontract CrystalPleat 3/8 inch Single Cell Cellular Shades.
1.	Fabric: Fade and stain resistant, anti-static, anti-microbial.
a.	Compliance:
1)	Antifungal and Antibacterial:  ASTM G 21 and ASTM G 22. 
2)	FR Rating:  NFPA 701 (scroll FR fabric)
b.	Description: 3/8 inch (9.5 mm) single cell construction selected from an assortment of non-woven spun-lace, point bond 100 percent polyester fabrics.
c.	Seams: Shades with railroaded fabric will have heat-welded seams.
d.	Style: ____________.
e.	Color Name: ____________.
f.	Color Number: ____________.
g.	Fabric Style, Color Name, Color Number:  As scheduled and indicated on Drawings.
h.	Fabric Style, Color Name, Color Number: As selected by Architect from manufacturer's standard fabric range.
2.	Lift System: Standard.
a.	Cord Locks: Snap-in design, injection-molded thermoplastic, incorporating a metal, free-floating, serrated cord-locking roller. 
b.	Lift Cords: 1.2 mm polyester and concealed. A snap tassel and joiner ball connect to a single Danskord for raising and lowering the shade. Cord, tassel and joiner ball are color coordinated with fabric.
c.	Headrails: 
1)	Size: 0.665 inch (17 mm) high x 1.540 inch (39 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
d.	Bottomrails: 
1)	Size: 0.36 inch (0.9 mm) high x 1.54 inch (39 mm) deep. 
2)	Materials: Extruded aluminum. 
3)	Wall Thickness: 0.045 inch (1.14 mm). 
4)	Finish: Painted to coordinate with fabric color.
3.	Lift System: 
a.	Continuous Cord Loop Lift System: White cord loop controls lowering and raising shade.
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
c.	Bottomrails: 
1)	Size: 0.36 inch (0.9 mm) high x 1.54 inch (39 mm) deep. 
2)	Materials: Extruded aluminum. 
3)	Wall Thickness: 0.045 inch (1.14 mm). 
4)	Finish: Painted to coordinate with fabric color.
4.	Lift System: 
a.	Cordless Lift System: Lift and lowering operation without use of cord controls.
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
c.	Bottomrails: 
1)	Size: 0.36 inch (0.9 mm) high x 1.54 inch (39 mm) deep. 
2)	Materials: Extruded aluminum. 
3)	Wall Thickness: 0.045 inch (1.14 mm). 
4)	Finish: Painted to coordinate with fabric color.
5.	Lift System: 
a.	Motor Lift System: Lift and lowering operation with a wireless controller 
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep. 
2)	Materials: Extruded aluminum headrail. 
3)	Wall Thickness: 0.045 inch (1.1 mm). 
4)	Finish: Painted to coordinate with fabric color. 
c.	Bottomrails: 
1)	Size: 0.36 inch (0.9 mm) high x 1.54 inch (39 mm) deep. 
2)	Materials: Extruded aluminum. 
3)	Wall Thickness: 0.045 inch (1.14 mm). 
4)	Finish: Painted to coordinate with fabric color. 
d.	Motors:
1)	Motor type: Low voltage wired.  
2)	Motors: concealed inside headrail 
3)	Power Supply Type: Low voltage battery 12 VDC  
4)	Power Supply Type: Low voltage wall plug, 110V-120V VAC.  
5)	Power Supply Type: Solar Recharge Kit  
6)	Power Supply Type: 5-10 motor Transformer Kit  
C.	Window Coverings: SWFcontract CrystalPleat 3/4 inch Single Cell Cellular Shades.
1.	Fabric: Fade and stain resistant, anti-static, anti-microbial.
a.	Compliance:
1)	Antifungal and Antibacterial:  ASTM G 21 and ASTM G 22. 
2)	FR Rating:  NFPA 701 (scroll FR fabric)
b.	Description: 3/4 inch (19 mm) single cell construction selected from an assortment of non-woven spun-lace, point bond 100 percent polyester fabrics.
c.	Seams: Shades with railroaded fabric will have heat-welded seams.
d.	Style: ____________.
e.	Color Name: ____________.
f.	Color Number: ____________.
g.	Fabric Style, Color Name, Color Number:  As scheduled and indicated on Drawings.
h.	Fabric Style, Color Name, Color Number: As selected by Architect from manufacturer's standard fabric range.
2.	Lift System: Standard.
a.	Cord Locks: Snap-in design, injection-molded thermoplastic, incorporating a metal, free-floating, serrated cord-locking roller. 
b.	Lift Cords: 1.2 mm polyester and concealed. A snap tassel and joiner ball connect to a single Danskord for raising and lowering the shade. Cord, tassel and joiner ball are color coordinated with fabric.
c.	Headrails: 
1)	Size: 0.812 inch (20.6 mm) high x 2 inches (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
d.	Bottomrails: 
1)	Size: 0.375 inch (0.95 mm) high x 2 inch (51 mm) deep. 
2)	Materials: Extruded aluminum. 
3)	Wall Thickness: 0.045 inch (1.14 mm). 
4)	Finish: Painted to coordinate with fabric color.
3.	Lift System: 
a.	Continuous Cord Loop Lift System: White cord loop controls lowering and raising shade.
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
c.	Bottomrails: 
1)	Size: 0.375 inch (0.95 mm) high x 2 inch (51 mm) deep. 
2)	Materials: Extruded aluminum. 
3)	Wall Thickness: 0.045 inch (1.14 mm). 
4)	Finish: Painted to coordinate with fabric color.
4.	Lift System: 
a.	Cordless Lift System: Lift and lowering operation without use of cord controls.
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
c.	Bottomrails: 
1)	Size: 0.375 inch (0.95 mm) high x 2 inch (51 mm) deep. 
2)	Materials: Extruded aluminum. 
3)	Wall Thickness: 0.045 inch (1.14 mm). 
4)	Finish: Painted to coordinate with fabric color.
5.	Lift System: 
a.	Motor Lift System: Lift and lowering operation with a wireless controller 
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep. 
2)	Materials: Extruded aluminum headrail. 
3)	Wall Thickness: 0.045 inch (1.1 mm). 
4)	Finish: Painted to coordinate with fabric color. 
c.	Bottomrails: 
1)	Size: 0.36 inch (0.9 mm) high x 1.54 inch (39 mm) deep. 
2)	Materials: Extruded aluminum. 
3)	Wall Thickness: 0.045 inch (1.14 mm). 
4)	Finish: Painted to coordinate with fabric color. 
d.	Motors:
1)	Motor type: Low voltage wired.  
2)	Motors: concealed inside headrail 
3)	Power Supply Type: Low voltage battery 12 VDC  
4)	Power Supply Type: Low voltage wall plug, 110V-120V VAC.  
5)	Power Supply Type: Solar Recharge Kit  
6)	Power Supply Type: 5-10 motor Transformer Kit
2.14	PLEATED SHADES
A.	Window Coverings: SWFcontract EvenPleat Pleated Shades.
1.	Fabric:  Flame retardant, fade and stain resistant.
a.	Compliance:
1)	Antifungal and Antibacterial:  ASTM G 21 and ASTM G 22. 
2)	FR Rating:  NFPA 701 (scroll FR fabric) 
b.	Description: Selected from an assortment of fade resistant, 100 percent polyester fabrics. EvenPleat technology ensures pleated material prevents sags or flattens.
c.	Seams: Shades with railroaded fabric will have heat-welded seams.
d.	Style: ____________.
e.	Color Name: ____________.
f.	Color Number: ____________.
g.	Fabric Style, Color Name, Color Number:  As scheduled and indicated on Drawings.
h.	Fabric Style, Color Name, Color Number: As selected by Architect from manufacturer's standard fabric range.
2.	Lift System: Standard.
a.	Cord Locks: Snap-in design, injection-molded thermoplastic, incorporating a metal, free-floating, serrated cord-locking roller. 
b.	Lift Cords: 0.9 mm polyester. A snap tassel and joiner ball connect to a single Danskord for raising and lowering the shade. Cord, tassel and joiner ball are color coordinated with fabric.
c.	Headrails: 
1)	Size: 0.812 inch (20.6 mm) high x 2 inches (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
d.	Bottomrails: Tubular shaped 0.024 inches (0.6 mm) thick phosphate-treated recycled steel and finished with a polyester primer and a topcoat of polyester baked enamel. The bottomrail shall be finished with a 7/8 inch (22 mm) wide crowned PVC slat, which is fitted into the last fabric pleat.
3.	Lift System: 
a.	Continuous Cord Loop Lift System: White cord loop controls lowering and raising shade.
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
c.	Bottomrails: Tubular shaped 0.024 inches (0.6 mm) thick phosphate-treated recycled steel and finished with a polyester primer and a topcoat of polyester baked enamel. The bottomrail shall be finished with a 7/8 inch (22 mm) wide crowned PVC slat, which is fitted into the last fabric pleat.
4.	Lift System: 
a.	Cordless Lift System: Lift and lowering operation without use of cord controls.
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
c.	Bottomrails: Tubular shaped 0.024 inches (0.6 mm) thick phosphate-treated recycled steel and finished with a polyester primer and a topcoat of polyester baked enamel. The bottomrail shall be finished with a 7/8 inch (22 mm) wide crowned PVC slat, which is fitted into the last fabric pleat. 
5.	Lift System: 
a.	Motor Lift System: Lift and lowering operation with a wireless controller 
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep. 
2)	Materials: Extruded aluminum headrail. 
3)	Wall Thickness: 0.045 inch (1.1 mm). 
4)	Finish: Painted to coordinate with fabric color. 
c.	Bottomrails: Tubular shaped 0.024 inches (0.6 mm) thick phosphate-treated recycled steel and finished with a polyester primer and a topcoat of polyester baked enamel. The bottomrail shall be finished with a 7/8 inch (22 mm) wide crowned PVC slat, which is fitted into the last fabric pleat.
d.	Motors:
1)	Motor type: Low voltage wired.  
2)	Motors: concealed inside headrail  
3)	Power Supply Type: Low voltage battery 12 VDC  
4)	Power Supply Type: Low voltage wall plug, 110V-120V VAC.  
5)	Power Supply Type: Solar Recharge Kit  
6)	Power Supply Type: 5-10 motor Transformer Kit  
B.	Window Coverings: SWFcontract FashionPleat Pleated Shades.
1.	Fabric:  Flame retardant, fade and stain resistant.
a.	Compliance:
1)	Antifungal and Antibacterial:  ASTM G 21 and ASTM G 22. 
2)	FR Rating:  NFPA 701 (scroll FR fabric) 
b.	Description: Selected from an assortment of fade resistant, 100 percent polyester fabrics.
c.	Seams: Shades with railroaded fabric will have heat-welded seams.
d.	Style: ____________.
e.	Color Name: ____________.
f.	Color Number: ____________.
g.	Fabric Style, Color Name, Color Number:  As scheduled and indicated on Drawings.
h.	Fabric Style, Color Name, Color Number: As selected by Architect from manufacturer's standard fabric range.
2.	Lift System: Standard.
a.	Cord Locks: Snap-in design, injection-molded thermoplastic, incorporating a metal, free-floating, serrated cord-locking roller. 
b.	Lift Cords: 0.9 mm polyester. A snap tassel and joiner ball connect to a single Danskord for raising and lowering the shade. Cord, tassel and joiner ball are color coordinated with fabric.
c.	Headrails: 
1)	Size: 0.812 inch (20.6 mm) high x 2 inches (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
d.	Bottomrails: Tubular shaped 0.024 inches (0.6 mm) thick phosphate-treated recycled steel and finished with a polyester primer and a topcoat of polyester baked enamel. The bottomrail shall be finished with a 7/8 inch (22 mm) wide crowned PVC slat, which is fitted into the last fabric pleat.
3.	Lift System: 
a.	Continuous Cord Loop Lift System: White cord loop controls lowering and raising shade.
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
c.	Bottomrails: Tubular shaped 0.024 inches (0.6 mm) thick phosphate-treated recycled steel and finished with a polyester primer and a topcoat of polyester baked enamel. The bottomrail shall be finished with a 7/8 inch (22 mm) wide crowned PVC slat, which is fitted into the last fabric pleat.
4.	Lift System: 
a.	Cordless Lift System: Lift and lowering operation without use of cord controls.
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep.
2)	Materials: Extruded aluminum headrail.
3)	Wall Thickness: 0.045 inch (1.1 mm).
4)	Finish: Painted to coordinate with fabric color.
c.	Bottomrails: Tubular shaped 0.024 inches (0.6 mm) thick phosphate-treated recycled steel and finished with a polyester primer and a topcoat of polyester baked enamel. The bottomrail shall be finished with a 7/8 inch (22 mm) wide crowned PVC slat, which is fitted into the last fabric pleat. 
5.	Lift System: 
a.	Motor Lift System: Lift and lowering operation with a wireless controller 
b.	Headrails: 
1)	Size: 1-7/16 inches (36.5 mm) high x 2 inch (51 mm) deep. 
2)	Materials: Extruded aluminum headrail. 
3)	Wall Thickness: 0.045 inch (1.1 mm). 
4)	Finish: Painted to coordinate with fabric color. 
c.	Bottomrails: Tubular shaped 0.024 inches (0.6 mm) thick phosphate-treated recycled steel and finished with a polyester primer and a topcoat of polyester baked enamel. The bottomrail shall be finished with a 7/8 inch (22 mm) wide crowned PVC slat, which is fitted into the last fabric pleat. 
d.	Motors:
1)	Motor type: Low voltage wired.  
2)	Motors: concealed inside headrail 
3)	Power Supply Type: Low voltage battery 12 VDC  
4)	Power Supply Type: Low voltage wall plug, 110V-120V VAC.  
5)	Power Supply Type: Solar Recharge Kit  
6)	Power Supply Type: 5-10 motor Transformer Kit 
PART 3    EXECUTION
3.1	PREPARATION
A.	Inspect mounting surfaces, blocking for shade brackets or pocket assemblies, suspended acoustical or gypsum ceiling for recessed shades and verify field measurements. Prepare substrates using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions. 
B.	Do not proceed with installation until substrates have been prepared using the methods recommended by the manufacturer and deviations from manufacturer's recommended tolerances are corrected. Commencement of installation constitutes acceptance of conditions.
C.	If preparation is the responsibility of another installer, notify Architect in writing of deviations from manufacturer's recommended installation tolerances and conditions.
3.2	INSTALLATION
A.	Install window treatments in accordance with manufacturer's instructions including the following.
1.	Install with adequate clearance to permit smooth operation of the shades throughout entire operational range. 
2.	Adjust and balance window coverings to operate smoothly, easily, safely, and free from binding or malfunction throughout entire operational range.
3.	Wire motors and controllers according to specifications and wiring diagrams prior to installation of motorized shades.
4.	Test electrically operated shades for proper operation.
3.3	CLEANING AND PROTECTION
A.	Clean surfaces after installation in accordance with manufacturer's written instructions. Do not use cleaning methods involving heat, bleach, abrasives, or solvents.
B.	Protect installed products until completion of project. Repair damaged or improperly installed before Substantial Completion.

END OF SECTION