SECTION 03 05 13

CONCRETE WASHOUT SYSTEM

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2025 -  2025 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Concrete Washout System with Integrated Brackets for Crane Lifting.
B.	RELATED SECTIONS
C.	Section 01 50 00 - Temporary Facilities and Controls
D.	Section 01 74 19 - Cleaning and Waste Management and Disposal
E.	Division 03, Concrete Sections.
1.2	REFERENCES
A.	Environmental Protection Agency (EPA), compliant.
B.	Environmental Protection Agency:
1.	National Pollutant Discharge Elimination System (NPDES), Construction General Permit; Current Edition, compliant.
C.	U.S. Green Building Council (USGBC):
1.	LEED v4.1-BD+C - LEED v4.1 for Building Design and Construction; 2023, compliant.
D.	Stormwater Pollution Prevention Plan, compliant.
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00, Administrative Requirements.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Instructions and recommendations for use.
3.	Storage and handling requirements.
1.4	QUALITY ASSURANCE
A.	Contractor/Equipment Operator Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
1.5	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.6	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results.
1.7	WARRANTY
A.	Manufacturer's standard lifetime warranty unless indicated otherwise.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: The Bone Bucket, which is located at:<BR />4370 N Poplar St.<BR />Eagle Mountain, UT 84005<BR />Tel: 385-221-9106<BR />Email: request info (bones@thebonebucket.com);Web: https://thebonebucket.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with the provisions of Section 01 60 00.
2.2	PRODUCT TYPES
A.	Above Grade Portable Concrete Washout:
1.	Basis of Design: Bone Bucket; as manufactured and supplied by The Bone Bucket; www.thebonebucket.com.
a.	Material: Plastic.
b.	Size (LxWxH): 78.4 inch (1991 mm) x 58.4 inch (1483 mm) x 12.3 inch (312 mm).
c.	Maximum Fill Volume: 0.75 cubic yards (approximately 8-10 trucks).
d.	Thickness: 1/4 inch (6.35 mm).
e.	Ice tray design, stackable, and reusable.
f.	Forklift slots for mobility.
g.	Pre-installed crane-liftable brackets.
PART 3    EXECUTION
3.1	PREPARATION
A.	Identify washout basin locations.
B.	Place on-site recycle basins.
C.	Collect concrete waste and washout in accordance with the Authority Having Jurisdiction.
D.	Place washout basins on flat, stable surface.
3.2	INSTALLATION AND USE
A.	Maintain and conduct installation and maintenance of basins in accordance with manufacturer's written requirements and the Authority Having Jurisdiction.
B.	Instructions for Use:
1.	Pour concrete washout into basin.
2.	Allow to dry.
3.	Once dry, flip the basin with a forklift to disengage dried concrete washout.
4.	Dispose of dried concrete washout in accordance with Section 01 74 19, Cleaning and Waste Management and Disposal.
5.	Repeat until concrete washout disposal is complete.
3.3	FIELD QUALITY CONTROL
A.	Do not allow washout materials or water into drainage ways, water bodies, wetlands or in the right-of-way of roadways.
B.	Do not bury waste materials.
C.	Dispose of waste in accordance with Authority Having Jurisdiction.
D.	Inspect basins after each use.
E.	Replace basin when basin can no longer safely hold or transport washout.
3.4	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturer's recommendations.
B.	Remove basins from site at completion of the Work and prior to Substantial Completion.

END OF SECTION