SECTION 08 71 13

COMMERCIAL DOOR OPERATORS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2017 -  2020 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Rolling Door and Grille Operators.
B.	Rolling Fire Door Operators.
C.	Sectional Door Operators.
D.	Counter Door Operators.
1.2	RELATED SECTIONS
A.	Section 05 50 00 - Metal Fabrications.
B.	Section 06 20 00 - Finish Carpentry.
C.	Section 08 33 36 - Side Coiling Grilles.
D.	Section 08 33 23 - Coiling Doors.
E.	Section 08 33 13 - Coiling Doors.
F.	Section 08 33 00 - Coiling Doors and Grilles.
G.	Section 08 36 16 - Single-Panel Doors.
H.	Section 08 71 53 - Security Door Hardware.
I.	Section 09 90 00 - Painting and Coating.
J.	Section 27 05 39 - Surface Raceways for Communications Systems.
K.	Section 26 05 00 - Common Work Results for Electrical.
1.3	REFERENCES
A.	NEMA 250 - Enclosures for Electrical Equipment (1000 Volts Maximum).
B.	NEMA 7 - Enclosures for hazardous locations Class I, Division 1, Group D, T2C
C.	NEMA 9 - Enclosures for hazardous locations Class II, Division 1, Groups F and G, T2C
D.	NEMA ICS 6 - Enclosures for Industrial Controls and Systems.
E.	NEMA MG 1 - Motors and Generators.
1.4	DESIGN / PERFORMANCE REQUIREMENTS
A.	Products Requiring Electrical Connection: Listed and classified by Underwriters Laboratories, Inc. acceptable to authority having jurisdiction as suitable for purpose specified.
B.	Electric Motors shall be alternating-current squirrel-cage motors conforming with NEMA MG 1.
C.	Fire Door Operators: Provide with Factory Mutual approval and complying to and listed in UL Directory.
D.	Explosion-proof Electric Motors shall be UL and CSA listed for hazardous location use in areas classified as Class I, Division I, Group D, T2C and Class II, Division I, Groups F and G, T2C.
E.	Explosion-proof Operators: Provide with Factory Mutual approval.
F.	Wiring Connections: Requirements for electrical characteristics.
1.	115 volts, 60 Hz single phase.
2.	208 volts, 60 Hz single phase or three phase.
3.	230 volts, 60 Hz single phase or three phase.
4.	460 volts, 60 Hz three phase.
5.	575 volts, 60 Hz three phase.
G.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
H.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Details of construction and fabrication.
4.	Installation methods.
I.	Shop Drawings: Include detailed plans, elevations, details of framing members, required clearances and accessories. Include relationship with adjacent construction.
J.	Manufacturer's Certificates: Certify products meet or exceed specified requirements.
K.	Operation and Maintenance Data: Submit lubrication requirements and frequency, and periodic adjustments required.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified with minimum of five years documented experience.
B.	Installer Qualifications: Authorized representative of the manufacturer with minimum five years documented experience.
C.	Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
1.	Install in areas designated by Architect.
2.	Do not proceed with remaining work until workmanship and installation is approved by Architect.
3.	Refinish mock-up area as required to produce acceptable work.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging until ready for installation.
B.	Protect materials from exposure to moisture. Do not deliver until after wet work is complete and dry.
C.	Store materials in a dry, warm, ventilated weathertight location.
1.7	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
1.8	WARRANTY
A.	Provide operators with a 2 year or 20,000 cycle limited warranty on motor and parts.
B.	Provide operators with a 2 year limited warranty on motor and parts.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: The Genie Company, which is located at:<BR />P. O. Box 67, One Door Dr.<BR />Mt. Hope, OH 44660<BR />Toll Free Tel: 800-843-4084<BR />Fax: 800-221-0132<BR />Email: request info (genie_company@geniecompany.com);Web: http://www.geniecompany.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	ROLLING DOOR AND GRILLE OPERATORS
A.	Heavy Duty Rolling Door and Grille Operator: Model GCL-GH True Gear Head Type Door Operator:
1.	Application:
a.	Rolling Steel Doors.
b.	Rolling Steel Fire Doors.
c.	Rolling Steel Grille.
2.	Electric Motor: UL listed.
a.	Rating:
1)	1/2 horsepower single phase or three phase with automatic thermal reset overload.
2)	3/4 horsepower or 1 horsepower single phase with manual reset overload.
3)	3/4 horsepower or 1 horsepower three phase with automatic thermal reset overload.
4)	3 horsepower three phase with automatic thermal reset overload.
b.	Motor frame comply with: 
1)	NEMA 48 for 1/2 hp single phase.
2)	NEMA 56 for 1/2 hp three phase.
3)	NEMA 56 3/4 and 1 hp all phases.
4)	NEMA 56 for 3 hp three phase.
c.	Construction: 
1)	Open drip-proof construction.
2)	Totally Enclosed Non Ventilated - TENV construction.
3)	Totally Enclosed Fan Cooled - TEFC construction.
4)	Washdown - NEMA 4 / NEMA 4X construction
d.	The operator shall be suited for: 
1)	NEMA ICS 6 Type 1 general purpose environment.
2)	NEMA ICS 6 Type 4 water tight dust tight environment.
3)	NEMA ICS 6 Type 4X water tight dust tight environment with corrosion resistance.
e.	Reduction: Primary reduction is worm gear in oil bath.
f.	Duty cycle: Accommodate heavy usage, up to 60 cycles per hour under a large constant load.
1)	Brake: DC Disc type with selectable Progressive Braking for smooth stopping.
2)	Clutch: Adjustable torque-limiter type. 
3)	Limit System: EZ limit system, magnetic type providing absolute positioning with push to set capability. Limit system shall remain synchronized with the door during manual operation and supply power interruptions.
3.	Control System: Microprocessor based with relay motor controls on a single board. System incorporates a 16 character Liquid Crystal Display (LCD) to display the system status. System shall include the following:
a.	Capable of monitoring and reporting on a variety of operating conditions, including: Current operating status, Current command status, Motor movement status, Current error status (if applicable), Hoist Interlock status (if applicable), External Interlock status, and 24VDC status. 
b.	A delay-on-reverse operating protocol. 
c.	Maximum run timers in both directions of travel that limit motor run time in the event a clutch slips or some other problem occurs. 
d.	Provisions for the connection of a 2-wire monitored photo-eye or a 2-wire monitored edge sensor, as well as non-monitored 2-wire sensing edges, photo-eyes or other entrapment protection devices. 
e.	Control action will be constant contact close until a monitored entrapment device is installed, allowing for selection of momentary contact.
f.	Provisions for connection of single and/or 3-button control stations. 
g.	Provisions for connection of an external 3-wire radio controls and related control devices. 
h.	On board open, close and stop control keys for local operation. 
i.	Intellicode 315Mhz radio receiver capable of storing 50 single button and/or 50 Open-Close-Stop transmitters with the ability to add and/or delete transmitters individually, identify and store activating transmitter IDs. 
4.	Mounting:
a.	Rolling Steel doors:
1)	Front of hood and chain/sprocket coupling to door.
2)	Top of hood and chain/sprocket coupling to door.
3)	Wall-mount and chain/sprocket coupling to door.
4)	Bench mount and chain/sprocket coupling to door.
5.	Release:
a.	Release shall be a pull and hold type mechanism with single cable operation and an integrated interlock switch on hoist units.
6.	Hoist: Chain hoist consists of chain pocket wheel, chain guard and smooth hand chain on hoist units.
7.	Entrapment Protection: 
a.	Control system shall have provisions to connect monitored entrapment protection devices such as monitored electric sensing edge, or monitored photo-eye and to provide constant contact close control operation in lieu of such devices.
8.	Control accessories:
a.	Operator Controls: 
1)	Push-button operated control stations with open, close, and stop buttons.
2)	Key operation with open, close, and stop controls.
3)	Push-button and key operated control stations with open, close, and stop buttons.
4)	Controls for interior location.
5)	Controls for exterior location.
6)	Controls for both interior and exterior location. 
7)	Controls surface mounted.
8)	Controls flush mounted.
b.	Special Operation: 
1)	Vehicle detector operation.
2)	Radio control operation.
3)	GENIE monitored photo-eyes.
4)	Commercial photo-eyes.
5)	Timer Close Module for unattended timed door closing. Auxiliary control inputs, safety inputs, timer hold input and automatic door closing feature with selectable time delay. Safety inputs can be configured using on board keypad.
6)	Commercial light package.
7)	Auxiliary Output Module for up, down, and mid-stop limit status via several auxiliary sets of dry contacts that are microprocessor controlled. ADA compliant outputs that activate when door is moving up, down, or both directions and can be configured using the on board keypad.
B.	Hazardous Location NEMA 7/9 Heavy Duty Rolling Door and Grille Operator: Model GCL-GH True Gear Head Type Door Operator:
1.	Application:
a.	Rolling Steel Doors.
b.	Rolling Steel Fire Doors.
c.	Rolling Steel Grille.
2.	Electric Motor: UL listed.
a.	Rating:
1)	1/2 horsepower single phase with automatic thermal reset overload with ability to configure for voltages of 115/208/230V.
2)	1 horsepower three phase with automatic thermal reset overload with ability to configure for voltages of 208/230/460V.
3)	3 horsepower three phase with automatic thermal reset overload with ability to configure for voltages of 208/230/460V.
b.	Motor frame comply with:
1)	NEMA 56C for 1/2 hp single phase.
2)	NEMA 56C for 1 hp three phase.
3)	NEMA 182C for 3 hp three phase.
c.	Construction:
1)	Hazardous location NEMA 7 construction.
2)	Hazardous location NEMA 9 construction.
d.	The operator shall be suited for:
1)	NEMA Type 7 construction for indoor use in hazardous (classified) locations classified as Class I, Division I, Group D, T2C, as defined in NFPA 70. 
2)	NEMA Type 9 construction for indoor use in hazardous (classified) locations classified as Class II, Division I, Groups F and G, T2C as defined in NFPA 70.
e.	Reduction: Primary reduction is worm gear in oil bath.
f.	Duty cycle: Accommodate heavy usage, up to 60 cycles per hour under a large constant load.
1)	Brake: Motor and electrical system will provide dynamic braking.
2)	Clutch: Optional adjustable torque-limiter type. Not available on 3 horsepower models.
3)	Limit System: Limit system shall be rotary type with vernier adjustment, synchronized with door during release operation. Limit system shall incorporate intrinsically safe wiring.
3.	Control System: Microprocessor based with on-board configuration and diagnostic LEDs. This system shall be capable of monitoring and reporting on a variety of operating conditions, including: Current operating status, Current maximum run time status, Motor running status, Current error status (if applicable), Timer to close status (if applicable), Open limit status, Close limit status, and Cycle count. System shall include the following:
a.	A delay-on-reverse operating protocol.
b.	The system shall include maximum run timers in both directions of travel that limit motor run time in the event a clutch slips or some other problem occurs.
c.	It shall include provisions for the connection of a 2-wire T2 monitored edge sensor for entrapment protection. 
d.	Control action will be constant contact close until a monitored entrapment device is installed, allowing for selection of momentary contact. 
e.	The system shall include provisions for connection of single or 3-button control stations. 
f.	The control system shall include on board open, close and stop control keys for local operation.
g.	The system shall include provisions for automatic door closure upon reaching the open limit and completion of adjustable time delay.
4.	Mounting:
a.	Rolling Steel doors:
1)	Front of hood and chain/sprocket coupling to door.
2)	Top of hood and chain/sprocket coupling to door.
3)	Wall-mount and chain/sprocket coupling to door.
4)	Bench mount and chain/sprocket coupling to door.
5.	Release:
a.	Release shall be a pull and hold type mechanism with single cable operation and an integrated interlock switch.
6.	Hoist: 
a.	Chain hoist consists of chain pocket wheel, chain guard and smooth hand chain on hoist units. Hoist must be field adjustable for Right Hand or Left Hand mounting.
7.	Entrapment Protection:
a.	UL 325 momentary contact control system shall have provisions to connect intrinsically safe monitored entrapment protection electric sensing edge, and to provide constant contact close control operation in lieu of such device.
8.	Control accessories:
a.	Operator Controls:
1)	Push-button operated control stations with open, close, and stop buttons.
2)	Key operation with open, close, and stop controls.
3)	Push-button and key operated control stations with open, close, and stop buttons.
4)	Controls for interior location.
5)	Controls for exterior location.
6)	Controls for both interior and exterior location.
7)	Controls surface mounted.
8)	Controls flush mounted.
C.	Commercial Rolling Door and Grille Operator: Model GCL-H/GCL-J Commercial Standard Duty Door Operator:
1.	Application:
a.	Rolling Steel Doors.
b.	Rolling Steel Fire Doors.
c.	Rolling Steel Grilles.
2.	Electric Motor: UL listed.
a.	Rating:
1)	1/2 horsepower single phase or three.
2)	3/4 single phase or three phase.
3)	1 horsepower single phase or three phase.
b.	Motor frame comply with: 
1)	NEMA 48 for 1/2 hp single phase.
2)	NEMA 56 for 1/2 hp three phase.
3)	NEMA 56 3/4 and 1 hp all phases.
c.	Construction: 
1)	Open drip-proof construction.
2)	Totally Enclosed Non Ventilated - TENV construction.
3)	Totally Enclosed Fan Cooled - TEFC construction.
4)	Washdown - NEMA 4 / NEMA 4X construction
d.	Reduction: Primary reduction is TensiBelt, an auto tension poly-V flex belt that does not require adjustment. Secondary reduction is by chain and sprocket.
e.	Duty cycle: Accommodate standard usage, up to 30 cycles per hour during peak usage periods.
1)	Brake: DC Disc type with selectable Progressive Braking for smooth stopping.
2)	Clutch: Adjustable friction disc type. 
3)	Limit System: EZ limit system, magnetic type providing absolute positioning with push to set capability. Limit System shall remain synchronized with the door during manual operation and supply power interruptions.
3.	Control System: Microprocessor based with relay motor controls on a single board. System incorporates a 16 character Liquid Crystal Display (LCD) to display the system status. System shall include the following:
a.	Capable of monitoring and reporting on a variety of operating conditions, including: Current operating status, Current command status, Motor movement status, Current error status (if applicable), Hoist Interlock status (if applicable), External Interlock status, and 24VDC status. 
b.	A delay-on-reverse operating protocol. 
c.	Maximum run timers in both directions of travel that limit motor run time in the event a clutch slips or some other problem occurs. 
d.	Provisions for connection of a 2-wire monitored photo-eye or a 2-wire monitored edge sensor, as well as non-monitored standard 2-wire sensing edges, photo-eyes or other entrapment protection devices. 
e.	Control action will be constant contact close until a monitored entrapment device is installed, allowing for selection of momentary contact.
f.	Provisions for connection of single and/or 3-button control stations. 
g.	Provisions for connection of an external 3-wire radio controls and related control devices. 
h.	On board open, close and stop control keys for local operation. 
i.	Intellicode 315Mhz radio receiver capable of storing 50 single button and/or 50 Open-Close-Stop transmitters with the ability to add and/or delete transmitters individually, identify and store activating transmitter IDs. 
4.	Mounting:
a.	Rolling Steel doors:
1)	Front of hood and chain/sprocket coupling to door.
2)	Top of hood and chain/sprocket coupling to door.
3)	Wall-mount and chain/sprocket coupling to door.
4)	Bench mount and chain/sprocket coupling to door.
5)	Front of hood horizontal and chain/sprocket coupling to door.
6)	Mounting for Hoist models, Left Hand or Right Hand.
5.	Release:
a.	Release shall be a pull and hold type mechanism with single cable operation and an integrated interlock switch.
6.	Hoist: Chain hoist consists of chain pocket wheel, chain guard and smooth hand chain on hoist units.
7.	Entrapment Protection: 
a.	Control system shall have provisions to connect monitored entrapment protection devices such as monitored electric sensing edge or monitored photo-eye and to provide constant contact close control operation in lieu of such devices.
8.	Control accessories:
a.	Operator Controls: 
1)	Push-button operated control stations with open, close, and stop buttons.
2)	Key operation with open, close, and stop controls.
3)	Push-button and key operated control stations with open, close, and stop buttons.
4)	Controls for interior location.
5)	Controls for exterior location.
6)	Controls for both interior and exterior location. 
7)	Controls surface mounted.
8)	Controls flush mounted.
b.	Special Operation: 
1)	Vehicle detector operation.
2)	Radio control operation.
3)	GENIE monitored photo-eyes.
4)	Commercial photo-eyes.
5)	Timer Close Module for unattended timed door closing. Auxiliary control inputs, safety inputs, timer hold input and automatic door closing feature with selectable time delay. Safety inputs can be configured using on board keypad. 
6)	Commercial light package.
7)	Auxiliary Output Module for up, down, and mid-stop limit status via several auxiliary sets of dry contacts that are microprocessor controlled. ADA compliant outputs that activate when door is moving up, down, or both directions and can be configured using the on board keypad.
D.	Commercial Rolling Grille Operator: GCL-J Commercial Standard Duty Egress Operator: 
1.	Application: 
a.	Rolling Steel Grilles. 
2.	Electric Motor: UL listed. 
a.	Rating: 
1)	1/2 horsepower single phase or three. 
2)	1 horsepower single phase or three phase. 
b.	Motor frame comply with: 
1)	NEMA 48 for 1/2 hp single phase. 
2)	NEMA 56 for 1/2 hp three phase. 
3)	NEMA 56 for 1 hp all phases. 
c.	Construction: 
1)	Open drip-proof construction. 
d.	Reduction: Primary reduction is TensiBelt, an auto tension poly-V flex belt that does not require adjustment. Secondary reduction is by chain and sprocket. 
e.	Duty cycle: Accommodate standard usage, up to 30 cycles per hour during peak usage periods. 
1)	Brake: DC Disc type with selectable Progressive Braking for smooth stopping. 
2)	Clutch: Adjustable friction disc type on primary reduction. 
3)	Limit System: EZ Limit system, magnetic type providing absolute positioning with push to set capability. Limit System shall remain synchronized with the door during manual operation, supply power interruptions, and after emergency egress release. 
4)	Door Release Clutch: 24VDC solenoid activated clutch that releases up upon loss of primary power. 
5)	Integral Centrifugal Governor: Governor shall limit door ascent speed during emergency egress test or alarm activated release. 
3.	Control System: Microprocessor based with relay motor controls on a single board. System incorporates a 16 character Liquid Crystal Display (LCD) to display the system status. System shall include the following: 
a.	Capable of monitoring and reporting on a variety of operating conditions, including: Current operating status, Current command status, Motor movement status, Current error status (if applicable), Hoist Interlock status (if applicable), External Interlock status, and 24VDC status. 
b.	A delay-on-reverse operating protocol. 
c.	Maximum run timers in both directions of travel that limit motor run time in the event a clutch slips or some other problem occurs. 
d.	Provisions for connection of a 2-wire monitored photo-eye or a 2-wire monitored edge sensor, as well as non-monitored standard 2-wire sensing edges, photo-eyes or other entrapment protection devices. 
e.	Control action will be constant contact close until a monitored entrapment device is installed, allowing for selection of momentary contact. 
f.	Provisions for connection of single and/or 3-button control stations. 
g.	Provisions for connection of an external 3-wire radio controls and related control devices. 
h.	On board open, close and stop control keys for local operation. 
i.	Egress activation form C output for notification of local egress activation to remote alarm system. 
j.	Capable of remote egress activation via normally closed contact to egress input for emergency egress operation. 
k.	Input for normally closed contact operation by test key switch or push-pull type emergency egress control station. 
l.	Intellicode 315 Mhz radio receiver capable of storing 50 single button and/or 50 Open-Close-Stop transmitters with the ability to add and/or delete transmitters individually, identify and store activating transmitter IDs. 
4.	Mounting: 
a.	Rolling Steel Grilles: 
1)	Front of hood and chain/sprocket coupling to door. 
2)	Top of hood and chain/sprocket coupling to door. 
3)	Wall-mount and chain/sprocket coupling to door. 
5.	Release: 
a.	Release shall be a 24VDC solenoid activated clutch that releases up upon loss of primary power, or removal of 24VDC from clutch controlled by internal egress accessory board. 
6.	Entrapment Protection: 
a.	Control system shall have provisions to connect monitored entrapment protection devices such as monitored electric sensing edge or monitored photo-eye and to provide constant contact close control operation in lieu of such devices. 
7.	Control accessories: 
a.	Operator Controls: 
1)	Push-button operated control stations with open, close, and stop buttons. 
2)	Key operation with open, close, and stop controls. 
3)	Push-button and key operated control stations with open, close, and stop buttons. 
4)	Test key operated control station for testing of emergency egress operation. 
5)	Push-pull button operation for local emergency egress activation. 
6)	Controls for interior location. 
7)	Controls for exterior location. 
8)	Controls for both interior and exterior location. 
9)	Controls surface mounted. 
10)	Controls flush mounted. 
b.	Special Operation: 
1)	Vehicle detector operation. 
2)	Radio control operation. 
3)	Genie monitored photo-eyes. 
4)	Commercial photo-eyes. 
5)	Timer Close Module for unattended timed door closing. Auxiliary control inputs, safety inputs, timer hold input and automatic door closing feature with selectable time delay. Safety inputs can be configured using on board keypad. 
6)	Commercial light package. 
7)	Auxiliary Output Module for up, down, and mid-stop limit status via several auxiliary sets of dry contacts that are microprocessor controlled. ADA compliant outputs that activate when door is moving up, down, or both directions and can be configured using the on board keypad. 
E.	Commercial Rolling Door and Grille Operator: Model GCL-MH/GCL-MJ Door Operator:
1.	Application:
a.	Rolling Steel Door.
b.	Rolling Steel Grille.
2.	Electric Motor: UL listed.
a.	Rating:
1)	1/2 horsepower single phase with automatic thermal reset overload.
b.	Motor frame comply with: 
1)	NEMA 42 for 1/2 hp single phase.
c.	Construction: 
1)	Open drip-proof construction.
d.	Reduction: Primary reduction is TensiBelt poly-V flex auto tension belt. Secondary reduction is by chain and sprocket.
e.	Duty cycle: Accommodate medium usage, up to 15 cycles per hour.
1)	Brake: Solenoid actuated band type.
2)	Clutch: Adjustable friction disc type.
3)	Limit System: Adjustable linear type synchronized with the door during release operation. Limit activation by opto-sensors.
3.	Control System: Microprocessor based with relay motor controls on a single board. System incorporates a Liquid Crystal Display (LCD) to display the system status. System shall include the following:
a.	A delay-on-reverse operating protocol. 
b.	Maximum run timers in both directions of travel that limit motor run time in the event a clutch slips or some other problem occurs. 
c.	Provisions for the connection of a 2-wire monitored photo-eye or a 2-wire monitored edge sensor, as well as non-monitored 2-wire sensing edges, photo-eyes or other entrapment protection devices.
d.	Control action will be constant contact close until a monitored entrapment device is installed, allowing for selection of momentary contact.
e.	Provisions for connection of single and/or 3-button control stations. 
f.	Provisions for connection of an external 3-wire radio controls and related control devices. 
g.	On board open, close and stop control keys for local operation. 
4.	Mounting:
a.	Rolling Steel doors:
1)	Front of hood and chain/sprocket coupling to door.
2)	Top of hood and chain/sprocket coupling to door.
3)	Wall-mount and chain/sprocket coupling to door.
4)	Mounting for Hoist models shall be Right Hand.
5.	Release:
a.	Release shall be a pull and hold type mechanism with single cable operation and an integrated interlock switch on hoist units.
6.	Hoist: Chain hoist with chain pocket wheel, chain guard and smooth hand chain on hoist units.
7.	Entrapment Protection: 
a.	Control system shall have provisions to connect monitored entrapment protection devices such as monitored electric sensing edge, or monitored photo-eye and to provide constant contact close control operation in lieu of such devices
8.	Control accessories:
a.	Operator Controls: 
1)	Push-button operated control stations with open, close, and stop buttons.
2)	Key operation with open, close, and stop controls.
3)	Push-button and key operated control stations with open, close, and stop buttons.
4)	Controls for interior location.
5)	Controls for exterior location.
6)	Controls for both interior and exterior location. 
7)	Controls surface mounted.
8)	Controls flush mounted.
b.	Special Operation: 
1)	Radio control operation.
2)	GENIE monitored photo-eyes.
3)	Commercial photo-eyes.
4)	Timer Close Module for unattended timed door closing. Auxiliary control inputs, safety inputs, timer hold input and automatic door closing feature with selectable time delay. Safety inputs can be configured using on board keypad.
5)	Auxiliary Output Module for up, down, and mid-stop limit status via several auxiliary sets of dry contacts that are microprocessor controlled. ADA compliant outputs that activate when door is moving up, down, or both directions and can be configured using the on board keypad.
2.3	ROLLING FIRE DOOR OPERATOR
A.	Commercial Rolling Steel Fire Door Operator: Model GCL-H Commercial Standard Duty Fire Door Operator:
1.	Application:
a.	Rolling Steel Fire Doors.
2.	Electric Motor: UL listed.
a.	Rating:
1)	1/2 horsepower single phase or three.
2)	3/4 single phase or three phase.
3)	1 horsepower single phase or three phase.
b.	Motor frame comply with:
1)	NEMA 48 for 1/2 hp single phase.
2)	NEMA 56 for 1/2 hp three phase.
3)	NEMA 56 3/4 and 1 hp all phases.
c.	Construction: Open drip-proof construction.
d.	Reduction: Primary reduction is TensiBelt, an auto tension poly-V flex belt that does not require adjustment. Secondary reduction is by chain and sprocket.
e.	Duty Cycle: Accommodate standard usage, up to 60 cycles per hour during peak usage periods.
1)	Brake: DC Disc type with selectable Progressive Braking for smooth stopping.
2)	Clutch: Adjustable friction disc type.
3)	Door Release Clutch: 24VDC solenoid activated clutch that releases up upon loss of primary and battery backup power.
4)	Limit System: EZ limit system, magnetic type providing absolute positioning with push to set capability. Limit System shall remain synchronized with the door during manual operation, supply power interruptions, and fire door release operation.
5)	Integral Centrifugal Governor: Governor shall limit door drop speed during manual test or alarm activated release.
3.	Control System: Microprocessor based with relay motor controls on a single board. System incorporates a 16 character Liquid Crystal Display (LCD) to display the system status. System shall include the following:
a.	Provide with an internal battery backup system capable of providing up to 24 hours of battery power to support alarm logic, smoke detector, release capability and audible and visible signaling appliances. Device shall monitor battery charge and annunciate the need for battery replacement via an integral sounder; an LCD display that indicates battery low condition. Battery backup/power system shall contain a management system providing trickle charge capabilities. 
b.	During a power outage, and upon depletion of the battery, the device will initiate door closure by releasing the electric clutch.
c.	Monitoring for an Alarm input while on internal battery backup power.
d.	Initiate gravity door closure through the release of the Door Release Clutch
e.	Includes LCD display selectable delay settings of 10, 20, 30 or 60 seconds upon alarm activation to allow for passageway clearance before initiating door closure.
f.	Capable of receiving an alarm input from compatible 2-wire normally open smoke detectors, 4-wire normally open smoke detectors, or normally open heat detectors, or input from a fire alarm control panel via a relay module providing a Form C dry contact output to the release device.
g.	Capable of receiving input from a maximum of two smoke detectors requiring use of an End-of-Line (EOL) device to ensure the integrity of the wiring.
h.	Provide with audible and visual signaling appliances to operate during the alarm closing cycle. Device shall be capable of activating and powering up to two (optional) audible/visible notification devices, e.g. strobes, horns or horn/strobes. 
i.	Fire door operator shall recognize that the door is in the closed position through monitoring of door position to prevent release of the Door Release Clutch when the door is closed.
j.	Provide with relay and trouble outputs to provide notification to a fire alarm control panel when an alarm or trouble state exists. 
k.	Circuit board shall have LCD display and diagnostic LEDs to assist with field installation by indicating alarm or trouble conditions present within the alarm activation device(s) or notification appliance(s).
l.	Operator shall provide remote key test switch to simulate an alarm condition during testing procedures.
m.	Operator shall provide an LCD configuration setting selectable for 2-minute or 4-minute safety timer that will initiate gravity door closure if the operator close cycle is not completed within the selected time. 
n.	Upon alarm, the operator shall attempt motorized door closure. 
o.	Upon alarm the operator shall provide release on obstruction selectable through the LCD display on the operator via a monitored sensing edge (by others). 
p.	Upon alarm the operator shall provide one or three time obstruction cycling of the door selectable through the LCD display on the operator via a monitored sensing edge (by others). 
q.	Operator shall provide an LCD configurable feature allowing automatic open after routine testing. 
r.	One audible and visual signaling appliance shall be provided to annunciate closure due to alarm, power loss conditions or test mode. 
s.	Capable of monitoring and reporting on a variety of operating conditions, including: Current operating status, Current command status, Motor movement status, Current error status (if applicable), Hoist Interlock status (if applicable), External Interlock status, and 24VDC status.
t.	Maximum run timers in both directions of travel that limit motor run time in the event a clutch slips or some other problem occurs.
u.	Provisions for connection of a 2-wire monitored photo-eye or a 2-wire monitored edge sensor, as well as non-monitored standard 2-wire sensing edges, photo-eyes or other entrapment protection devices.
v.	Control action will be constant contact close until a monitored entrapment device is installed, allowing for selection of momentary contact.
w.	Provisions for connection of single and/or 3-button control stations.
x.	On board open, close and stop control keys for local operation.
y.	Intellicode 315Mhz radio receiver capable of storing 50 single button and/or 50 Open-Close-Stop transmitters with the ability to add and/or delete transmitters individually, identify and store activating transmitter IDs.
z.	On board non-resettable cycle counter.
4.	Mounting:
a.	Rolling Steel doors:
1)	Front of hood and chain/sprocket coupling to door.
2)	Top of hood and chain/sprocket coupling to door.
3)	Wall-mount and chain/sprocket coupling to door.
4)	Bench mount and chain/sprocket coupling to door.
5)	Front of hood horizontal and chain/sprocket coupling to door.
6)	Mounting for Hoist models, Left Hand or Right Hand.
5.	Release: Release shall be a pull and hold type mechanism with single cable operation and an integrated interlock switch.
6.	Hoist: Chain hoist consists of chain pocket wheel, chain guard and smooth hand chain on hoist units.
7.	Fusible Release: Capable of holding and releasing door via a fusible link/sash chain assembly attached to a release mechanism within the operator construction.
8.	Entrapment Protection:
a.	Control system shall have provisions to connect monitored entrapment protection devices such as monitored electric sensing edge or monitored photo-eye and to provide constant contact close control operation in lieu of such devices. 
9.	Control accessories:
a.	Operator Controls:
1)	Push-button operated control stations with open, close, and stop buttons.
2)	Key operation with open, close, and stop controls.
3)	Push-button and key operated control stations with open, close, and stop buttons.
4)	Controls for interior location.
5)	Controls for exterior location.
6)	Controls for both interior and exterior location.
7)	Controls surface mounted.
8)	Controls flush mounted.
b.	Special Operation:
1)	Vehicle detector operation.
2)	Radio control operation.
3)	GENIE monitored photo-eyes.
4)	Commercial photo-eyes.
5)	Timer Close Module for unattended timed door closing. Auxiliary control inputs, safety inputs, timer hold input and automatic door closing feature with selectable time delay. Safety inputs can be configured using on board keypad.
6)	Visual and/or audible signal devices.
7)	Auxiliary Output Module for up, down, and mid-stop limit status via several auxiliary sets of dry contacts that are microprocessor controlled. ADA compliant outputs that activate when door is moving up, down, or both directions and can be configured using the on board keypad.
2.4	SECTIONAL DOOR OPERATORS
A.	Heavy Duty Sectional Door Operator: Model GCL-GT/GCL-GH True Gear Head Type Door Operator:
1.	Application:
a.	Standard Lift Sectional Door.
b.	Lift Clearance Sectional Door.
c.	Full Vertical Sectional Door.
2.	Electric Motor: UL listed.
a.	Rating:
1)	1/2 horsepower single phase or three phase with automatic thermal reset overload.
2)	3/4 horsepower or 1 horsepower single phase with manual reset overload.
3)	3/4 horsepower or 1 horsepower three phase with automatic thermal reset overload.
4)	3 horsepower three phase with automatic thermal reset overload.
b.	Motor frame comply with: 
1)	NEMA 48 for 1/2 hp single phase.
2)	NEMA 56 for 1/2 hp three phase.
3)	NEMA 56 3/4 and 1 hp all phases.
4)	NEMA 56 for 3 hp three phase.
c.	Construction: 
1)	Open drip-proof construction.
2)	Totally Enclosed Non Ventilated - TENV construction.
3)	Totally Enclosed Fan Cooled - TEFC construction.
4)	Washdown - NEMA 4 / NEMA 4X construction
d.	Reduction: Primary reduction is worm gear in oil bath. 
e.	Duty cycle: Accommodate heavy usage, up to 60 cycles per hour under a large constant load.
1)	Brake: DC Disc type with selectable Progressive Braking for smooth stopping.
2)	Clutch: Adjustable torque-limiter type. 
3)	Limit System: EZ limit system, magnetic type providing absolute positioning with push to set capability. Limit System shall remain synchronized with the door during manual operation and supply power interruptions.
3.	Control System: Microprocessor based with relay motor controls on a single board. System incorporates a 16 character Liquid Crystal Display (LCD) to display the system status. System shall include the following:
a.	Capable of monitoring and reporting on a variety of operating conditions, including: Current operating status, Current command status, Motor movement status, Current error status (if applicable), Hoist Interlock status (if applicable), External Interlock status, and 24VDC status. 
b.	A delay-on-reverse operating protocol. 
c.	Maximum run timers in both directions of travel that limit motor run time in the event a clutch slips or some other problem occurs. 
d.	Provisions for the connection of a 2-wire monitored photo-eye or a 2-wire monitored edge sensor, as well as non-monitored 2-wire sensing edges, photo-eyes or other entrapment protection devices.
e.	Control action will be constant contact close until a monitored entrapment device is installed, allowing for selection of momentary contact.
f.	Provisions for connection of single and/or 3-button control stations. 
g.	Provisions for connection of an external 3-wire radio controls and related control devices. 
h.	On board open, close and stop control keys for local operation. 
i.	Trolley operators with an inherent secondary reversal system. 
j.	Intellicode 315Mhz radio receiver capable of storing 50 single button and/or 50 Open-Close-Stop transmitters with the ability to add and/or delete transmitters individually, identify and store activating transmitter IDs. 
4.	Mounting:
a.	Sectional Steel Doors:
1)	Jackshaft/Hoist that is side or center mounted with:
a)	Chain/sprocket coupling to door.
2)	Trolley:
a)	Single trolley.
b)	Side-mount trolley with hoist.
c)	Dual trolley.
5.	Release:
a.	Release shall be a pull and hold type mechanism with single cable operation and an integrated interlock switch on hoist units.
b.	Release shall consist of a manual disconnect door arm on trolley units.
6.	Hoist: Chain hoist consists of chain pocket wheel, chain guard and smooth hand chain on hoist units.
7.	Entrapment Protection: 
a.	Control system shall have provisions to connect monitored entrapment protection devices such as monitored electric sensing edge, or monitored photo-eye and to provide constant contact close control operation in lieu of such devices.
8.	Secondary Reversal:
a.	Trolley Models Only: When the clutch is detected slipping in the close direction the operator will reverse the door to the open limit. For door/operator protection only and not intended for entrapment protection.
b.	Control system designed to accept an optional non-monitored external reversing device.
9.	Control accessories:
a.	Operator Controls: 
1)	Push-button operated control stations with open, close, and stop buttons.
2)	Key operation with open, close, and stop controls.
3)	Push-button and key operated control stations with open, close, and stop buttons.
4)	Controls for interior location.
5)	Controls for exterior location.
6)	Controls for both interior and exterior location. 
7)	Controls surface mounted.
8)	Controls flush mounted.
b.	Special Operation: 
1)	Vehicle detector operation.
2)	Radio control operation.
3)	GENIE monitored photo-eyes.
4)	Commercial photo-eyes.
5)	Timer Close Module for unattended timed door closing. Auxiliary control inputs, safety inputs, timer hold input and automatic door closing feature with selectable time delay. Safety inputs can be configured using on board keypad.
6)	Commercial light package.
7)	Auxiliary Output Module for up, down, and mid-stop limit status via several auxiliary sets of dry contacts that are microprocessor controlled. ADA compliant outputs that activate when door is moving up, down, or both directions and can be configured using the on board keypad.
B.	Hazardous Location NEMA 7/9 Heavy Duty Sectional Door Operator: Model GCL-GH True Gear Head Type Door Operator:
1.	Application:
a.	Standard Lift Sectional Door.
b.	Lift Clearance Sectional Door.
c.	Full Vertical Sectional Door.
2.	Electric Motor: UL listed.
a.	Rating:
1)	1/2 horsepower single phase with automatic thermal reset overload with ability to configure for voltages of 115/208/230V.
2)	1 horsepower three phase with automatic thermal reset overload with ability to configure for voltages of 208/230/460V.
3)	3 horsepower three phase with automatic thermal reset overload with ability to configure for voltages of 208/230/460V.
b.	Motor frame comply with:
1)	NEMA 56C for 1/2 hp single phase.
2)	NEMA 56C 1 hp three phase.
3)	NEMA 182C for 3 hp three phase.
c.	Construction:
1)	Hazardous location NEMA 7 construction.
2)	Hazardous location NEMA 9 construction.
d.	The operator shall be suited for:
1)	NEMA Type 7 construction for indoor use in hazardous (classified) locations classified as Class I, Division I, Group D, T2C as defined in NFPA 70. 
2)	NEMA Type 9 construction for indoor use in hazardous (classified) locations classified as Class II, Division I, Groups F and G, T2C as defined in NFPA 70.
e.	Reduction: Primary reduction is worm gear in oil bath.
f.	Duty cycle: Accommodate heavy usage, up to 60 cycles per hour under a large constant load.
1)	Brake: Motor and electrical system will provide dynamic braking.
2)	Clutch: Optional adjustable torque-limiter type. Not available on 3 horsepower models.
3)	Limit System: Limit system shall be rotary type with vernier adjustment, synchronized with door during release operation. Limit system shall incorporate intrinsically safe wiring.
3.	Control System: Microprocessor based with on-board configuration and diagnostic LEDs. This system shall be capable of monitoring and reporting on a variety of operating conditions, including: Current operating status, Current maximum run time status, Motor running status, Current error status (if applicable), Timer to close status (if applicable), Open limit status, Close limit status, and Cycle count. System shall include the following:
a.	A delay-on-reverse operating protocol.
b.	The system shall include maximum run timers in both directions of travel that limit motor run time in the event a clutch slips or some other problem occurs.
c.	It shall include provisions for the connection of a 2-wire T2 monitored edge sensor for entrapment protection. 
d.	Control action will be constant contact close until a monitored entrapment device is installed, allowing for selection of momentary contact. 
e.	The system shall include provisions for connection of single or 3-button control stations. 
f.	The control system shall include on board open, close and stop control keys for local operation.
g.	The system shall include provisions for automatic door closure upon reaching the open limit and completion of adjustable time delay.
4.	Mounting:
a.	Sectional Steel Doors:
1)	Jackshaft/Hoist that is side or center mounted with
a)	Chain/sprocket coupling to door.
b.	Trolley.
1)	Single trolley.
2)	Side-mount trolley with hoist.
3)	Dual trolley.
5.	Release:
a.	Release shall be a pull and hold type mechanism with single cable operation and an integrated interlock switch on hoist units.
b.	Release shall consist of a manual disconnect door arm on trolley units.
c.	Hoist: Chain hoist consists of chain pocket wheel, chain guard and smooth hand chain on hoist units.
6.	Entrapment Protection:
a.	UL 325 momentary contact control system shall have provisions to connect intrinsically safe monitored entrapment protection electric sensing edge, and to provide constant contact close control operation in lieu of such device.
7.	Control accessories:
a.	Operator Controls:
1)	Push-button operated control stations with open, close, and stop buttons.
2)	Key operation with open, close, and stop controls.
3)	Push-button and key operated control stations with open, close, and stop buttons.
4)	Controls for interior location.
5)	Controls for exterior location.
6)	Controls for both interior and exterior location.
7)	Controls surface mounted.
8)	Controls flush mounted.
C.	Commercial Sectional Door Operator: Model GCL-T/GCL-H/GCL-J Commercial Door Operator:
1.	Application:
a.	Standard Lift Sectional Door.
b.	Lift Clearance Sectional Door.
c.	Full Vertical Sectional Door.
2.	Electric Motor: UL listed.
a.	Rating:
1)	1/2 horsepower single phase or three.
2)	3/4 single phase or three phase.
3)	1 horsepower single phase or three phase.
b.	Motor frame comply with: 
1)	NEMA 48 for 1/2 hp single phase.
2)	NEMA 56 for 1/2 hp three phase.
3)	NEMA 56 3/4 and 1 hp all phases.
c.	Construction: 
1)	Open drip-proof construction.
2)	Totally Enclosed Non Ventilated - TENV construction.
3)	Totally Enclosed Fan Cooled - TEFC construction.
4)	Washdown - NEMA 4 / NEMA 4X construction
d.	Reduction: Primary reduction is TensiBelt, an auto tension poly-V flex belt that does not require adjustment. Secondary reduction is by chain and sprocket.
e.	Duty cycle: Accommodate standard usage, up to 60 cycles per hour during peak usage periods.
1)	Brake: DC Disc type with selectable Progressive Braking for smooth stopping.
2)	Clutch: Adjustable friction disc type. 
3)	Limit System: EZ Limit system, magnetic type providing absolute positioning with push to set capability. Limit System shall remain synchronized with the door during manual operation and supply power interruptions.
3.	Control System: Microprocessor based with relay motor controls on a single board. System incorporates a 16 character Liquid Crystal Display (LCD) to display the system status. System shall include the following:
a.	Capable of monitoring and reporting on a variety of operating conditions, including: Current operating status, Current command status, Motor movement status, Current error status (if applicable), Hoist Interlock status (if applicable), External Interlock status, and 24VDC status. 
b.	A delay-on-reverse operating protocol. 
c.	Maximum run timers in both directions of travel that limit motor run time in the event a clutch slips or some other problem occurs. 
d.	Provisions for the connection of a 2-wire monitored photo-eye or a 2-wire monitored edge sensor, as well as non-monitored 2-wire sensing edges, photo-eyes or other entrapment protection devices.
e.	Control action will be constant contact close until a monitored entrapment device is installed, allowing for selection of momentary contact.
f.	Provisions for connection of single and/or 3-button control stations. 
g.	Provisions for connection of an external 3-wire radio controls and related control devices. 
h.	On board open, close and stop control keys for local operation. 
i.	Intellicode 315Mhz radio receiver capable of storing 50 single button and/or 50 Open-Close-Stop transmitters with the ability to add and/or delete transmitters individually identify and store activating transmitter IDs. 
4.	Mounting:
a.	Sectional Steel Doors: 
1)	Jackshaft/Hoist that is side or center mounted with
a)	Chain/sprocket coupling to door.
2)	Trolley.
a)	Single trolley.
b)	Side-mount trolley with hoist.
c)	Dual trolley.
5.	Release:
a.	Release shall be a pull and hold type mechanism with single cable operation and an integrated interlock switch on hoist units.
b.	Release shall consist of a manual disconnect door arm on trolley units.
6.	Hoist: Chain hoist consists of chain pocket wheel, chain guard and smooth hand chain on hoist units.
7.	Entrapment Protection: 
a.	Control system shall have provisions to connect monitored entrapment protection devices such as monitored electric sensing edge, or monitored photo-eye and to provide constant contact close control operation in lieu of such devices.
8.	Secondary Reversal:
a.	When the clutch is detected slipping in the close direction the operator will reverse the door to the open limit. For door/operator protection only not intended for entrapment
b.	Control system designed to accept an optional non-monitored external reversing device.
9.	Control accessories:
a.	Operator Controls: 
1)	Push-button operated control stations with open, close, and stop buttons.
2)	Key operation with open, close, and stop controls.
3)	Push-button and key operated control stations with open, close, and stop buttons.
4)	Controls for interior location.
5)	Controls for exterior location.
6)	Controls for both interior and exterior location. 
7)	Controls surface mounted.
8)	Controls flush mounted.
b.	Special Operation: 
1)	Vehicle detector operation.
2)	Radio control operation.
3)	GENIE monitored photo-eyes.
4)	Commercial photo-eyes.
5)	Timer Close Module for unattended timed door closing. Auxiliary control inputs, safety inputs, timer hold input and automatic door closing feature with selectable time delay. Safety inputs can be configured using on board keypad.
6)	Commercial light package.
7)	Auxiliary Output Module for up, down, and mid-stop limit status via several auxiliary sets of dry contacts that are microprocessor controlled. ADA compliant outputs that activate when door is moving up, down, or both directions and can be configured using the on board keypad.
D.	Commercial Sectional Door Operator: Model GCL-MT/GCL-MH/GCL-MJ Door Medium Duty Operator:
1.	Application:
a.	Standard Lift Sectional Door.
b.	Lift Clearance Sectional Door.
c.	Full Vertical Sectional Door.
2.	Electric Motor: UL listed.
a.	Rating:
1)	1/2 horsepower single phase with automatic thermal reset overload.
b.	Motor frame comply with: 
1)	NEMA 42 for 1/2 hp single phase.
c.	Construction: 
1)	Open drip-proof construction.
d.	Reduction: Primary reduction is TensiBelt poly-V flex auto tension belt. Secondary reduction is by chain and sprocket.
e.	Duty cycle: Accommodate medium usage, up to 15 cycles per hour.
1)	Brake: Solenoid actuated band type. Optional on trolley models, standard on jackshaft and hoist models.
2)	Limit System: Adjustable linear type synchronized with the door during release operation. Limit activation by opto sensors
3.	Control System: Microprocessor based with relay motor controls on a single board. System incorporates a Liquid Crystal Display (LCD) to display the system status. System shall include the following:
a.	A delay-on-reverse operating protocol. 
b.	Maximum run timers in both directions of travel that limit motor run time in the event a clutch slips or some other problem occurs. 
c.	Provisions for the connection of a 2-wire monitored photo-eye or a 2-wire monitored edge sensor, as well as non-monitored 2-wire sensing edges, photo-eyes or other entrapment protection devices. 
d.	Control action will be constant contact close until a monitored entrapment device is installed, allowing for selection of momentary contact.
e.	Provisions for connection of single and/or 3-button control stations. 
f.	Provisions for connection of an external 3-wire radio controls and related control devices. 
g.	On board open, close and stop control keys for local operation. 
h.	Trolley operators with an inherent secondary reversal system.
4.	Mounting:
a.	Sectional Steel Doors: 
1)	Jackshaft/Hoist that is side mounted with
a)	Chain/sprocket coupling to door.
2)	Trolley.
a)	Single trolley.
5.	Release:
a.	Release shall be a pull and hold type mechanism with single cable operation and an integrated interlock switch on hoist units.
b.	Release shall consist of a manual disconnect door arm on trolley units.
6.	Hoist: Chain hoist with chain pocket wheel, chain guard and smooth hand chain.
7.	Entrapment Protection: 
a.	Control system shall have provisions to connect monitored entrapment protection devices such as monitored electric sensing edge or monitored photo-eye and to provide constant contact close control operation in lieu of such devices.
8.	Secondary Reversal:
a.	Trolley models only. When the clutch is detected slipping in the close direction the operator will reverse the door to the open limit. For door/operator protection only not intended for entrapment
b.	Control system designed to accept an optional non-monitored external reversing device.
9.	Control accessories:
a.	Operator Controls: 
1)	Push-button operated control stations with open, close, and stop buttons.
2)	Key operation with open, close, and stop controls.
3)	Push-button and key operated control stations with open, close, and stop buttons.
4)	Controls for interior location.
5)	Controls for exterior location.
6)	Controls for both interior and exterior location. 
7)	Controls surface mounted.
8)	Controls flush mounted.
b.	Special Operation: 
1)	Radio control operation.
2)	GENIE monitored photo-eyes.
3)	Commercial photo-eyes.
4)	Timer Close Module for unattended timed door closing. Auxiliary control inputs, safety inputs, timer hold input and automatic door closing feature with selectable time delay. Safety inputs can be configured using on board keypad.
5)	Auxiliary Output Module for up, down, and mid-stop limit status via several auxiliary sets of dry contacts that are microprocessor controlled. ADA compliant outputs that activate when door is moving up, down, or both directions and can be configured using the on board keypad.
2.5	COILING COUNTER DOORS
A.	Counter Door Operator: Model GCX Counter Door Operator:
1.	Electric Motor: Intermittent-duty, with instant reverse and automatic reset thermal overload. UL listed.
a.	Rating:
1)	1/2 horsepower single phase.
2)	115 V.
b.	Motor frame comply with: 
1)	NEMA 42 for 1/2 hp single phase.
c.	Construction: 
1)	Open drip-proof construction.
d.	Reduction: Helical gear primary reduction and hardened bevel gear secondary reduction.
e.	Duty cycle: Accommodate light duty usage, up to 4 cycles per hour.
1)	Limit System: EZ limit system, magnetic type providing absolute positioning with push to set capability. Limit System shall remain synchronized with the door during manual operation and supply power interruptions.
2.	Control System: Microprocessor based with relay motor controls on a single board. System incorporates a 16 character Liquid Crystal Display (LCD) to display the system status. System shall include the following:
a.	A delay-on-reverse operating protocol. 
b.	Maximum run timers in both directions of travel that limit motor run time in the event a problem occurs. 
c.	Provisions for the connection of a 2-wire monitored photo-eye or a 2-wire monitored edge sensor, as well as non-monitored 2-wire sensing edges, photo-eyes or other entrapment protection devices. 
d.	Control action will be constant contact close until a monitored entrapment device is installed, allowing for selection of momentary contact.
e.	Provisions for connection of single and/or 3-button control stations. 
f.	On board open, close and stop control keys for local operation.
3.	Mounting:
a.	Counter doors:
1)	Front of hood and chain/sprocket coupling to door.
4.	Release:
a.	Release shall be a pull and hold type mechanism with single cable operation and an integrated interlock switch on hoist units.
5.	Hand Crank: Hand crank for manual door control.
6.	Entrapment Protection: 
a.	Control system shall have provisions to connect monitored entrapment protection devices such as monitored electric sensing edge, or monitored photo-eye and to provide constant contact close control operation in lieu of such devices.
7.	Control accessories:
a.	Operator Controls: 
1)	Push-button operated control stations with open, close, and stop buttons.
2)	Key operation with open, close, and stop controls.
3)	Push-button and key operated control stations with open, close, and stop buttons.
4)	Controls for interior location.
5)	Controls for exterior location.
6)	Controls for both interior and exterior location. 
7)	Controls surface mounted.
8)	Controls flush mounted.
b.	Special Operation: 
1)	Radio control operation.
2)	GENIE monitored photo-eyes.
3)	Commercial photo-eyes.
4)	Fire Door Time Delay Release. 
5)	Timer Close Module for unattended timed door closing. Auxiliary control inputs, safety inputs, timer hold input and automatic door closing feature with selectable time delay. Safety inputs can be configured using on board keypad.
6)	Auxiliary Output Module for up, down, and mid-stop limit status via several auxiliary sets of dry contacts that are microprocessor controlled. ADA compliant outputs that activate when door is moving up, down, or both directions and can be configured using the on board keypad.
8.	Automatic Closure:
a.	Fire Door Release Device time-relay release mechanism with motor close option provides an added measure of safety to control the doors' closure.
1)	Voltage: 120 VAC
2)	Voltage output 24 VDC
3)	Release time delay: Factory set at 10 seconds can be field adjusted by dipswitch settings to 20, 30 and 60 seconds.
4)	Must use normally open proximity switch to detect door is closed.
5)	Can support 2 or 4 wire smoke detector system (maximum of 4 Class B Style A detectors. Release devices are normally open contacts. Provided with 4 wire detectors when detectors are specified with an end of line relay.
6)	Unit has two 12 VDC batteries 24 VDC output.
7)	Power Loss Time delay: 48 hours.
8)	Unit can power an optional ADA horn / strobe 24 VDC.
9)	Load Rating: Support and Release 40 lbs. maximum.
10)	Auxiliary output module must be installed to accept wiring from Fire Door release device.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Verify door sizes, configuration, tolerances and conditions are acceptable.
B.	Examine conditions of substrates, supports, and other conditions under which this work is to be performed.
C.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions.
B.	Use anchorage devices to securely fasten assembly without distortion or stress.
C.	Fit and align assembly including hardware; level and plumb, to provide smooth operation.
D.	Coordinate installation of electrical service with Section 26 05 00 - Common Work Results for Electrical. Complete wiring from disconnect to unit components.
3.4	ADJUSTING
A.	Test for proper operation and adjust as necessary to provide proper operation without binding or distortion.
B.	Adjust hardware and operating assemblies for smooth and noiseless operation.
3.5	CLEANING
A.	Clean components using non-abrasive materials and methods recommended by manufacturer.
B.	Touch-up, repair or replace damaged products before Substantial Completion.
3.6	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.
3.7	SCHEDULES
A.	:
B.	:

END OF SECTION