SECTION 10 51 00

LOCKERS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2015 -  2024 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Metal grid athletic lockers.
1.2	RELATED SECTIONS
A.	Section 06 10 00 - Rough Carpentry.
B.	Section 09 22 16 - Non-Structural Metal Framing.
C.	Division 16 - Electrical for power wiring.
1.3	REFERENCES
A.	American National Standards Institute (ANSI):
1.	ANSI A208.1 - Particleboard.
B.	American Society of Civil Engineers (ASCE):
1.	ASCE 7 - Minimum Design Loads for Buildings and Other Structures.
C.	ASTM International (ASTM):
1.	ASTM A501 - Standard Specification for Hot-Formed Welded and Seamless Carbon Steel Structural Tubing. 
2.	ASTM C510 - Standard Specification for General Requirements for Steel Rods and Coarse Round Wire, Carbon Steel.
D.	GREENGUARD Environmental Institute (GEI): 
1.	GREENGUARD certified low emitting products.
E.	Laminating Materials Association: 
1.	LMA EDG-1: Voluntary Product Standard and Typical Physical Properties of Edgebanding Materials.
F.	National Fire Protection Association (NFPA):
1.	NFPA 70 - National Electrical Code (NEC).
G.	National Electrical Manufacturers Association (NEMA):
1.	NEMA LD 3 - High Pressure Decorative Laminates.
H.	Underwriters Laboratory (UL): 
1.	UL 514A - Metallic Outlet Boxes.
I.	U.S. Architectural & Transportation Barriers Compliance Board:
1.	Americans with Disabilities Act (ADA) and Architectural Barriers Act (ABA) Accessibility Guidelines for Buildings and Facilities.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Rated capacities, construction details, material descriptions, dimensions of individual components, profiles, and finishes.
3.	Delivery, storage, handling, and installation instructions and recommendations.
4.	Maintenance instructions and recommendations. 
C.	Shop Drawings:
1.	Show fabrication and installation details. Distinguish between factory and field work. 
2.	Include plans, elevations, sections, details, attachments and work by others.
3.	Show system layouts, room locations, clearances, spacing, and relationship to adjacent construction. 
4.	Show trim and accessories. 
5.	Indicate seismic bracing and fastening requirements.
D.	Product Schedule: 
1.	Use designations indicated on the Drawings.
2.	Include room locations, dimensions, accessories, finishes, and project specific notes. 
E.	Verification Samples: 
1.	Exposed Finishes: Not less than 8 by 10 inches (200 by 250 mm), for each type, color, pattern, surface and material selected.
2.	Exposed Hardware and Accessories: One full size unit for each type and finish.
F.	Closeout Submittals:
1.	Operation and Maintenance Data: For adjusting, repairing and replacing components and accessories.
2.	Warranty: Submit manufacturer's sample warranty.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Minimum 5 years experience in manufacture of similar products in use in similar environments, including project size, and complexity, and with the production capacity to meet the construction and installation schedule.
B.	Installer Qualifications: Manufacturer's authorized representative, trained and approved for installation of units required for this Project.
C.	Source Limitations: Obtain components and accessories through one source from a single approved manufacturer.
D.	Electrical Components: Listed and labeled per NFPA 70, Article 100 by a testing agency acceptable to authorities having jurisdiction.
E.	Regulatory Requirements: Where components are indicated to comply with accessibility requirements, comply with the U.S. Architectural & Transportation Barriers Compliance Board's "Americans with Disabilities Act (ADA) and Architectural Barriers Act (ABA) Accessibility Guidelines for Buildings and Facilities".
F.	Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and installation workmanship.
1.	Finish areas designated by Architect including shims, sealants, and accessories.
2.	Provide full size units, if accepted, units may remain as part of the completed work. 
3.	Do not proceed with remaining work until workmanship is approved by Architect.
4.	Refinish mock-up area as required to produce acceptable work.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Deliver materials in manufacturer's original unopened containers with manufacturer's labels attached. 
B.	Do not deliver lockers until spaces to receive them are clean, dry, and ready for their installation. Ship to jobsite only after roughing-in, painting and other finishing work has been completed, installation areas are ready to accept work.
C.	Handle and install materials to avoid damage.
1.7	PROJECT CONDITIONS
A.	Environmental Limitations: Do not deliver or install lockers until spaces are enclosed and weather tight, wet work in spaces is complete and dry, HVAC system is operating and maintaining ambient temperature at occupancy levels during the remainder of the construction period.
B.	Field Measurements: Verify field measurements as indicated on Shop Drawings. Where measurements are not possible, provide control dimensions and templates. 
1.	Coordinate installation and location of blocking and supports as requested. 
2.	Verify openings, clearances, storage requirements and other dimensions relevant to the installation and final application.
C.	Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Wenger Corporation, including all Wenger, J.R. Clancy and
 GearBoss product brands. Wenger Corporation, which is located at: 555 Park Dr.;
 Owatonna, MN 55060; Toll Free Tel: 800-4WENGER (493-6437); Tel: (507) 455-4100; Fax:
 (507) 455-4258; Email: info@wengercorp.com; Wenger Corporation - Syracuse, which is
 located at 7041 Interstate Island Road, Syracuse, NY 13209; Toll Free Tel: 800-836-1885;
 Tel: (315) 451-3440; Email: info@wengercorp.com; Web: https://www.wengercorp.com
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements. 
1.	Warranty terms and conditions: Wenger offers the most warranty protection available in the industry. We do not make exceptions for the normal levels of wear and tear common to learning environments. Our only such stated exception is failure resulting from vandalism or uncontrolled moisture or humid. Delete if not required. Approval of Comparable Products: Submit the following in accordance with project substitution requirements, within time period allowed for substitution review:
a.	Product data, including certified independent test data indicating compliance with requirements including: modularity of individual units; ventilation, strength of door, hinge and latch construction; replaceable construction for compartment and foot locker doors; impact and abrasion resistance of surfaces and edge banding. 
b.	Samples of each type of product specified.
c.	Project References: minimum of 5 installations not less than 5 years old, with owner contact information, available for evaluation by Architect.
d.	Sample warranty including terms and conditions.
2.	Submit substitution request not less than 15 days prior to bid date. Substitutions following award of contract are not allowed except as stipulated in Division 01 General Requirements.
3.	Manufacturer must meet each separate requirements of Submittals Article.
2.2	METAL GRID ATHLETIC LOCKERS
A.	Metal Lockers:
1.	ADA compliant as indicated on the Drawings.
2.	GREENGUARD certified low emitting products. 
3.	Bolt-through construction.
4.	Modular construction, all parts repairable and replaceable. 
B.	AirPro Metal Grid Athletic Lockers by Wenger Corporation: Wall-mounted locker with lockable foot locker, integral bench seat, and apparel hooks.
1.	Type: Single tier.
2.	Type: Double tier.
3.	Configuration: Wall of lockers.
4.	Configuration: Island of lockers.
5.	Locker Size: Custom style as indicated on the Drawings.
6.	Locker Size: 15 inch (381 mm) wide by 30.5 inch (775 mm) deep by 70 inch (1778 mm) high, mounted with top bracket at 78 inches (1980 mm) above finished floor.
7.	Locker Size: 18 inch (457 mm) wide by 30.5 inch (775 mm) deep by 70 inch (1778 mm) high, mounted with top bracket at 78 inches (1980 mm) above finished floor.
8.	Locker Size: 21 inch (533 mm) wide by 30.5 inch (775 mm) deep by 70 inch (1778 mm) high, mounted with top bracket at 78 inches (1980 mm) above finished floor.
9.	Locker Size: 24 inch (610 mm) wide by 30.5 inch (775 mm) deep by 70 inch (1778 mm) high, mounted with top bracket at 78 inches (1980 mm) above finished floor.
10.	Locker Size: 27 inch (685 mm) wide by 30.5 inch (775 mm) deep by 70 inch (1778 mm) high, mounted with top bracket at 78 inches (1980 mm) above finished floor.
11.	Locker Size: 30 inch (762 mm) wide by 30.5 inch (775 mm) deep by 70 inch (1778 mm) high, mounted with top bracket at 78 inches (1980 mm) above finished floor.
12.	Locker Size: Width as indicated wide by 30.5 inch (775 mm) deep by 70 inch (1778 mm) high, mounted with top bracket at 78 inches (1980 mm) above finished floor.
13.	Seismic Performance: Comply with ASCE 7 Section 9, "Earthquake Loads" based upon seismic design criteria indicated on the Structural Documents.
14.	Steel Grid Infill: 2 inch (51 mm) square pattern, welded to steel tube frame.
15.	Integral Seat and Foot Locker: Laminate-clad composite wood panel seat and foot locker lid, 3/4 inch (19 mm) thick, with lockable seat security compartment, replaceable split pin hinge, and locking hasp for padlock by Owner.
16.	Shelf and Seat: 3/4 inch (19 mm) thick, formaldehyde free industrial grade composite wood with polyester, antimicrobial laminate finish.
17.	Apparel Hooks: One double and two single hooks, bolted to locker shelf and sides.
C.	Locker Materials:
1.	Materials to meet Sustainable Design Requirements: 
a.	No Added Urea Formaldehyde Products: Provide products made with composite products and adhesives with no urea formaldehyde added.
2.	Steel Tube: ASTM A501, hot-formed steel tubing.
3.	Steel Wire: ASTM C510, cold drawn steel wire.
4.	Particleboard: To ANSI A208.1, minimum 43 lb/cu. ft. (689 kg/cu. m) density..
a.	Provide fire retardant treated type. 
5.	Plywood: APA standards PS1-98 section 5.7.4 or 5.7.1 or ANSI /HPVA HP-1-2004 Panel provide with HDF skins to prevent grain telegraphing.
6.	Laminate Finish: Composite, of thickness indicated, finished with thermally-fused anti-microbial polyester surfacing on both sides, meeting performance properties of NEMA LD3 for VGS grade, with heat bonded, radiused, 3 mm thick extruded PVC edge banding.
a.	Surface Abrasion Resistance: Taber Wheel, 400 cycles, for solid colors.
7.	PVC Edge Banding: LMA EDG-1, radiused PVC extrusions, 3 mm thick, heat-bonded.
8.	Anchors and Fasteners: 
a.	Factory Provided: Material, type, and size recommended by manufacturer for secure anchorage to substrate.
b.	Field Installed: Manufacturer-recommended fasteners furnished by Contractor as required for locker substrate and project requirements.
D.	Locker Fabrication:
1.	Fabricate components square, and rigid. Make exposed metal safe to touch and free of sharp ends or burrs.
2.	Form frames, panels, doors, and accessories from one-piece, or one rigid assembly, unless specifically shown on Shop Drawings.
3.	Factory preassemble metal components by welding all joints, and connections; with no bolts, nuts, screws, or rivets used in assembly, except as required for knock down shipping and attachment to mounting surfaces.
E.	Metal Locker Accessories:
1.	Door Type: Steel grid infill, 1-inch (25 mm) square pattern 0.16-inch (4.1-mm) diameter wire in 1-1/4-inch (31.7 mm) outside diameter,16-gauge tube steel frame, with replaceable split pin hinge and locking hasp for padlock by Owner.
2.	Door Type: Laminate wood panel infill, in welded steel tube frame with replaceable split pin hinge and locking hasp for padlock by Owner.
3.	Door Type: Door Ready, open body can accept door after initial install.
4.	Identification Plates, Name and Brackets: 20-gauge steel, powder-coated paint. 12 inches (314 mm) wide by 2.125 inches (54 mm) high.
5.	Shoulder Pad and Helmet Topper: 3/4-inch (19 mm) diameter welded steel tubing frame with steel mounting plate; powder-coated, color: black 18-3/4 inch (476 mm) high. 
6.	Five-Sided Security Box Mounted in Locker: 18 gauge steel, powder-coated paint. Size: 6 inch (152 mm) wide by 12 inch (305 mm) long by 11-1/4 inch (286 mm) high.
7.	Electrical Kit: Steel electrical enclosure and face plate for single-gang Decora receptacle finished in black, UL 514A approved available in all standard locker widths.
a.	Kit includes joining connectors and brackets for ease of assembly. 
b.	Wiring and installation of electrical kit shall be performed by licensed electrician on site per local jurisdiction codes under Division 26.
c.	Configuration Options:
1)	Electrical housing 15 amp black single-gang Decora receptacle outlet with USB-A and USB-C ports. 
2)	Electrical housing single-gang box for use only with customer sourced receptacles. 
3)	Electrical housing single-gang box with 15 amp black Decora receptacle outlet with USB-A and USB-C ports.
8.	Lacrosse and Hockey Stick Security: Manufacturer's standard configuration.
9.	Wood Back Panel: Required.
10.	Custom Features: As indicated on the Drawings.
F.	Metal Locker Finishes: Color selected by designer from manufacturer's standard range of colors and patterns. 
1.	Locker Top and Bottom Grid Color: Black (standard).
2.	Locker Top and Bottom Grid Color: As selected from manufacturer's full range.
3.	Locker Top and Bottom Grid Color: As indicated on the Drawings.
4.	Laminate Seat/Shelf Color: Graphite (standard)
5.	Laminate Seat/Shelf Color: As selected from manufacturer's full range.
6.	Laminate Seat/Shelf Color: As indicated on the Drawings.
7.	Wood Door Panel and Color: As selected from manufacturer's full range.
8.	Wood Door Panel and Color: As indicated on the Drawings.
9.	Wood Back Panel and Color: As selected from manufacturer's full range.
10.	Wood Back Panel and Color: As indicated on the Drawings.
G.	Warranty:
1.	Special Warranty: Submit manufacturer's written 10-year limited warranty to repair or replace components that fail in materials or craftsmanship during the warranty period. Failures include the following.
a.	Fracturing or breaking components including panels, shelves, or hardware resulting from normal wear and tear and use other than vandalism.
b.	Collapse or failure of metal grid locker components not resulting from overloading or vandalism.
c.	Delamination or other failures of bonding or assembly.
d.	Warping not resulting from leaks, flooding, or other uncontrolled moisture or humidity.
e.	Faulty operation of hardware.
2.	This Warranty does not extend to mechanical or electrical component parts made by others such as fans, lights, digital locks and similar items. Component parts of this nature are covered under their independent manufactures' warranties. This Warranty does not extend to items that are consumable in nature such as bulbs, batteries and similar items.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared. 
B.	Examine installation areas and mounting surfaces with Installer present, for compliance with manufacturer's installation tolerances including required clearances, floor level, location of blocking and anchoring reinforcements, and other existing conditions that may affect installation or performance. 
C.	Confirm location of electrical power.
D.	Prepare written report, endorsed by Installer, listing conditions detrimental to performance of the Work. If preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
E.	Proceed with installation only after correction of unsatisfactory conditions.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install components plumb, level, and true; using integral levelers and anchors in accordance with manufacturer's recommendations, shop drawings and other approved submittals.
B.	Install seismic fastening in accordance with approved shop drawings.
C.	Fasten components to adjacent construction through back, near top and bottom. Fasten at indicated height using fasteners recommended by manufacturer. Comply with mounting height requirements for accessible components. 
D.	Through-bolt adjacent units using connector bolts provided by manufacturer.
E.	Install hardware uniformly and precisely without binding. 
1.	Adjust and align hardware so moving parts operate freely and contact points meet accurately. 
2.	Allow for final adjustment after installation to ensure hardware operates smoothly without warping or binding and closes with uniform reveals.
3.4	CLEANING AND PROTECTION
A.	Repair or replace defective work as directed by Architect upon inspection.
B.	Clean surfaces. Touch up marred finishes, or replace damaged components that cannot be restored to factory-finished appearance. Use only materials and procedures recommended or furnished by manufacturer.
C.	Turn over operation and maintenance instructions to Owner. Instruct the Owner's personnel upon request. 
D.	Protect installed products from damage, abuse, dust, dirt, stain, or paint until completion of project. Do not permit use during construction.

END OF SECTION