SECTION 12 35 30

KITCHEN CASEWORK

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2021 -  2021 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Kitchen Casework (Endeavor) (Builder's Mark).
1.2	RELATED SECTIONS
A.	Section 06 10 00 - Rough Carpentry.
B.	Section 06 20 00 - Finish Carpentry.
1.3	REFERENCES
A.	American National Standards Institute 
1.	ANSI/BHMA A156.9 - American National Standard for Cabinet Hardware; Builders Hardware Manufacturers Association.
2.	ANSI/KCMA A161.1 - Performance and Construction Standard for Kitchen and Vanity Cabinets; Kitchen Cabinet Manufacturers Association; 2012 (ANSI/KCMA A161.1).
B.	Builders Hardware Manufacturers Association (BHMA):
C.	Kitchen Cabinet Manufacturers Association (KCMA):
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Verification Samples: Two representative units of each type, size, pattern, and color.
D.	Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as a standard for comparison with completed work. 
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.6	PRE-INSTALLATION CONFERENCE
A.	Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.8	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.9	WARRANTY
A.	Manufacturer's Warranty: Provide manufacturer's material and workmanship warranty.
1.	Limited Warranty Duration: 1 year.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Supplier: Wolf Home Products, which is located at: 20 West Market Street; York, PA 17401; ASD Toll Free: 800-388-9653; Email: _____; Web: www.wolfhomeproducts.com.
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	KITCHEN CASEWORK
A.	Basis of Design: Endeavor Kitchen Cabinets as manufactured by Wolf Home Products.
1.	Cabinet Construction: 
a.	Industrial Grade Furniture Board: 5/8 inch (16 mm). Glued and doweled construction.
2.	Exterior: Color matched to door and drawer fronts.
3.	Shelves: 
a.	Furniture Board: 3/4 inch (19 mm). In white laminated melamine and edge banded with white thermoplastic edge banding
4.	Front Edge:
a.	Thermoplastic edge banding color matched to door/drawer front.
5.	Standard Drawers: 
a.	Formed metal sides. 
b.	Back and Bottom: 5/8 inch (16 mm) melamine.
c.	Undermount Drawer Glides: Soft-close, full-extension 
6.	Optional Drawers:
a.	Melamine laminate drawer box: 1/2 inch (13 mm)
b.	Roller Bearing Glides: Side mount, soft-close, full-extension.
7.	Bottom Edge: Sealed from moisture with thermoplastic edge banding.
8.	Doors:
a.	5-Piece shaker style.
b.	Hinges: Six-way Soft-close
c.	Finish: SmartShield Technology.
9.	Color: Grey.
10.	Color: White.
11.	Color: To be determined by the architect.
12.	Color: As detailed on the Drawings.
13.	Finish: Smart Shield.
B.	Basis of Design: Builder's Mark Cabinets as manufactured by Wolf Home Products.
1.	Wall Cabinet Construction: 
a.	Top: 1/2 inch (13 mm) industrial-grade furniture-board.
b.	Drawers: 1/2 inch (13 mm) industrial-grade furniture board.
1)	Drawer Guides: Side-mounted. Fully captured drawer bottoms.
c.	Adjustable Shelves: 1/2 inch (13 mm) industrial-grade furniture-board.
d.	Sides: Low-pressure melamine.
e.	Hanging Rail: 1/2 inch (13 mm) industrial-grade furniture-board.
f.	Bottom: 1/2 inch (13 mm) industrial-grade furniture-board.
g.	Back: 1/8 inch (3 mm) laminated MDF cabinet.
h.	Sides: 3/8 inch (9 mm) industrial-grade furniture board
i.	Face Frames: 3/4 x 1-1/2 inch (19 x 38 mm)solid wood. Dadoed and joined with wood screws or doweled.
j.	Doors: Mortise and tenon, flat panel.
1)	Six-way adjustable, fully concealed hinge.
k.	Single-Door Cabinets: Hinged left. 
1)	Flip cabinets at installation for right hinge applications.
l.	Finish: SmartShield.
2.	Base Cabinet Construction:
a.	Drawer Boxes: 1/2 inch (13 mm) industrial-grade furniture-board. Butt jointed and stapled.
1)	Drawer Glides: Side-mounted, 3/4 inch (19 mm) extension, epoxy-coated, 75 lb. nylon, lubricated roller.
b.	Half-Depth Fixed Shelves: 4-1/2 inch (114 mm) industrial-grade furniture-board.
c.	Sides: 3/8 inch (9 mm) industrial-grade furniture board for base and vanity cabinets. 
1)	Tall Cabinet Sides: 1/2 inch (13 mm) sides on tall cabinets
d.	Hanging Rails: 1/2 inch (13 mm) industrial-grade furniture-board.
e.	Backs: 1/4 inch (6 mm) furniture-board.
f.	Bottoms: 1/2 inch (13 mm) industrial-grade furniture-board.
g.	Toe Kicks: 1/2 inch (13 mm) industrial furniture-board.
h.	Face Frames: 3/4 x 1-1/2 inch (19 x 38 mm) solid wood. Dadoed and joined with wood screws or doweled.
i.	Single-Door Cabinets: Hinged left. 
1)	Base, tall and vanity cabinet doors will be reversed during installation for right hinge applications.
j.	Doors: Mortise and tenon, flat panel.
1)	Style: Pearl.
2)	Six-way adjustable, fully concealed hinge.
k.	Doors Style and Color: Sierra Espresso stain.
l.	Doors Style and Color: Sierra Harvest moon stain.
m.	Doors Style and Color: Sierra Graphite stain.
n.	Doors Style and Color: Sierra White paint
o.	Doors Style and Color: Sierra Haze paint.
p.	Doors Style and Color: Shea Pearl Smartshield.
q.	Doors Style and Color: Shea Cinder SmartShield.
r.	Doors Style and Color: Sloan Mocha stain.
s.	Finish: SmartShield.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
B.	Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
3.5	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturer's recommendations. 
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION