SECTION 08 88 53

SECURTY GLAZING ANCHORING SYSTEM

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2021 -  2021 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Security window film anchoring system. (Z SECURE)
1.2	RELATED SECTIONS
A.	Division 08 - Openings.
B.	Section 08 50 00 - Windows.
C.	Section 08 53 00 - Plastic Windows.
D.	Section 08 53 13 - Vinyl Windows.
E.	Section 08 83 13 - Mirrored Glass Glazing.
F.	Section 08 88 56 - Ballistics-Resistant Glazing.
G.	Section 08 83 13 - Mirrored Glass Glazing.
H.	Section 08 87 13 - Solar Control Film.
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Verification Samples: Two representative units of each type, size, pattern, and color.
D.	Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction. 
1.	Manufacturer will require the following information to submit Shop Drawings:
a.	Dimensions of window openings
b.	Glazing thickness.
c.	Overall depth of window opening.
d.	Substrate material.
1.4	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as a standard for comparison with completed work. 
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.5	PRE-INSTALLATION CONFERENCE
A.	Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.7	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.8	WARRANTY
A.	Manufacturer's standard limited warranty unless indicated otherwise.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Z Secure Attachment System, which is located at:<BR />650 E. Hwy. 121 Business, Suite 311<BR />Lewisville, TX 75057 <BR />Tel: 972-485-0100<BR />Email: request info (tim1@hometint.com          );Web: https://zsecurefordoors.com | https://zsecurefordoors.com/gallery 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	PRODUCT TYPES
A.	Basis of Design: Z SECURE Securement System as manufactured by Z Secure.
1.	Description: A securement system which withstands more blows than traditional Glass. A pane of glass with adhered security film is installed into a door or window frame opening. The security film faces the inside or opposite the "attack"side in most cases. Security film can be applied to both sides for added strength and protection. The inside leg (glass coupler) of the Z-frame profile adheres to the security film on the glass pane. The opposite outer leg (support coupler) of the Z-frame profile adheres to the side of the door or window frame opposite to the "attack" side.
2.	Window Perimeter Securement Z-Frame Brackets: 
a.	Securement Frame Profile: "Z" Channel 0.040 inch ( mm) thick aluminum. Cut to fill window opening perimeter.
1)	Corners: Mitered.
2)	Custom color on opposite of attack side.
3)	Window Openings: As determined by the Architect.
4)	Window Opening: As detailed on the Drawings.
5)	Window Opening (WxH): ____ x ____ inch (____ x ____ mm).
6)	Profile Overlap of Perimeter Opening (Support Coupler): 5/8 inch ( mm) minimum.
b.	Overall Inside Leg Length (Glass Coupler): ____ inch (____ mm).
c.	Z-Frame 90 Degree Offset:
1)	(Frame Support Width - Glass Pane and Security Film thickness)/2
2)	Permissible Offset Range: 1/4 to 7/8 inch (6 to 22 mm)
d.	Finish: Clear anodized.
e.	Finish and Color: ________.
f.	Finish and Color: As determined by the Architect.
g.	Finish and Color: As detailed on the Drawings.
3.	Adhering System Glazing Security Film to Z-Secure: 3MTM VHBTM Tape clear 1/2 inch (13 mm) using UV Adhesive Promoter or Primer 94.
4.	Adhering System Door or Window Support Frame to Z-Secure: 3MTM VHBTM Tape clear .5/8 inch (16 mm) using UV Adhesive Promoter or Primer 94.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
1.	Installation is to be performed by an authorized representative for Z-Secure.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
B.	Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
3.5	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturer's recommendations. 
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION