IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2023-01-18T16:03:37"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skylight_CM_AmericanSkylites:CM1414 - Single Dome - Glazing as Specified" | object type "Skylight_CM_AmericanSkylites:CM1414 - Single Dome - Glazing as Specified" | names: "Skylight_CM_AmericanSkylites:CM1414 - Single Dome - Glazing as Specified:105669" | material: materials ("None", "Sealant Tape", "None", "Frame - Aluminum - Bronze Anodized", "Santoprene Gasket Material", "Aluminum 0.060" - Finish as Specified", "Sealant", "Sealant", "Flashing - As Specified", "Wood Materials - Pine", "Wood Materials - Pine") | property sets: Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Constraints, Construction

Types
  IFCWINDOWSTYLE "Skylight_CM_AmericanSkylites:CM1414 - Single Dome - Glazing as Specified" | 1 occurrence | material: materials ("None", "Sealant Tape", "None", "Frame - Aluminum - Bronze Anodized", "Santoprene Gasket Material", "Aluminum 0.060" - Finish as Specified", "Sealant", "Sealant", "Flashing - As Specified", "Wood Materials - Pine", "Wood Materials - Pine") | property sets: Skylight_CM_AmericanSkylites:CM1414 - Single Dome - Glazing as Specified:105669, Analytical Properties, Construction, Energy Analysis, Identity Data, Materials and Finishes

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCWINDOW) | on 1 type object
    Category = "Windows" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
    Family = "Skylight_CM_AmericanSkylites" (IFCLABEL)
    Family and Type = "Skylight_CM_AmericanSkylites: CM1414 - Single Dome - Glazing as Specified" (IFCLABEL)
    Host Id = "105659" (IFCLABEL)
    Type = "CM1414 - Single Dome - Glazing as Specified" (IFCLABEL)
    Type Id = "105644" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Windows" (IFCLABEL)
    Family Name = "Skylight_CM_AmericanSkylites" (IFCTEXT)
    Manufacturer Address = "525 113th St. Arlington TX 76011" (IFCTEXT)
    Manufacturer Fax = "817-633-4616" (IFCTEXT)
    Manufacturer Phone - Toll Free = "800-772-7401" (IFCTEXT)
    Manufacturer Phone = "817-633-4666" (IFCTEXT)
    Manufacturer Website = "http://www.americanskylites.com" (IFCTEXT)
    Send Message = "http://admin.arcat.com/users.pl?action=UserEmail&company=American%20Skylites,%20Inc.&coid=30446&rep=108&fax=817-633-4616&mf=" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCWINDOW) | on 1 type object
    Manufacturer = "American Skylights, Inc" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWINDOW)
    Reference = "CM1414 - Single Dome - Glazing as Specified" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "CM1414 - Single Dome - Glazing as Specified" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCWINDOW)
    DmHt = 0.1875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    flshloc = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCWINDOW)
    Cant Size = 0.020833333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Cant Strip = TRUE (IFCBOOLEAN)
    Curb Height = 1. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 type object
    Curb Thickness = 0.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Dome Type = "Glazing_Double Dome : As Specified" (IFCLABEL)
    Flashing Clearance = 0.03125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Flashing Extension = 1.3333333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCWINDOW)
    Area = 37.62454078646013 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Height = 1.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    OD Curb Height = 1.4375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    OD Curb Width = 1.4375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 0.9375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 0.9375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 1.5138230422420493 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
    Width = 1.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Graphics | properties | on 1 object (1 IFCWINDOW)
    Usage Notes = "Skylight Height must exceed Width. Rotate Skylight after placement" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCWINDOW)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B3020110" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "ARCAT Inc., 2009" (IFCTEXT)
    Cost = 0. (IFCREAL)
    Description = "CM1414 Single Dome Skylight - Glazing As Specified" (IFCTEXT)
    Drawn By = "Robert S. Weygant, CSI, CDT, SCIP" (IFCTEXT)
    Keynote = "08620" (IFCTEXT)
    Manufacturer = "American Skylights, Inc" (IFCTEXT)
    Model = "CM1414" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Mark = "62" (IFCTEXT)
    Type Name = "CM1414 - Single Dome - Glazing as Specified" (IFCTEXT)
    URL = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCWINDOW)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 20 (IFCINTEGER)
    Installation Phase = "Roof Enclosure" (IFCTEXT)
    Maintenance Schedule (Months) = 12 (IFCINTEGER)
    Warranty Duration (Years) = 10 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Skylight_CM_AmericanSkylites:CM1414 - Single Dome - Glazing as Specified:105669 | predefined | on 1 type object
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Energy Analysis | properties | on 1 type object
    SHGC = 1.1154999999999999 (IFCREAL)
    U_Factor = 0.80000000000000004 (IFCREAL)
  Materials and Finishes | properties | on 1 type object
    Cladding = "Frame - Aluminum - Bronze Anodized" (IFCLABEL)
    Curb Material = "Wood Materials - Pine" (IFCLABEL)
    Flashing Material = "Flashing - As Specified" (IFCLABEL)
    Frame Material = "Aluminum 0.060" - Finish as Specified" (IFCLABEL)
    Inner Dome Material = "None" (IFCLABEL)
    Outer Dome Material = "Acrylic - Clear" (IFCLABEL)
  Structural Analysis | properties | on 1 type object
    E283_Air Infiltration = 43023285.509370565 (IFCPRESSUREMEASURE) [PASCAL]
    E330_Uniform Load_Neg = 517106796.98762703 (IFCPRESSUREMEASURE) [PASCAL]
    E330_Uniform Load_Pos = 475738253.22861683 (IFCPRESSUREMEASURE) [PASCAL]
    E547_E331_Water Penetration = 103421359.3975254 (IFCPRESSUREMEASURE) [PASCAL]
  Text | properties | on 1 type object
    Building Codes = "http://www.americanskylites.com/dade_county_approved.html" (IFCTEXT)
    Construction Details = "http://www.arcat.com/details/american/american.html?coid=30446" (IFCTEXT)
    Green Building-LEED = "http://www.arcat.com/green/green_building.shtml" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos30/arc30446.html" (IFCTEXT)
    Product Properties = "http://www.arcat.com/bim/bim_info.pl?fn=Skylight_Curb-Mount_AmericanSkylights" (IFCTEXT)
    Sales Information = "http://www.americanskylites.com/contact.html" (IFCTEXT)
    SpecWizard = "http://www.arcat.com/specwizard/08600asi/index.htm?mf=&coid=30446" (IFCTEXT)
    Specification = "http://www.arcat.com/sd/clients/american.html?coid=30446" (IFCTEXT)