IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2023-01-19T08:08:48"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Lift_Wheelchair_Ascension_Virtuoso-Portable:as Specified" | object type "Lift_Wheelchair_Ascension_Virtuoso-Portable:as Specified" | names: "Lift_Wheelchair_Ascension_Virtuoso-Portable:as Specified:133206" | material: materials ("Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "Plastic- Ascension - Clear", "Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "Plastic- Ascension - Clear", "Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCBUILDINGELEMENTPROXYTYPE "Lift_Wheelchair_Ascension_Virtuoso-Portable:as Specified" | 1 occurrence | material: materials ("Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "Plastic- Ascension - Clear", "Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "Plastic- Ascension - Clear", "Steel - Ascension - Black Powdercoat", "Steel - Ascension - Black Powdercoat", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Analytical Model, Constraints, Dimensions, Electrical, Identity Data, Other

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Lift_Wheelchair_Ascension_Virtuoso-Portable" (IFCLABEL)
    Family and Type = "Lift_Wheelchair_Ascension_Virtuoso-Portable: as Specified" (IFCLABEL)
    Type = "as Specified" (IFCLABEL)
    Type Id = "133181" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
    Family Name = "Lift_Wheelchair_Ascension_Virtuoso-Portable" (IFCTEXT)
    Manufacturer Address = "3526 E. Ft. Lowell Rd. Tucson, AZ 85716" (IFCTEXT)
    Manufacturer Fax = "520-881-4983" (IFCTEXT)
    Manufacturer Phone - Toll Free = "800-459-0400" (IFCTEXT)
    Manufacturer Phone = "520-881-3993" (IFCTEXT)
    Manufacturer Website = "http://www.wheelchairlift.com/" (IFCTEXT)
    Send Message = "" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "as Specified" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Ascension" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "as Specified" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "Basic Wall : Wall 1" (IFCTEXT)
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Clearance Depth = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Clearance Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 119.96971167304733 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 15.402592000983734 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Platform Clear Length = 4.5208333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Platform Clear Width = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Height = 3.666666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Length = 5.3958333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Width = 3.9375000000000004 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Caster Height = 0.35416666666666663 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Casters Visible = TRUE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Frame Finish = "Steel - Ascension - Black Powdercoat" (IFCLABEL)
    Glazing Tint = "Plastic- Ascension - Clear" (IFCLABEL)
    Glazing Type = "Thermoplastic Panels" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "D1010310" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc." (IFCTEXT)
    Description = "Ascension Portable Wheelchair Vertical Lift - Virtuoso 5460P as Specified" (IFCTEXT)
    Drawn By = "Sumex Design, Inc." (IFCTEXT)
    Keynote = "14420" (IFCTEXT)
    Manufacturer = "Ascension" (IFCTEXT)
    Model = "Virtuoso 5460P" (IFCTEXT)
    OmniClass Number = "23.50.05.14.17.11" (IFCTEXT)
    OmniClass Title = "Platform Lifts" (IFCTEXT)
    Revision = "R1_2015-08" (IFCTEXT)
    Type Comments = "Unit can collapse to fit through 36'' entrances" (IFCTEXT)
    Type Name = "as Specified" (IFCTEXT)
    URL = "http://www.wheelchairlift.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Analytical Model | properties | on 1 type object
    Available Options = "as Specified" (IFCTEXT)
    Capacity = "1 Person Occupancy @ 750 lbs" (IFCTEXT)
    Lift Height = 5. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Lift Travel Speed = "7 ft/min" (IFCTEXT)
    Standards Conformance = "ADAAG ; ASME 17.1 1996, A18.1 ; ANSI 117.1" (IFCTEXT)
  Electrical | properties | on 1 type object
    Electrical_Amperage = 13. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Electrical_Frequency = 60. (IFCFREQUENCYMEASURE) [HERTZ]
    Electrical_Phase = 1 (IFCINTEGER)
    Electrical_Voltage = 120. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Structural | properties | on 1 type object
    Unit Weight = 1025. (IFCREAL)
  Text | properties | on 1 type object
    Building Codes = "" (IFCTEXT)
    Construction Details = "" (IFCTEXT)
    Green Building-LEED = "" (IFCTEXT)
    Installation-Fabrication = "" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos30/arc30670.html" (IFCTEXT)
    Product Properties = "" (IFCTEXT)
    Sales Information = "http://www.wheelchairlift.com/about/where-to-buy" (IFCTEXT)
    SpecWizard = "" (IFCTEXT)
    Specification = "http://www.arcat.com/sdspecs/htm04/14_42_16asc.htm" (IFCTEXT)
    Test Data = "" (IFCTEXT)