IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2023-01-19T09:22:40"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCDOOR | type IFCDOORSTYLE "Door_Sliding_AssaAbloy_AllGlass-BiPart:FSL 10 ft" | object type "Door_Sliding_AssaAbloy_AllGlass-BiPart:FSL 10 ft" | names: "Door_Sliding_AssaAbloy_AllGlass-BiPart:FSL 10 ft:266575" | material: materials ("Metal - Aluminum - Besam - Anodized - Clear", "Metal - Aluminum - Besam - Anodized - Clear", "Plastic - Black", "Plastic - Black", "Metal - Aluminum - Besam - Anodized - Clear", "Glass", "Metal - Aluminum - Besam - Anodized - Clear", "Metal - Aluminum - Besam - Anodized - Clear", "Glass", "Metal - Aluminum - Besam - Anodized - Clear", "Metal - Aluminum - Besam - Anodized - Clear", "Glass", "Metal - Aluminum - Besam - Anodized - Clear", "Metal - Aluminum - Besam - Anodized - Clear", "Glass", "Metal - Aluminum - Besam - Anodized - Clear", "Metal - Aluminum - Besam - Anodized - Clear") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, IfcDoorPanelProperties

Types
  IFCDOORSTYLE "Door_Sliding_AssaAbloy_AllGlass-BiPart:FSL 10 ft" | 1 occurrence | material: materials ("Metal - Aluminum - Besam - Anodized - Clear", "Metal - Aluminum - Besam - Anodized - Clear", "Plastic - Black", "Plastic - Black", "Metal - Aluminum - Besam - Anodized - Clear", "Glass", "Metal - Aluminum - Besam - Anodized - Clear", "Metal - Aluminum - Besam - Anodized - Clear", "Glass", "Metal - Aluminum - Besam - Anodized - Clear", "Metal - Aluminum - Besam - Anodized - Clear", "Glass", "Metal - Aluminum - Besam - Anodized - Clear", "Metal - Aluminum - Besam - Anodized - Clear", "Glass", "Metal - Aluminum - Besam - Anodized - Clear", "Metal - Aluminum - Besam - Anodized - Clear") | property sets: Door_Sliding_AssaAbloy_AllGlass-BiPart:FSL 10 ft:266575, Door_Sliding_AssaAbloy_AllGlass-BiPart:FSL 10 ft:266575:1, Analytical Model, Analytical Properties, Constraints, Construction

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "Door_Sliding_AssaAbloy_AllGlass-BiPart" (IFCLABEL)
    Family and Type = "Door_Sliding_AssaAbloy_AllGlass-BiPart: FSL 10 ft" (IFCLABEL)
    Head Height = 7.4791666666666679 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "266565" (IFCLABEL)
    Type = "FSL 10 ft" (IFCLABEL)
    Type Id = "266547" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Doors" (IFCLABEL)
    Family Name = "Door_Sliding_AssaAbloy_AllGlass-BiPart" (IFCTEXT)
    Manufacturer Address = "1900 Airport Rd., Monroe, NC 28110" (IFCTEXT)
    Manufacturer Fax = "704-290-5555" (IFCTEXT)
    Manufacturer Phone - Toll Free = "877-SPEC-123" (IFCTEXT)
    Manufacturer Website = "http://www.besam-usa.com/en/besam/us/" (IFCTEXT)
    Send Message = "http://www.arcat.com/users.pl?action=UserEmail&company=Besam%20Entrance%20Solutions&coid=30906&rep=141&fax=704-290-5555&mf=" (IFCTEXT)
  Pset_ConcreteElementGeneral | properties | on 1 object (1 IFCDOOR) | on 1 type object
    FireRating = "As Specified" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireRating = "As Specified" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "FSL 10 ft" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 type object
    FireRating = "As Specified" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Manufacturer = "ASSA ABLOY Entrance Systems" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR)
    Reference = "FSL 10 ft" (IFCIDENTIFIER)
  IfcDoorPanelProperties | properties | on 1 object (1 IFCDOOR) | on 1 type object
    PanelWidth (no value)
  Constraints | properties | on 1 object (1 IFCDOOR)
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    RO Offset = 0.020833333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCDOOR)
    Offset from Wall CL = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Wall CL Offset Notes = "Use positive or negative values to determine location" (IFCTEXT)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCDOOR)
    Area = 116.90786714294113 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Clear Opening Height = 6.7395833333333348 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Glazing Thickness = 0.020833333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Height = 6.8750000000000009 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 5.7888384696226067 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Clear Opening Width = 3.8437500000000004 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Frame Thickness = 0.375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 7.4791666666666679 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Jamb Width = 0.14583333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Thickness = 0.15625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Width = 2.4895833333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 7.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 10.041666666666668 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Thickness = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCDOOR)
    Electrical_Amperage = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Electrical_Frequency = 0. (IFCFREQUENCYMEASURE) [HERTZ]
    Electrical_Voltage = 0. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Graphics | properties | on 1 object (1 IFCDOOR)
    Include Threshold = FALSE (IFCBOOLEAN)
    Rail Height_Bottom = 0.58333333333333337 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Mark = "40" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2030110" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc." (IFCTEXT)
    Description = "ASSA ABLOY All Glass BiPart Sliding Door - Besam SL500 CGL BP FSL10 as Specified" (IFCTEXT)
    Drawn By = "Sumex Design, Inc. / Robert S. Weygant, CSI, CDT, SCIP" (IFCTEXT)
    Fire Rating = "As Specified" (IFCTEXT)
    Keynote = "08463" (IFCTEXT)
    Manufacturer = "ASSA ABLOY Entrance Systems" (IFCTEXT)
    Model = "Besam SL500 CGL BP FSL10" (IFCTEXT)
    OmniClass Number = "23.30.10.17.11" (IFCTEXT)
    OmniClass Title = "Sliding Doors" (IFCTEXT)
    Type Mark = "136" (IFCTEXT)
    Type Name = "FSL 10 ft" (IFCTEXT)
    URL = "http://www.besam-usa.com/en/besam/us/" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCDOOR)
    Frame Finish = "Metal - Aluminum - Besam - Anodized - Clear" (IFCLABEL)
    Glazing Configuration = "" (IFCTEXT)
    Glazing Tint = "Glass" (IFCLABEL)
    Glazing Type = "" (IFCTEXT)
    Hardware Finish = "Plastic - Black" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCDOOR)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Door_Sliding_AssaAbloy_AllGlass-BiPart:FSL 10 ft:266575 | predefined | on 1 type object
  Door_Sliding_AssaAbloy_AllGlass-BiPart:FSL 10 ft:266575:1 | predefined | on 1 type object
  Analytical Model | properties | on 1 type object
    Standards Conformance = "as Specified" (IFCTEXT)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Text | properties | on 1 type object
    Building Codes = "" (IFCTEXT)
    Construction Details = "http://www.arcat.com/details/besamaut/besamaut.html?coid=30906" (IFCTEXT)
    Green Building-LEED = "http://www.arcat.com/green/clients/leed_data_30906.html" (IFCTEXT)
    Installation-Fabrication = "http://www.besam-usa.com/en/besam/us/Downloads/" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos30/arc30906.html" (IFCTEXT)
    Product Properties = "http://www.besam-usa.com/en/besam/us/Products/" (IFCTEXT)
    Sales Information = "http://www.besam-usa.com/en/besam/us/About-us/Contact-Us/" (IFCTEXT)
    SpecWizard = "http://www.arcat.com/specwizard/clients/besamaut.html?coid=30906" (IFCTEXT)
    Specification = "http://www.arcat.com/sd/clients/besamaut.html?coid=30906" (IFCTEXT)
    Test Data = "" (IFCTEXT)