IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-01-22T10:43:35"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Overhead_Door-CHI_Overhead_Doors-Sectional_Full_View:Sectional Full View - 3297 - Dark bronze" | object type "Overhead_Door-CHI_Overhead_Doors-Sectional_Full_View:Sectional Full View - 3297 - Dark bronze" | names: "Overhead_Door-CHI_Overhead_Doors-Sectional_Full_View:Sectional Full View - 3297 - Dark bronze:470656" | material: materials ("Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Silver", "Metal - C.H.I Overhead Doors - Silver", "Metal - C.H.I Overhead Doors - Silver", "Metal - C.H.I Overhead Doors - Silver") | property sets: Pset_BuildingElementProxyCommon, Pset_ConcreteElementGeneral, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "Overhead_Door-CHI_Overhead_Doors-Sectional_Full_View:Sectional Full View - 3297 - Dark bronze" | 1 occurrence | material: materials ("Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Black", "Metal - C.H.I Overhead Doors - Silver", "Metal - C.H.I Overhead Doors - Silver", "Metal - C.H.I Overhead Doors - Silver", "Metal - C.H.I Overhead Doors - Silver") | property sets: Constraints, Construction, Dimensions, Electrical, Identity Data, Materials and Finishes

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    C Desired Panel Height = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Desired Panel Width = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Hook From Wall = 0.21875000000000003 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Motor Offset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Motor Side = 0.54133858267716539 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Operator Control Offset From Ground = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Operator Control Side Offset = 3.166666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Panel Height Overlap = 0.059895833333333343 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Panel Wall Offset = 0.03125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Panel Width Overlap = 0.14192708333333334 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Springs Back = FALSE (IFCBOOLEAN)
    C Springs Back Width = 9.1666666666666679 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Springs Front = FALSE (IFCBOOLEAN)
    C Wall Edge Offset = 0.020833333333333336 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Overhead_Door-CHI_Overhead_Doors-Sectional_Full_View" (IFCLABEL)
    Family and Type = "Overhead_Door-CHI_Overhead_Doors-Sectional_Full_View: Sectional Full View - 3297 - Dark bronze" (IFCLABEL)
    Host Id = "470646" (IFCLABEL)
    Panel Height = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Min Height = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Min Width = 8. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Width = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Type = "Sectional Full View - 3297 - Dark bronze" (IFCLABEL)
    Type Constraint = 1 (IFCINTEGER)
    Type Id = "470628" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    C Appeance = 5 (IFCINTEGER)
    C Door Bottom Offset = 0.029947916666666671 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Side Rail Radius = 1.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Constraints = 22 (IFCINTEGER)
    Family Name = "Overhead_Door-CHI_Overhead_Doors-Sectional_Full_View" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Sectional Full View - 3297 - Dark bronze" (IFCIDENTIFIER)
  Pset_ConcreteElementGeneral | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    ConstructionType = "Glass garage doors" (IFCLABEL)
    FireRating = "Contact Manufacturer for More Information" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "C.H.I. Overhead Doors" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Sectional Full View - 3297 - Dark bronze" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    12" Radius = TRUE (IFCBOOLEAN)
    15" Radius = FALSE (IFCBOOLEAN)
    2" Track = TRUE (IFCBOOLEAN)
    3" Track = FALSE (IFCBOOLEAN)
    Control Panel Offset from Ground = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Control Panel from Door Side = 1. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Desired Head Room = 5. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Head Room = 1.2500000000000002 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Head Room Warning = "Desired Head Room only affects "Lift Track" option" (IFCTEXT)
    JDC Operator - Left = FALSE (IFCBOOLEAN)
    JDC Operator - Right = FALSE (IFCBOOLEAN)
    Lift Track = FALSE (IFCBOOLEAN)
    Low Headroom = FALSE (IFCBOOLEAN)
    Mounting Option = 1 (IFCINTEGER)
    Mounting Option Description = "Standard Lift Track" (IFCTEXT)
    Operator Constraint = 1 (IFCINTEGER)
    Springs Back = TRUE (IFCBOOLEAN)
    Springs Front = FALSE (IFCBOOLEAN)
    Springs Option Description = "Options Not Available" (IFCTEXT)
    Standard Track = TRUE (IFCBOOLEAN)
    Steel Jamb = TRUE (IFCBOOLEAN)
    TDC Operator = TRUE (IFCBOOLEAN)
    Vertical Lift = FALSE (IFCBOOLEAN)
    Wood Jamb = FALSE (IFCBOOLEAN)
  Construction | properties | on 1 type object
    Construction Type = "Glass garage doors" (IFCTEXT)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 766.57706917206542 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Desired Height = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Desired Width = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Height = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Width = 9.8333333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Max Height = 16. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Max Width = 24.166666666666668 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 29.425211221948793 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Panel Thickness = 0.16666666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Power Factor = 1. (IFCREAL)
  Electrical | properties | on 1 type object
    Load Classification = "Other" (IFCLABEL)
    Number of Phases = 1 (IFCINTEGER)
    Number of Poles = 1 (IFCINTEGER)
    Voltage = 115. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2030410" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©2024 C.H.I. Overhead Doors - a NUCOR® company All information presented is based on the specifications and features available at the time of printing and is subject to change without notice." (IFCTEXT)
    Description = "Glass Garage Doors" (IFCTEXT)
    Fire Rating = "Contact Manufacturer for More Information" (IFCTEXT)
    Keynote = "08 30 00" (IFCTEXT)
    Manufacturer = "C.H.I. Overhead Doors" (IFCTEXT)
    Manufacturer Address = "1485 Sunrise Drive, Arthur, IL 61911" (IFCTEXT)
    Manufacturer Email = "aia@chiohd.com" (IFCTEXT)
    Manufacturer Fax Number = "800-738-5006" (IFCTEXT)
    Manufacturer Phone Number = "800-677-2650" (IFCTEXT)
    Model = "3297" (IFCTEXT)
    OmniClass Number = "23.30.10.21" (IFCTEXT)
    OmniClass Title = "Special Function Doors" (IFCTEXT)
    Product Documentation Link = "https://www.chiohd.com/hubfs/3297-full-view-aluminum.pdf" (IFCTEXT)
    Product Page URL = "https://www.chiohd.com/commercial-doors/commercial-full-view-aluminum/3297" (IFCTEXT)
    Support Email = "mailto:support@bimsmith.com" (IFCTEXT)
    Support Phone = "(224) 699-9545" (IFCTEXT)
    Type Name = "Sectional Full View - 3297 - Dark bronze" (IFCTEXT)
    URL = "https://www.chiohd.com/" (IFCTEXT)
    Version = "2021-v1.a" (IFCTEXT)
    Warranty URL = "https://www.chiohd.com/support/warranty" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Panel Finish = "Metal - Powder Coat - C.H.I Overhead Doors - Dark Bronze" (IFCLABEL)
  Model Properties | properties | on 1 type object
    Air Infiltration = "0.42" (IFCTEXT)
    Appearance = "Fullview with equal spacing" (IFCTEXT)
    Certified Windload = TRUE (IFCBOOLEAN)
    Closing Speed = "Contact Manufacturer for More Information" (IFCTEXT)
    DASMA Thermal Verification Program = FALSE (IFCBOOLEAN)
    IECC Compliant = FALSE (IFCBOOLEAN)
    Impact = TRUE (IFCBOOLEAN)
    Opening Speed = "Contact Manufacturer for More Information" (IFCTEXT)
    R-Value = "3.07" (IFCTEXT)
    STC = "27" (IFCTEXT)
    U Factor = "0.88" (IFCTEXT)