IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-07-10T14:05:40"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCDOOR | type IFCDOORSTYLE "3715-1Basic:By Type" | object type "3715-1Basic:By Type" | names: "3715-1Basic:By Type:130196" | material: materials ("White", "White", "White", "White", "White", "White", "White") | property sets: Pset_DoorCommon, Pset_ElementShading, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints

Types
  IFCDOORSTYLE "3715-1Basic:By Type" | 1 occurrence | material: materials ("White", "White", "White", "White", "White", "White", "White") | property sets: 3715-1Basic:By Type:130196, 3715-1Basic:By Type:130196:1, Analytical Properties, Constraints, Construction, Dimensions

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "3715-1Basic" (IFCLABEL)
    Family and Type = "3715-1Basic: By Type" (IFCLABEL)
    Head Height = 14. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "130186" (IFCLABEL)
    Type = "By Type" (IFCLABEL)
    Type Id = "130162" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Doors" (IFCLABEL)
    Family Name = "3715-1Basic" (IFCTEXT)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "By Type" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_ElementShading | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Color = "White" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Manufacturer = "Clopay Building Products Company" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR)
    Reference = "By Type" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCDOOR)
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Double End Stiles = FALSE (IFCBOOLEAN)
    FloorToSection2 = 2. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    FloorToSection3 = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    FloorToSection4 = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    FloorToSection5 = 8. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    FloorToSection6 = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    FloorToSection7 = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumArraySections = 2 (IFCINTEGER)
    NumSections = 7 (IFCINTEGER)
    NumSectionsNotRounded = 7. (IFCREAL)
    Section Height = 2. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    VisArray = TRUE (IFCBOOLEAN)
    VisSection3 = TRUE (IFCBOOLEAN)
    VisSection4 = TRUE (IFCBOOLEAN)
    VisSection5 = TRUE (IFCBOOLEAN)
    VisSection6 = FALSE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCDOOR)
    Area = 212.52797137608027 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 32.383537127509129 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Door Height = 14. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Width = 12.166666666666666 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 14. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Maximum Size = "Maximum 32' 2'' wide by 26' 0'' high. Additional limitations may apply do to door weight. Consult Clopay for specificiations and shop drawings." (IFCTEXT)
    Opening Height = 14. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Width = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overlap = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Thickness = 0.16666666666666666 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2030410" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "2010, Clopay Building Products Company, Inc." (IFCTEXT)
    Description = "1-3/8'' thick polyurethane insulated, stucco embossed 27 gauge steel exterior with light ribbed pattern." (IFCTEXT)
    File Revision = "02 (August, 2012)" (IFCTEXT)
    Keynote = "08 36 13" (IFCTEXT)
    Manufacturer = "Clopay Building Products Company" (IFCTEXT)
    Model = "3715" (IFCTEXT)
    OmniClass Number = "23.30.10.17.37.14" (IFCTEXT)
    OmniClass Title = "Sectional Overhead Doors" (IFCTEXT)
    Omniclass Table = "23-30 10 17 37" (IFCTEXT)
    Type Mark = "4" (IFCTEXT)
    Type Name = "By Type" (IFCTEXT)
    URL = "www.clopaydoor.com" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCDOOR)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  3715-1Basic:By Type:130196 | predefined | on 1 type object
  3715-1Basic:By Type:130196:1 | predefined | on 1 type object
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Overlapping Jamb = TRUE (IFCBOOLEAN)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Energy Analysis | properties | on 1 type object
    R-Value = "12.9" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    GreenFormat = "http://www.greenformat.com/products/1536-Polyurethane%20Insulated%20Doors.rtf" (IFCTEXT)
    LEED = "http://products.construction.com/swts_content_files/151607/303186.pdf" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Color = "White" (IFCLABEL)
    Core Material = "Expanded polyurethane" (IFCTEXT)
    Exterior Steel = "27 ga. galvanized, primed, and finish painted" (IFCTEXT)
    Hardware = "14 ga. min. steel hinges; 10-ball steel rollers" (IFCTEXT)
    Interior Steel = "28 ga. galvanized, primed, and finish painted" (IFCTEXT)
    Track = "Galvanized steel (gauge varies according to door size)" (IFCTEXT)
  Text | properties | on 1 type object
    CAD and Specifications = "http://www.clopaydoor.com/insulated-polyurethane-specs.aspx" (IFCTEXT)
    Manufacturer Address = "1400 W. Market St., Troy, OH 45373" (IFCTEXT)
    Manufacturer Phone Number = "1-800-526-4301" (IFCTEXT)
    Manufacturer Website = "http://www.clopaydoor.com" (IFCTEXT)
    Product Features and Benefits = "http://www.clopaydoor.com/insulated-polyurethane-applications.aspx" (IFCTEXT)
    Sales Information = "http://www.clopaydoor.com/where-to-buy.aspx?type=dealer" (IFCTEXT)
    Spec Wizard = "http://www.arcat.com/specwizard/08360clo/index.htm" (IFCTEXT)
    Windload = "Doors available rated for various design pressures; consult Clopay for avaialbility and specifications" (IFCTEXT)