IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2023-01-19T12:14:55"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCDOOR | type IFCDOORSTYLE "Door_Sectional_Clopay_Insulated-HorizontalTrack-LowHeadroom:ByType" | object type "Door_Sectional_Clopay_Insulated-HorizontalTrack-LowHeadroom:ByType" | names: "Door_Sectional_Clopay_Insulated-HorizontalTrack-LowHeadroom:ByType:226288" | material: materials ("Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Glass - Insulated - Clopay - Clear Tempered", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Glass - Insulated - Clopay - Clear Tempered", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Glass - Insulated - Clopay - Clear Tempered", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized") | property sets: Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, IfcDoorPanelProperties, Constraints

Types
  IFCDOORSTYLE "Door_Sectional_Clopay_Insulated-HorizontalTrack-LowHeadroom:ByType" | 1 occurrence | material: materials ("Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Glass - Insulated - Clopay - Clear Tempered", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Glass - Insulated - Clopay - Clear Tempered", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Glass - Insulated - Clopay - Clear Tempered", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Stucco Emboss - Tan", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized", "Metal - Steel - Clopay - Galvanized") | property sets: Door_Sectional_Clopay_Insulated-HorizontalTrack-LowHeadroom:ByType:226288, Door_Sectional_Clopay_Insulated-HorizontalTrack-LowHeadroom:ByType:226288:1, Analytical Model, Analytical Properties, Constraints, Construction

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "Door_Sectional_Clopay_Insulated-HorizontalTrack-LowHeadroom" (IFCLABEL)
    Family and Type = "Door_Sectional_Clopay_Insulated-HorizontalTrack-LowHeadroom: ByType" (IFCLABEL)
    Head Height = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "226278" (IFCLABEL)
    Type = "ByType" (IFCLABEL)
    Type Id = "226260" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Doors" (IFCLABEL)
    Family Name = "Door_Sectional_Clopay_Insulated-HorizontalTrack-LowHeadroom" (IFCTEXT)
    Manufacturer Address = "8585 Duke Blvd. Mason, OH 45040-3101" (IFCTEXT)
    Manufacturer Fax = "513-770-3519" (IFCTEXT)
    Manufacturer Phone - Toll Free = "800-526-4301" (IFCTEXT)
    Manufacturer Phone = "513-770-4800" (IFCTEXT)
    Manufacturer Website = "http://www.arcat.com/users.pl?action=UserEmail&company=Clopay%20Building%20Products%20Company&coid=31487&rep=114&fax=513-770-3519&mf=" (IFCTEXT)
    Send Message = "http://www.clopaydoor.com/" (IFCTEXT)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ByType" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Manufacturer = "Clopay Building Products Company" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR)
    Reference = "ByType" (IFCIDENTIFIER)
  IfcDoorPanelProperties | properties | on 1 object (1 IFCDOOR)
    PanelWidth (no value)
  Constraints | properties | on 1 object (1 IFCDOOR)
    DblWidth = 14.833333333333334 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Front Mount = TRUE (IFCBOOLEAN)
    Int Width = 12.333333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    IntBottom = 0.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    IntTop = 0.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Lift Clearance = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rad = 0.072916666666666657 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Torsion Spring Height above Head = 0.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    TorsionWidth = 13.833333333333334 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Track Radius = 1.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    NumPanels = 7 (IFCINTEGER)
    NumPanels_3211 = 7 (IFCINTEGER)
    NumPanels_Standard = 6 (IFCINTEGER)
    P10 = FALSE (IFCBOOLEAN)
    P11 = FALSE (IFCBOOLEAN)
    P4 = TRUE (IFCBOOLEAN)
    P5 = TRUE (IFCBOOLEAN)
    P6 = TRUE (IFCBOOLEAN)
    P7 = TRUE (IFCBOOLEAN)
    P8 = FALSE (IFCBOOLEAN)
    P9 = FALSE (IFCBOOLEAN)
    RO Offset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCDOOR)
    3" Track = FALSE (IFCBOOLEAN)
    Double Torsion Shaft = FALSE (IFCBOOLEAN)
    Lock Left = FALSE (IFCBOOLEAN)
    Lock Right = FALSE (IFCBOOLEAN)
    Operator_Jackshaft Left = FALSE (IFCBOOLEAN)
    Operator_Jackshaft Right = FALSE (IFCBOOLEAN)
    Operator_Standard = FALSE (IFCBOOLEAN)
    Panel Type_1 = "Door Panel : Standard" (IFCLABEL)
    Panel Type_10 = "Door Panel : Standard" (IFCLABEL)
    Panel Type_11 = "Door Panel : Standard" (IFCLABEL)
    Panel Type_2 = "Door Panel : Standard" (IFCLABEL)
    Panel Type_3 = "Door Panel : Standard" (IFCLABEL)
    Panel Type_4 = "Door Panel : Standard" (IFCLABEL)
    Panel Type_5 = "Door Panel : Standard" (IFCLABEL)
    Panel Type_6 = "Door Panel : Vision Panels - 24x12" (IFCLABEL)
    Panel Type_7 = "Door Panel : Standard" (IFCLABEL)
    Panel Type_8 = "Door Panel : Standard" (IFCLABEL)
    Panel Type_9 = "Door Panel : Standard" (IFCLABEL)
    Rear Mount Torsion Spring = FALSE (IFCBOOLEAN)
  Construction | properties | on 1 type object
    3211 Spacing = TRUE (IFCBOOLEAN)
    Breakaway Bottom Section = FALSE (IFCBOOLEAN)
    Function = "Interior" (IFCIDENTIFIER)
    Pass Door = TRUE (IFCBOOLEAN)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCDOOR)
    Area = 667.7047730717793 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Bottom Astragal Height = 0.29166666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Horizontal Support Height = 2. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Jackshaft Offset = 0.83333333333333337 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Width = 12.166666666666666 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Roof Rise per Foot = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 129.72615962225723 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Door Height = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Width = 12.166666666666666 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Frame Thickness = 0.39583333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Maximum Size = "Consult Clopay Specifications & Shop Drawings" (IFCTEXT)
    Opening Height = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Width = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Height = 1.7142857142857142 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Thickness = 0.14583333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Track Offset = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Mark = "16" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2030410" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc." (IFCTEXT)
    Description = "Clopay Overhead Door as Specified" (IFCTEXT)
    Drawn By = "Sumex Design, Inc. / Robert S. Weygant, CSI, CDT, SCIP" (IFCTEXT)
    Fire Rating = "" (IFCTEXT)
    Keynote = "08360" (IFCTEXT)
    Manufacturer = "Clopay Building Products Company" (IFCTEXT)
    Model = "As Specified" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Revision = "R1_09-2011" (IFCTEXT)
    Type Mark = "16" (IFCTEXT)
    Type Name = "ByType" (IFCTEXT)
    URL = "http://www.clopaydoor.com/" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCDOOR)
    Bottom Astragal Material = "Rubber - Clopay - Black" (IFCLABEL)
    Track Material = "Metal - Steel - Clopay - Galvanized" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Door Glazing = "Glass - Insulated - Clopay - Clear Tempered" (IFCLABEL)
    Frame Finish = "Metal - Steel - Clopay - Stucco Emboss - Tan" (IFCLABEL)
    Hardware Finish = "Metal - Steel - Clopay - Galvanized" (IFCLABEL)
    Panel Material = "Metal - Steel - Clopay - Stucco Emboss - Tan" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCDOOR)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Door_Sectional_Clopay_Insulated-HorizontalTrack-LowHeadroom:ByType:226288 | predefined | on 1 type object
  Door_Sectional_Clopay_Insulated-HorizontalTrack-LowHeadroom:ByType:226288:1 | predefined | on 1 type object
  Analytical Model | properties | on 1 type object
    AAMA Designation = "" (IFCTEXT)
    ADA Compliant = TRUE (IFCBOOLEAN)
    ASTM Conformance = "" (IFCTEXT)
    Air Infiltration = "" (IFCTEXT)
    Building Code Conformance = "" (IFCTEXT)
    R_Value = 0. (IFCREAL)
    Sound Transmission Class (STC) = 0 (IFCINTEGER)
    Water Penetration = "" (IFCTEXT)
    Wind Load = "" (IFCTEXT)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Text | properties | on 1 type object
    Building Codes = "" (IFCTEXT)
    Construction Details = "http://www.arcat.com/details/clopay/clopay.html?coid=31487" (IFCTEXT)
    Green Building-LEED = "http://www.arcat.com/green/clients/leed_data_31487.html" (IFCTEXT)
    Installation-Fabrication = "" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos31/arc31487.html?isac=1&r=1" (IFCTEXT)
    Product Properties = "" (IFCTEXT)
    Sales Information = "http://www.clopaydoor.com/contact-us.aspx" (IFCTEXT)
    SpecWizard = "http://www.arcat.com/specwizard/clients/clopay.html?coid=31487" (IFCTEXT)
    Specification = "http://www.arcat.com/sd/clients/clopay.html?coid=31487" (IFCTEXT)
    Test Data = "" (IFCTEXT)