IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2023-01-23T10:54:58"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Fireplaces_DaVinci_TimberFyre_48x30-SS-TF:Timberfyre Signle Sided 48" x 30"" | object type "Fireplaces_DaVinci_TimberFyre_48x30-SS-TF:Timberfyre Signle Sided 48" x 30"" | names: "Fireplaces_DaVinci_TimberFyre_48x30-SS-TF:Timberfyre Signle Sided 48" x 30":95533" | material: materials ("Matel", "Glass", "Matel", "Matel", "Matel", "Matel", "Matel", "Matel") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "Fireplaces_DaVinci_TimberFyre_48x30-SS-TF:Timberfyre Signle Sided 48" x 30"" | 1 occurrence | material: materials ("Matel", "Glass", "Matel", "Matel", "Matel", "Matel", "Matel", "Matel") | property sets: Constraints, Data, Dimensions, Electrical - Loads, Electrical Engineering, Identity Data

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Fireplaces_DaVinci_TimberFyre_48x30-SS-TF" (IFCLABEL)
    Family and Type = "Fireplaces_DaVinci_TimberFyre_48x30-SS-TF: Timberfyre Signle Sided 48" x 30"" (IFCLABEL)
    Type = "Timberfyre Signle Sided 48" x 30"" (IFCLABEL)
    Type Id = "95499" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Fireplaces_DaVinci_TimberFyre_48x30-SS-TF" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Timberfyre Signle Sided 48" x 30"" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Davinci Custom Fireplaces" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Timberfyre Signle Sided 48" x 30"" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Depth = 2. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Height = 5.0520833333333339 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 4.166666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Work Plane = "???" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 82.636969994842985 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 10.338757395660474 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Depth = 2. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Exhaust = 0.66666666666666674 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 5.0520833333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Intakes = 0.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 4.166666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    X1 = 0.70833333333333337 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    X2 = 0.54166666666666663 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©2020 Travis Industries, Inc" (IFCTEXT)
    Cost = 0. (IFCREAL)
    Description = "" (IFCTEXT)
    Keynote = "" (IFCTEXT)
    Manufacturer = "Davinci Custom Fireplaces" (IFCTEXT)
    Model = "Timberfyre Signle Sided 48" x 30"" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Product Documentation Link = "https://www.travisindustries.com/docs/98800900.pdf" (IFCTEXT)
    Product Page URL = "https://www.arcat.com/arcatcos/cos49/arc49714.html" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "Timberfyre Signle Sided 48" x 30"" (IFCTEXT)
    URL = "https://www.davincifireplace.com/" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Exhaust Air,Other Air,Power,Domestic Hot Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Data | properties | on 1 type object
    CAD Details = "https://www.arcat.com/company/davinci-custom-fireplaces-a-division-of-travis-industries-49714/cad" (IFCTEXT)
    Specifications = "https://www.arcat.com/company/davinci-custom-fireplaces-a-division-of-travis-industries-49714/spec" (IFCTEXT)
  Electrical - Loads | properties | on 1 type object
    Apparent Load = 0. (IFCPOWERMEASURE) [WATT]
  Electrical Engineering | properties | on 1 type object
    Electrical Req'd = 119.99999225760001 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Gas Req'd = "115,000 BTU's" (IFCTEXT)
    Number Pole = 1 (IFCINTEGER)
  Materials and Finishes | properties | on 1 type object
    Glass = "Glass" (IFCLABEL)
    Matel = "Matel" (IFCLABEL)
  Model Properties | properties | on 1 type object
    LP = "Min = 11"wc (2.74 kpa), Max = 13"wc (3.23 kpa)" (IFCTEXT)
    NG = "Min = 5.5"wc (1.37kpa), Max = 7"wc (1.74 kpa)" (IFCTEXT)