IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2024-01-05T09:05:40"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.70.21 - Exporter 21.1.70.21 - Default UI"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1686682715 (2023-06-13T18:58:35Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Columns_Fire-Trol_Fireproof_Square-Type-SO-Rating-2-Hour:Pipe24SCH160-27X27X0.25" | object type "Columns_Fire-Trol_Fireproof_Square-Type-SO-Rating-2-Hour:Pipe24SCH160-27X27X0.25" | names: "Columns_Fire-Trol_Fireproof_Square-Type-SO-Rating-2-Hour:Pipe24SCH160-27X27X0.25:114836" | material: materials ("Fire-Trol - Concrete - Vermiculite", "Fire-Trol - Metal - A500 Grade B", "Fire-Trol - Concrete - ASTM-C94", "Fire-Trol - Metal - A-53 Grade B") | property sets: Pset_ColumnCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Constraints

Types
  IFCCOLUMNTYPE "Columns_Fire-Trol_Fireproof_Square-Type-SO-Rating-2-Hour:Pipe24SCH160-27X27X0.25" | COLUMN | 1 occurrence | material: materials ("Fire-Trol - Metal - A-53 Grade B", "Fire-Trol - Metal - A500 Grade B", "Fire-Trol - Concrete - Vermiculite", "Fire-Trol - Concrete - ASTM-C94") | property sets: Data, Dimensions, Identity Data, Materials and Finishes, Other, Structural

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCCOLUMN) | on 1 type object
    Category = "Structural Columns" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCCOLUMN)
    Category = "Structural Columns" (IFCLABEL)
    Family = "Columns_Fire-Trol_Fireproof_Square-Type-SO-Rating-2-Hour: Pipe24SCH160-27X27X0.25" (IFCLABEL)
    Family and Type = "Columns_Fire-Trol_Fireproof_Square-Type-SO-Rating-2-Hour: Pipe24SCH160-27X27X0.25" (IFCLABEL)
    Type = "Columns_Fire-Trol_Fireproof_Square-Type-SO-Rating-2-Hour: Pipe24SCH160-27X27X0.25" (IFCLABEL)
    Type Id = "Columns_Fire-Trol_Fireproof_Square-Type-SO-Rating-2-Hour: Pipe24SCH160-27X27X0.25" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Structural Columns" (IFCLABEL)
    Family Name = "Columns_Fire-Trol_Fireproof_Square-Type-SO-Rating-2-Hour" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Pipe24SCH160-27X27X0.25" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCCOLUMN) | on 1 type object
    Manufacturer = "Fire-Trol" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCCOLUMN) | on 1 type object
    Reference = "Pipe24SCH160-27X27X0.25" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN) | on 1 type object
    Description = "Round core column with square shell" (IFCTEXT)
    Reference = "Pipe24SCH160-27X27X0.25" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCCOLUMN)
    Base Level = "Level: Level 1" (IFCLABEL)
    Base Offset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Column Location Mark = "" (IFCTEXT)
    Column Style = "Vertical" (IFCIDENTIFIER)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Grids = TRUE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Level = "Level: Level 1" (IFCLABEL)
    Top Offset = 8.20209973753281 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCCOLUMN)
    Length = 8.20209973753281 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 41.5231299212598 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Core I.D. = 1.80466666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Core O.D. = 2. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Core Wall Thickness = 0.195333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Shell Depth = 2.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Shell Wall Thickness = 0.0208333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Shell Width = 2.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Materials and Finishes | properties | on 1 object (1 IFCCOLUMN)
    Structural Material = "Fire-Trol - Metal - A-53 Grade B" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Core Filled Material = "Fire-Trol - Concrete - ASTM-C94" (IFCLABEL)
    Interior Core Column Material = "Fire-Trol - Metal - A-53 Grade B" (IFCLABEL)
    Outer Shell Filled Material = "Fire-Trol - Concrete - Vermiculite" (IFCLABEL)
    Outer Shell Material = "Fire-Trol - Metal - A500 Grade B" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCCOLUMN)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 1 object (1 IFCCOLUMN)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
  Structural | properties | on 1 type object
    Section Shape = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Date Created = "19.06.23" (IFCTEXT)
    Date Updated = "19.06.23" (IFCTEXT)
    Description = "Round core column with square shell" (IFCTEXT)
    Manufacturer = "Fire-Trol" (IFCTEXT)
    Model = "Pipe24SCH160-27X27X0.25" (IFCTEXT)
    OmniClass Number = "23.13.31.11" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Product Page URL = "https://fire-trol.com/fire-trol-prefabricated-fireproof-columns-type-so/" (IFCTEXT)
    Product data url = "https://www.bimobject.com/fire-trol/product/prefabricated-fireproof-columns-square-type-so" (IFCTEXT)
    Type Name = "Pipe24SCH160-27X27X0.25" (IFCTEXT)
    URL = "https://fire-trol.com/" (IFCTEXT)
    Version = 1 (IFCINTEGER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Data | properties | on 1 type object
    Fire Ratings = "X106" (IFCTEXT)
    Warranty = "A one-year limited warranty is provided by manufacturer." (IFCTEXT)
    Weight per foot = 705.567423896482 (IFCREAL)