IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
File name: "Project Number"
Time stamp: "2025-08-25T13:06:30-05:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "23.0.11.19 - Exporter 23.0.11.19 - Default UI"
Application: "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)" | change NOCHANGE | created 1756139501 (2025-08-25T16:31:41Z)

Units
  LENGTHUNIT: INCH (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:1/4" Head" | elevation 0.
        contains 12 elements
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 30"" | object type "Basic Wall:Generic - 30"" | names: "Basic Wall:Generic - 30":309091", "Basic Wall:Generic - 30":309132", "Basic Wall:Generic - 30":313008" | material: layers "Basic Wall:Generic - 30"" ("Default Wall" 21.) | property sets: Constraints, Cross-Section Definition, Dimensions, Identity Data, Other, Phasing
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1" | object type "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1" | names: "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1:311077", "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1:311207" | material: materials ("Regency Fireplace - Metal - Silver", "Regency Fireplace - Metal - Black Inner Panel", "<Unnamed>", "Regency Fireplace - Glass - Clear", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Wood - Birch Log Set Firebed"); materials ("Regency Fireplace - Metal - Silver", "Regency Fireplace - Metal - Black Inner Panel", "<Unnamed>", "Regency Fireplace - Glass - Clear", "Regency Fireplace - Metal - Black", "Regency Fireplace - Wood - Birch Log Set Firebed") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Construction
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Generic - 30"" | object type "Basic Wall:Generic - 30"" | names: "Basic Wall:Generic - 30":312580" | material: layers "Basic Wall:Generic - 30"" ("Default Wall" 21.) | property sets: Constraints, Cross-Section Definition, Dimensions, Identity Data, Other, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1" | object type "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1" | names: "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1:312710" | material: materials ("Regency Fireplace - Metal - Silver", "Regency Fireplace - Metal - Black Inner Panel", "Regency Fireplace - Clearance", "<Unnamed>", "Regency Fireplace - Glass - Clear", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Wood - Birch Log Set Firebed") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1" | object type "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1" | names: "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1:313097" | material: materials ("Regency Fireplace - Metal - Silver", "Regency Fireplace - Metal - Black Inner Panel", "Regency Fireplace - Clearance", "<Unnamed>", "Regency Fireplace - Glass - Clear", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Wood - Birch Log Set Firebed") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Construction
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill:Vent" | object type "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill:Vent" | names: "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill:Vent:407391", "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill:Vent:407570" | material: materials ("Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White"); "Regency Fireplace - Metal - White" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction, Dimensions
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill:Vent" | object type "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill:Vent" | names: "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill:Vent:409375", "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill:Vent:411633" | material: materials ("Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White"); "Regency Fireplace - Metal - White" | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction, Dimensions

Types
  IFCWALLTYPE "Basic Wall:Generic - 30"" | STANDARD | 4 occurrences | material: layers "Basic Wall:Generic - 30"" ("Default Wall" 21.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1" | 2 occurrences | material: materials ("Regency Fireplace - Metal - Silver", "Regency Fireplace - Metal - Black Inner Panel", "<Unnamed>", "Regency Fireplace - Glass - Clear", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Wood - Birch Log Set Firebed") | property sets: Constraints, Construction, Data, Dimensions, Electrical, Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1" | 1 occurrence | material: materials ("Regency Fireplace - Metal - Silver", "Regency Fireplace - Metal - Black Inner Panel", "Regency Fireplace - Clearance", "<Unnamed>", "Regency Fireplace - Glass - Clear", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Wood - Birch Log Set Firebed") | property sets: Constraints, Construction, Data, Dimensions, Electrical, Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E:CB50E-NG1" | 1 occurrence | material: materials ("Regency Fireplace - Metal - Silver", "Regency Fireplace - Metal - Black Inner Panel", "Regency Fireplace - Clearance", "<Unnamed>", "Regency Fireplace - Glass - Clear", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Metal - Black", "Regency Fireplace - Wood - Birch Log Set Firebed") | property sets: Constraints, Construction, Data, Dimensions, Electrical, Identity Data
  IFCAIRTERMINALTYPE "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill:Vent" | 2 occurrences | material: materials ("Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White") | property sets: Constraints, Identity Data, Materials and Finishes, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCAIRTERMINALTYPE "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill:Vent" | 2 occurrences | material: materials ("Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White", "Regency Fireplace - Metal - White") | property sets: Constraints, Identity Data, Materials and Finishes, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements

Property sets
  Pset_ProductRequirements | properties | on 5 objects (4 IFCBUILDINGELEMENTPROXY, 1 IFCOPENINGELEMENT) | on 3 type objects
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 4 objects (4 IFCFLOWTERMINAL) | on 2 type objects
    Category = "Air Terminals" (IFCLABEL)
  Pset_ProductRequirements | properties | on 4 objects (3 IFCWALL, 1 IFCWALLSTANDARDCASE) | on 1 type object
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCOPENINGELEMENT)
    Id = "312710" (IFCTEXT)
    UniqueId = "019d9c0c-4a5d-4091-9f17-29111c502ec0-0004c586" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCWALL)
    Id = "309091" (IFCTEXT)
    UniqueId = "019d9c0c-4a5d-4091-9f17-29111c502ec0-0004b763" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCWALL)
    Id = "309132" (IFCTEXT)
    UniqueId = "019d9c0c-4a5d-4091-9f17-29111c502ec0-0004b78c" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Id = "311077" (IFCTEXT)
    UniqueId = "019d9c0c-4a5d-4091-9f17-29111c502ec0-0004bf25" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Id = "311207" (IFCTEXT)
    UniqueId = "019d9c0c-4a5d-4091-9f17-29111c502ec0-0004bfa7" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Id = "312580" (IFCTEXT)
    UniqueId = "019d9c0c-4a5d-4091-9f17-29111c502ec0-0004c504" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCWALL)
    Id = "313008" (IFCTEXT)
    UniqueId = "019d9c0c-4a5d-4091-9f17-29111c502ec0-0004c6b0" (IFCTEXT)
  Identity Data: 9 more contents on 6 objects not shown
  Other | properties | on 4 objects (3 IFCWALL, 1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall" (IFCLABEL)
    Family and Type = "Basic Wall: Generic - 30"" (IFCLABEL)
    Type = "Generic - 30"" (IFCLABEL)
    Type Id = "249" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E" (IFCLABEL)
    Family and Type = "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E: CB50E-NG1" (IFCLABEL)
    Front side = TRUE (IFCBOOLEAN)
    Left corner = FALSE (IFCBOOLEAN)
    Left offset = 39.251968503937 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Left panel = FALSE (IFCBOOLEAN)
    Left side = FALSE (IFCBOOLEAN)
    Nom Chase enclosure height = 62.992125984251963 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Nom Option = 1 (IFCINTEGER)
    Nom Side option = 1 (IFCINTEGER)
    Nom Vent offset = 2. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Option 1 = FALSE (IFCBOOLEAN)
    Option 2 = FALSE (IFCBOOLEAN)
    Option 3 = FALSE (IFCBOOLEAN)
    Right corner = FALSE (IFCBOOLEAN)
    Right offset = 39.251968503937 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Right panel = FALSE (IFCBOOLEAN)
    Right side = FALSE (IFCBOOLEAN)
    Type = "CB50E-NG1" (IFCLABEL)
    Type Id = "420461" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCOPENINGELEMENT)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E" (IFCLABEL)
    Family and Type = "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E: CB50E-NG1" (IFCLABEL)
    Front side = TRUE (IFCBOOLEAN)
    Left corner = FALSE (IFCBOOLEAN)
    Left offset = 39.251968503937 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Left panel = FALSE (IFCBOOLEAN)
    Left side = FALSE (IFCBOOLEAN)
    Nom Chase enclosure height = 62.992125984251963 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Nom Option = 1 (IFCINTEGER)
    Nom Side option = 1 (IFCINTEGER)
    Nom Vent offset = 2. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Option 1 = TRUE (IFCBOOLEAN)
    Option 2 = FALSE (IFCBOOLEAN)
    Option 3 = FALSE (IFCBOOLEAN)
    Right corner = FALSE (IFCBOOLEAN)
    Right offset = 39.251968503937 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Right panel = FALSE (IFCBOOLEAN)
    Right side = FALSE (IFCBOOLEAN)
    Type = "CB50E-NG1" (IFCLABEL)
    Type Id = "420461" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCFLOWTERMINAL)
    Category = "Air Terminals" (IFCLABEL)
    Family = "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill" (IFCLABEL)
    Family and Type = "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill: Vent" (IFCLABEL)
    N = 3 (IFCINTEGER)
    Type = "Vent" (IFCLABEL)
    Type Id = "413413" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCFLOWTERMINAL)
    Category = "Air Terminals" (IFCLABEL)
    Family = "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill" (IFCLABEL)
    Family and Type = "Fire-Products_Fire-Protection_Regency-Fireplace_Ventilation-Grill: Vent" (IFCLABEL)
    N = 13 (IFCINTEGER)
    Type = "Vent" (IFCLABEL)
    Type Id = "413413" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E" (IFCLABEL)
    Family and Type = "HVAC_Fireplaces_Regency-Fireplace_San-Francisco-gas-fireplace_CB50E: CB50E-NG1" (IFCLABEL)
    Front side = TRUE (IFCBOOLEAN)
    Left corner = FALSE (IFCBOOLEAN)
    Left offset = 39.251968503937 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Left panel = FALSE (IFCBOOLEAN)
    Left side = FALSE (IFCBOOLEAN)
    Nom Chase enclosure height = 62.992125984251963 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Nom Option = 2 (IFCINTEGER)
    Nom Side option = 1 (IFCINTEGER)
    Nom Vent offset = 2. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Option 1 = FALSE (IFCBOOLEAN)
    Option 2 = TRUE (IFCBOOLEAN)
    Option 3 = TRUE (IFCBOOLEAN)
    Right corner = FALSE (IFCBOOLEAN)
    Right offset = 39.251968503937 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Right panel = FALSE (IFCBOOLEAN)
    Right side = FALSE (IFCBOOLEAN)
    Type = "CB50E-NG1" (IFCLABEL)
    Type Id = "420461" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: 1/4" Head" (IFCLABEL)
    Type = "1/4" Head" (IFCLABEL)
    Type Id = "27" (IFCLABEL)
  Other: 3 more contents on 0 objects not shown
  Constraints | properties | on 5 objects (4 IFCBUILDINGELEMENTPROXY, 1 IFCOPENINGELEMENT)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Host = "Basic Wall : Generic - 30"" (IFCTEXT)
    Level = "Level 1" (IFCLABEL)
    Schedule Level = "Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCWALL)
    Base Constraint = "Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Base Offset = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Top Offset = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 62.992125984253519 (IFCLENGTHMEASURE) [INCH (conversion based)]
  Constraints | properties | on 1 object (1 IFCWALL)
    Base Constraint = "Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Base Offset = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Top Offset = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 62.992125984250968 (IFCLENGTHMEASURE) [INCH (conversion based)]
  Constraints | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Base Constraint = "Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Base Offset = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Top Offset = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 69.960460426344142 (IFCLENGTHMEASURE) [INCH (conversion based)]
  Constraints | properties | on 1 object (1 IFCWALL)
    Base Constraint = "Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Base Offset = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Top Offset = 0. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 74.316870034447817 (IFCLENGTHMEASURE) [INCH (conversion based)]
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Elevation from Level = 62.992125984250968 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Host = "Basic Wall : Generic - 30"" (IFCTEXT)
    Level = "Level 1" (IFCLABEL)
    Schedule Level = "Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Elevation from Level = 59.688976377952741 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Host = "Basic Wall : Generic - 30"" (IFCTEXT)
    Level = "Level 1" (IFCLABEL)
    Schedule Level = "Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Elevation from Level = 56.188976377952635 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Host = "Basic Wall : Generic - 30"" (IFCTEXT)
    Level = "Level 1" (IFCLABEL)
    Schedule Level = "Level 1" (IFCLABEL)
  Constraints: 4 more contents on 2 objects not shown
  Cross-Section Definition | properties | on 4 objects (3 IFCWALL, 1 IFCWALLSTANDARDCASE)
    Cross-Section = "Vertical" (IFCIDENTIFIER)
  Dimensions | properties | on 3 objects (2 IFCBUILDINGELEMENTPROXY, 1 IFCOPENINGELEMENT)
    Area = 134.90671398613122 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 59.558384566091057 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Area = 134.90671398613122 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 13.31662541590498 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 2 objects (2 IFCFLOWTERMINAL)
    Area = 18.11151411824283 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Height = 2.9999999999999996 (IFCLENGTHMEASURE) [INCH (conversion based)]
    L = 49.599999999999994 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Length = 49.999999999999993 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Size = "" (IFCTEXT)
    Volume = 0.029929533193128494 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 2 objects (2 IFCFLOWTERMINAL)
    Area = 10.313629649506195 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Height = 10. (IFCLENGTHMEASURE) [INCH (conversion based)]
    L = 14.6 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Length = 15. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Size = "" (IFCTEXT)
    Volume = 0.020925970625818774 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 26.684164479440717 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 60.999999999999979 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Volume = 20.341029744560295 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 26.684164479439652 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 61.000000000000021 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Volume = 16.840253962624903 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 23.805990006186551 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 48.999999999999986 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Volume = 20.280602656159118 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 44.899775645812468 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 87.000000000000412 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Volume = 49.385158600464763 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions: 2 more contents on 1 objects not shown
  Phasing | properties | on 13 objects (4 IFCBUILDINGELEMENTPROXY, 4 IFCFLOWTERMINAL, 3 IFCWALL, 1 IFCOPENINGELEMENT)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 4 objects (3 IFCWALL, 1 IFCWALLSTANDARDCASE)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (4 IFCBUILDINGELEMENTPROXY, 1 IFCOPENINGELEMENT)
    Reference = "CB50E-NG1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (3 IFCWALL, 1 IFCWALLSTANDARDCASE)
    Reference = "Generic - 30"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCFLOWTERMINAL)
    Reference = "Vent" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (3 IFCWALL, 1 IFCWALLSTANDARDCASE)
    Reference = "Generic - 30"" (IFCLABEL)
  Pset_WallCommon | properties | on 4 objects (3 IFCWALL, 1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Generic - 30"" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "CB50E-NG1" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Depth = 20.944881889763774 (IFCPOSITIVELENGTHMEASURE) [INCH (conversion based)]
    Height = 37.007874015748023 (IFCPOSITIVELENGTHMEASURE) [INCH (conversion based)]
    Width = 5. (IFCPOSITIVELENGTHMEASURE) [INCH (conversion based)]
  Pset_ProvisionForVoid | properties | on 3 type objects
    Depth = 20.944881889763774 (IFCPOSITIVELENGTHMEASURE) [INCH (conversion based)]
    Height = 37.007874015748023 (IFCPOSITIVELENGTHMEASURE) [INCH (conversion based)]
    Width = 59.999999999999993 (IFCPOSITIVELENGTHMEASURE) [INCH (conversion based)]
  Construction | properties | on 4 objects (4 IFCFLOWTERMINAL)
    Installation clearance = FALSE (IFCBOOLEAN)
  Construction | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Chase enclosure height = 62.992125984251963 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Corner Installation Kit = FALSE (IFCBOOLEAN)
    Corner Installation Kit note = "Corner conversion liner panel is installed only in corner fireplaces on glass" (IFCTEXT)
    Heat Wave Installation = FALSE (IFCBOOLEAN)
    Installation clearance = FALSE (IFCBOOLEAN)
    Installation options (ventilation openings) = 1 (IFCINTEGER)
    Installation options note = "Option 1 - Floor to ceiling with top opening" (IFCTEXT)
    Side option = 1 (IFCINTEGER)
    Side option note = "Front side" (IFCTEXT)
    Vent offset = 2.9999999999999996 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Vent offset note = "Only works with installation option 2, changes from 0″ to 2″" (IFCTEXT)
  Construction | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCOPENINGELEMENT)
    Chase enclosure height = 62.992125984251963 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Corner Installation Kit = FALSE (IFCBOOLEAN)
    Corner Installation Kit note = "Corner conversion liner panel is installed only in corner fireplaces on glass" (IFCTEXT)
    Heat Wave Installation = FALSE (IFCBOOLEAN)
    Installation clearance = TRUE (IFCBOOLEAN)
    Installation options (ventilation openings) = 1 (IFCINTEGER)
    Installation options note = "Option 1 - Floor to ceiling with top opening" (IFCTEXT)
    Side option = 1 (IFCINTEGER)
    Side option note = "Front side" (IFCTEXT)
    Vent offset = 2.9999999999999996 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Vent offset note = "Only works with installation option 2, changes from 0″ to 2″" (IFCTEXT)
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Chase enclosure height = 62.992125984251963 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Corner Installation Kit = FALSE (IFCBOOLEAN)
    Corner Installation Kit note = "Corner conversion liner panel is installed only in corner fireplaces on glass" (IFCTEXT)
    Heat Wave Installation = FALSE (IFCBOOLEAN)
    Installation clearance = TRUE (IFCBOOLEAN)
    Installation options (ventilation openings) = 2 (IFCINTEGER)
    Installation options note = "Option 2 - Low framing with vents in front/2 sides or top" (IFCTEXT)
    Side option = 1 (IFCINTEGER)
    Side option note = "Front side" (IFCTEXT)
    Vent offset = 2.9999999999999996 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Vent offset note = "Only works with installation option 2, changes from 0″ to 2″" (IFCTEXT)
  Construction | properties | on 3 type objects
    WIFI Dongle Installation = TRUE (IFCBOOLEAN)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 21. (IFCLENGTHMEASURE) [INCH (conversion based)]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Electrical - Loads | properties | on 5 objects (4 IFCBUILDINGELEMENTPROXY, 1 IFCOPENINGELEMENT)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Materials and Finishes | properties | on 5 objects (4 IFCBUILDINGELEMENTPROXY, 1 IFCOPENINGELEMENT)
    Firebed Material = "Regency Fireplace - Wood - Birch Log Set Firebed" (IFCLABEL)
    Inner Panel Material = "Regency Fireplace - Metal - Black Inner Panel" (IFCLABEL)
  Materials and Finishes | properties | on 3 type objects
    Housing Material = "Regency Fireplace - Metal - Black" (IFCLABEL)
  Materials and Finishes | properties | on 2 type objects
    Housing Material = "Regency Fireplace - Metal - White" (IFCLABEL)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "CB50E-NG1" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 4 objects (4 IFCFLOWTERMINAL)
    Reference = "Vent" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Grid Line 1/2"" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "1/4" Head" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.10000000000000001 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
  Graphics | properties | on 1 type object
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Pset_ElementShading | properties | on 1 type object
    Roughness = 11.999999999999998 (IFCPOSITIVELENGTHMEASURE) [INCH (conversion based)]
  Data | properties | on 3 type objects
    CSA P.4.1 = "57.49%" (IFCTEXT)
    Fuel Type = "Natural Gas" (IFCTEXT)
    Manifold Pressure - High = "3.8” W.C. (0.94 kPa)" (IFCTEXT)
    Manifold Pressure - Low = "1.1” W.C. (0.27 kPa)" (IFCTEXT)
    Maximum Input Altitude 0-4500 ft. (0-1372m) = "35,000 Btu/h (11.42 kW)" (IFCTEXT)
    Minimum Input Altitude 0-4500 ft. (0-1372m) = "19,000Btu/h (6.15 kW)" (IFCTEXT)
    Minimum Supply Pressure = "5” W.C. (1.25 kPa)" (IFCTEXT)
    Orifce Size -Altitude 0-4500 ft = "# 36 DMS" (IFCTEXT)
  Electrical | properties | on 3 type objects
    Apparent Load = 0. (IFCPOWERMEASURE) [WATT]
    Current = 1.5 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Frequency = 60. (IFCFREQUENCYMEASURE) [HERTZ]
    Number of Poles = 1 (IFCINTEGER)
    Power Consumption = 0. (IFCPOWERMEASURE) [WATT]
    Power Factor = 1. (IFCREAL)
    Voltage = 120. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Mechanical | properties | on 3 type objects
    Duct Connector Description = "5” Inner /8” Outer" (IFCTEXT)
    Duct Diameter = 3.9999999999999991 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Gas Connector Description = "Natural gas supply" (IFCTEXT)
    Gas flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Pipe Diameter = 0.49999999999999989 (IFCLENGTHMEASURE) [INCH (conversion based)]
    Ventilation flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Pset_ManufacturerTypeInformation | properties | on 5 type objects
    Manufacturer = "Regency Fireplace" (IFCLABEL)