IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2026-05-18T14:51:23-05:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "23.0.11.19 - Exporter 23.0.11.19 - Default UI"
Application: "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)" | change NOCHANGE | created 1673537642 (2023-01-12T15:34:02Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window_NewConstruction_SH_Vinyl_Harvey:18210" | object type "Window_NewConstruction_SH_Vinyl_Harvey:18210" | names: "Window_NewConstruction_SH_Vinyl_Harvey:18210:109154" | material: materials ("Screen", "Aluminum", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Glass - Laminated - Clear", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Glass - Laminated - Clear", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Constraints, Construction, Dimensions

Types
  IFCWINDOWSTYLE "Window_NewConstruction_SH_Vinyl_Harvey:18210" | 1 occurrence | material: materials ("Screen", "Aluminum", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Glass - Laminated - Clear", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Glass - Laminated - Clear", "ARCAT - Vinyl - PVC - 0.070" - White", "ARCAT - Vinyl - PVC - 0.070" - White") | property sets: Window_NewConstruction_SH_Vinyl_Harvey:18210:109154, Analytical Model, Analytical Properties, Construction, Dimensions, Identity Data

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCWINDOW) | on 1 type object
    Category = "Windows" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
    Family = "Window_NewConstruction_SH_Vinyl_Harvey" (IFCLABEL)
    Family and Type = "Window_NewConstruction_SH_Vinyl_Harvey: 18210" (IFCLABEL)
    Head Height = 1.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "109153" (IFCLABEL)
    Type = "18210" (IFCLABEL)
    Type Id = "109135" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Windows" (IFCLABEL)
    Family Name = "Window_NewConstruction_SH_Vinyl_Harvey" (IFCTEXT)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWINDOW)
    Reference = "18210" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "18210" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCWINDOW)
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCWINDOW)
    Casing_908 = FALSE (IFCBOOLEAN)
    Casing_Flat = FALSE (IFCBOOLEAN)
    Extension Jamb = FALSE (IFCBOOLEAN)
    Simulated Divided Lites = FALSE (IFCBOOLEAN)
  Construction | properties | on 1 type object
    RO Spacing = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Wall Closure = "By host" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCWINDOW)
    Area = 22.740464713930134 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Extension Jamb Depth = 0.38020833333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Mullion Width = 0.052083333333333336 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Sill Height = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.47103672360622978 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Glass Thickness = 0.072916666666666671 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 1.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 1.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 1.791666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 1.791666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Energy Analysis | properties | on 1 object (1 IFCWINDOW)
    R_Value = 0. (IFCREAL)
    SHGC = 0. (IFCREAL)
    U_Factor = 0. (IFCREAL)
  Identity Data | properties | on 1 object (1 IFCWINDOW)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2020100" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    CAD Details = "https://www.arcat.com/company/harvey-building-products-32985/cad" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc. 2023" (IFCTEXT)
    Description = "Harvey BP - 18210 Vinyl Single Hung Window" (IFCTEXT)
    DrawnBy = "Robert S. Weygant. CSI, CDT, SCIP" (IFCTEXT)
    Keynote = "08 53 13" (IFCTEXT)
    Manufacturer = "Harvey Building Products" (IFCTEXT)
    Model = "18210" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Product Page URL = "https://www.arcat.com/arcatcos/cos32/arc32985.html" (IFCTEXT)
    Type Mark = "77" (IFCTEXT)
    Type Name = "18210" (IFCTEXT)
    URL = "https://harveywindows.com/" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCWINDOW)
    Extension Jamb Material = "ARCAT - Vinyl - PVC - 0.070" - White" (IFCLABEL)
    Glass = "Glazed Sash : Glass w/ Diamond Muntins" (IFCLABEL)
    MuntinMatl = "ARCAT - Vinyl - PVC - 0.070" - White" (IFCLABEL)
    Screen = "Screen" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Frame Material = "ARCAT - Vinyl - PVC - 0.070" - White" (IFCLABEL)
    Glass Type = "ARCAT - Glass - Laminated - Clear" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCWINDOW)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Window_NewConstruction_SH_Vinyl_Harvey:18210:109154 | predefined | on 1 type object
  Analytical Model | properties | on 1 type object
    AAMA Conformance = "H-R50 (DP50)" (IFCTEXT)
    E283_Air-Infiltration = "0.05 cfm/sq. ft. at 1.57 psf" (IFCTEXT)
    E330_Structural-Test-Pressure = "45.14 psf positive and negative" (IFCTEXT)
    E547_Water-Resistance = "No leakage at 4.60 psf" (IFCTEXT)
    F588_Forced-Entry = "Type B; Grade 10" (IFCTEXT)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Text | properties | on 1 type object
    Specification = "https://www.arcat.com/company/harvey-building-products-32985/spec" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "Harvey Building Products" (IFCLABEL)