IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-01-13T13:53:02"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Bleacher-Telescopic-Hussey-MAXAM-Wall_Attached:26" Row, 16" Rise" | object type "Bleacher-Telescopic-Hussey-MAXAM-Wall_Attached:26" Row, 16" Rise" | names: "Bleacher-Telescopic-Hussey-MAXAM-Wall_Attached:26" Row, 16" Rise:168352" | material: materials ("Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction

Types
  IFCBUILDINGELEMENTPROXYTYPE "Bleacher-Telescopic-Hussey-MAXAM-Wall_Attached:26" Row, 16" Rise" | 1 occurrence | material: materials ("Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color") | property sets: Constraints, Construction, Dimensions, Identity Data, Materials and Finishes, Other

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Bleacher-Telescopic-Hussey-MAXAM-Wall_Attached" (IFCLABEL)
    Family and Type = "Bleacher-Telescopic-Hussey-MAXAM-Wall_Attached: 26" Row, 16" Rise" (IFCLABEL)
    Front Closure Height = 0.99479166666666674 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Front Row Height = 1.328125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Type = "26" Row, 16" Rise" (IFCLABEL)
    Type Id = "168309" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
    Family Name = "Bleacher-Telescopic-Hussey-MAXAM-Wall_Attached" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "26" Row, 16" Rise" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Hussey Seating Company" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "26" Row, 16" Rise" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "Basic Wall : Wall 1" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Number of Operable End Rails = 2 (IFCINTEGER)
    Number of Operable Tiers = 3 (IFCINTEGER)
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Row Spacing Graphic Dimension = 2.1666666666666665 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Row Rise Constraint = 3 (IFCINTEGER)
    Row Rise Note = "Do Not Change Row Rise Constraint" (IFCTEXT)
    Row Spacing Constraint = 4 (IFCINTEGER)
    Row Spacing Note = "Do Not Change Row Spacing Constraint" (IFCTEXT)
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Estimated Seat Count = 24 (IFCINTEGER)
    Number of Tiers = 4 (IFCINTEGER)
    Tier Limitation Chart = "Contact Hussey Seating Company" (IFCTEXT)
  Construction | properties | on 1 type object
    Courtside XC12 Note = "Not available for 22'' Row Spacing" (IFCTEXT)
    Seat Type = "Bleacher Seat : Courtside XC10" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 450.72950791839122 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Bank Length = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Closed Dimension = 3.333333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Open Dimension = 7.484375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Unit Depth = 7.484375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Unit Height = 5.875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Top Deck Height = 5.333333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 17.178531704545996 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Row Rise = 1.3333333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Row Spacing = 2.1666666666666665 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Show End Rails Left = TRUE (IFCBOOLEAN)
    Show End Rails Right = TRUE (IFCBOOLEAN)
    Show in Open Position = TRUE (IFCBOOLEAN)
    Show in Stowed Position = FALSE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Seat Color = "Hussey - 301 Blue" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Bleacher Deck Material = "Hussey - Plywood - 001 Natural - Bleacher Decking" (IFCLABEL)
    End Rail Color = "Hussey - Bleacher Rail Color" (IFCLABEL)
    Front Closure Material = "Hussey - Galvanized Steel" (IFCLABEL)
    Nose Beam Material = "Hussey - Galvanized Steel" (IFCLABEL)
    Riser Material = "Hussey - Galvanized Steel" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "E1020900" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BIM Version = "v3.1" (IFCTEXT)
    CSI MasterFormat = "12 66 00" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright Notice = "© Hussey Seating Co. All Rights Reserved." (IFCTEXT)
    Created By = "Revitus" (IFCTEXT)
    Creator URL = "http://www.revituspro.com/" (IFCTEXT)
    Description = "MAXAM Telescopic Gym Bleacher Bank - Wall Attached" (IFCTEXT)
    Manufacturer = "Hussey Seating Company" (IFCTEXT)
    Manufacturer Address 1 = "38 Dyer Street Extension" (IFCTEXT)
    Manufacturer Address 2 = "North Berwick, Maine 03906" (IFCTEXT)
    Manufacturer Email Contact = "mailto:revit@husseyseating.com?Subject=Revit Inquiry" (IFCTEXT)
    Manufacturer Phone Number = "1.800.341.0401" (IFCTEXT)
    Model = "MAXAM" (IFCTEXT)
    OmniClass Number = "23.40.50.34.14" (IFCTEXT)
    OmniClass Title = "Gymnasium Equipment" (IFCTEXT)
    Product Page URL = "http://www.husseyseating.com/maxam-gym-bleachers/" (IFCTEXT)
    Type Comments = "Bleacher Bank" (IFCTEXT)
    Type Name = "26" Row, 16" Rise" (IFCTEXT)
    URL = "http://www.husseyseating.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Text | properties | on 1 type object
    Bank Length Increment = "18'' Typical Increments" (IFCTEXT)
    Bank Length Maximum = "25'-6''" (IFCTEXT)
    Bank Length Minimum = "9'-0''" (IFCTEXT)