IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-01-13T14:03:50"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Bleacher_Aisle-Telescopic-Hussey-MAXAM_Plus-Wall_Attached-Simplified:33" Row, 16" Rise" | object type "Bleacher_Aisle-Telescopic-Hussey-MAXAM_Plus-Wall_Attached-Simplified:33" Row, 16" Rise" | names: "Bleacher_Aisle-Telescopic-Hussey-MAXAM_Plus-Wall_Attached-Simplified:33" Row, 16" Rise:424254" | material: materials ("Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction

Types
  IFCBUILDINGELEMENTPROXYTYPE "Bleacher_Aisle-Telescopic-Hussey-MAXAM_Plus-Wall_Attached-Simplified:33" Row, 16" Rise" | 1 occurrence | material: materials ("Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Rail Color", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip", "Hussey - Bleacher Step - Abrasive Strip") | property sets: Constraints, Construction, Dimensions, Identity Data, Materials and Finishes, Other

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Bleacher_Aisle-Telescopic-Hussey-MAXAM_Plus-Wall_Attached-Simplified" (IFCLABEL)
    Family and Type = "Bleacher_Aisle-Telescopic-Hussey-MAXAM_Plus-Wall_Attached-Simplified: 33" Row, 16" Rise" (IFCLABEL)
    Front Closure Height = 0.99479166666666674 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Front Row Height = 1.328125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Front Step Height = 0.65364583333333337 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Multiple Handrails = FALSE (IFCBOOLEAN)
    Single Handrail = TRUE (IFCBOOLEAN)
    Type = "33" Row, 16" Rise" (IFCLABEL)
    Type Id = "424211" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
    Family Name = "Bleacher_Aisle-Telescopic-Hussey-MAXAM_Plus-Wall_Attached-Simplified" (IFCTEXT)
    Front Step Depth = 1.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "33" Row, 16" Rise" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Hussey Seating Company" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "33" Row, 16" Rise" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Actual Chair Array Width = 1.75 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Armrest Visibility = TRUE (IFCBOOLEAN)
    Calculated Chair Array Width = 3.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Calculated Chair Array Width Maximum = 2.75 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Calculated Number of Seats per Row = 3 (IFCINTEGER)
    Cup Holder Visibility = TRUE (IFCBOOLEAN)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Handrail Array Value = 2 (IFCINTEGER)
    Host = "Basic Wall : Wall 1" (IFCTEXT)
    Metro Chair Top Deck Height = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Number of Handrails = 1 (IFCINTEGER)
    Number of Intermediate Steps = 2 (IFCINTEGER)
    Number of Operable End Rails = 2 (IFCINTEGER)
    Number of Operable Tiers = 3 (IFCINTEGER)
    Number of Seats per Row = 2 (IFCINTEGER)
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Row Spacing Graphic Dimension = 2.7526041666666661 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Not Metro Chair = FALSE (IFCBOOLEAN)
    Row Rise Constraint = 3 (IFCINTEGER)
    Row Rise Note = "Do Not Change Row Rise Constraint" (IFCTEXT)
    Row Spacing Constraint = 3 (IFCINTEGER)
    Row Spacing Note = "Do Not Change Row Spacing Constraint" (IFCTEXT)
    Scheduled Seat Width = 1.75 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Estimated Seat Count = 2 (IFCINTEGER)
    Number of Tiers = 4 (IFCINTEGER)
    Tier Limitation Chart = "Contact Hussey Seating Company" (IFCTEXT)
  Construction | properties | on 1 type object
    Metro Chair = TRUE (IFCBOOLEAN)
    Seat Type = "Bleacher Seat : Metro Chair" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 211.34046397126258 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Bank Length = 4.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Closed Dimension = 4.083333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Open Dimension = 9.234375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Unit Depth = 9.234375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Unit Height = 5.875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Top Deck Height = 5.333333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 15.903254894006954 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Row Rise = 1.3333333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Row Spacing = 2.75 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Seat Width = 1.75 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Step Depth = 1.375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Step Height = 0.66666666666666663 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Seat Down = TRUE (IFCBOOLEAN)
    Show Arms = TRUE (IFCBOOLEAN)
    Show Cup Holders = TRUE (IFCBOOLEAN)
    Show End Rails Left = TRUE (IFCBOOLEAN)
    Show End Rails Right = FALSE (IFCBOOLEAN)
    Show Front Aisle Step = TRUE (IFCBOOLEAN)
    Show in Open Position = TRUE (IFCBOOLEAN)
    Show in Stowed Position = FALSE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Seat Color = "Hussey - 301 Blue" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Aisle Step Material = "Hussey - Bleacher Step" (IFCLABEL)
    Bleacher Deck Material = "Hussey - Plywood - 001 Natural - Bleacher Decking" (IFCLABEL)
    End Rail Color = "Hussey - Bleacher Rail Color" (IFCLABEL)
    Front Closure Material = "Hussey - Galvanized Steel" (IFCLABEL)
    Handrail Color = "Hussey - Bleacher Rail Color" (IFCLABEL)
    Nose Beam Material = "Hussey - Galvanized Steel" (IFCLABEL)
    Riser Material = "Hussey - Galvanized Steel" (IFCLABEL)
    Stanchion Color = "Hussey - 301 Blue" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "E1020900" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BIM Version = "v3.1" (IFCTEXT)
    CSI MasterFormat = "12 66 00" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright Notice = "© Hussey Seating Co. All Rights Reserved." (IFCTEXT)
    Created By = "Revitus" (IFCTEXT)
    Creator URL = "http://www.revituspro.com/" (IFCTEXT)
    Description = "MAXAM Plus Telescopic Gym Bleacher Aisle - Wall Attached" (IFCTEXT)
    Manufacturer = "Hussey Seating Company" (IFCTEXT)
    Manufacturer Address 1 = "38 Dyer Street Extension" (IFCTEXT)
    Manufacturer Address 2 = "North Berwick, Maine 03906" (IFCTEXT)
    Manufacturer Email Contact = "mailto:revit@husseyseating.com?Subject=Revit Inquiry" (IFCTEXT)
    Manufacturer Phone Number = "1.800.341.0401" (IFCTEXT)
    Model = "MAXAM Plus" (IFCTEXT)
    OmniClass Number = "23.40.50.34.14" (IFCTEXT)
    OmniClass Title = "Gymnasium Equipment" (IFCTEXT)
    Product Page URL = "http://www.husseyseating.com/maxam-telescopic-platform/" (IFCTEXT)
    Type Comments = "Bleacher Aisle Unit" (IFCTEXT)
    Type Name = "33" Row, 16" Rise" (IFCTEXT)
    URL = "http://www.husseyseating.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Text | properties | on 1 type object
    Aisle Width Note = "Locked at 4'-6''" (IFCTEXT)
    Metro Chair Arms Note = "Not Available with 18'' Width" (IFCTEXT)
    Metro Chair Standard Widths = "18'', 19'', 20'', 21'', 22''" (IFCTEXT)