IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-01-13T14:25:28"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 6 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MXP-Hussey-Portable-Metro:36" Row Spacing" | object type "MXP-Hussey-Portable-Metro:36" Row Spacing" | names: "MXP-Hussey-Portable-Metro:36" Row Spacing:906941" | material: materials ("Hussey - End Rail Color", "Hussey - Powder Coat - 983 Black", "Hussey - Decking - AlumaDeck - 005 Aluminum", "Hussey - Galvanized Steel", "Hussey - Polymer - 301 Blue", "<Unnamed>", "Hussey - Powder Coat - 301 Blue") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "End_Rail-Hussey-Removable:Removable End Rail" | object type "End_Rail-Hussey-Removable:Removable End Rail" | names: "End_Rail-Hussey-Removable:Removable End Rail:907047", "End_Rail-Hussey-Removable:Removable End Rail:907048", "End_Rail-Hussey-Removable:Removable End Rail:907049" (+1 more) | material: materials ("Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - Bleacher Rail Color"); materials ("Hussey - End Rail Color", "Hussey - Bleacher Rail Color") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "End_Rail-Hussey-Removable:Removable End Rail" | object type "End_Rail-Hussey-Removable:Removable End Rail" | names: "End_Rail-Hussey-Removable:Removable End Rail:907051" | material: materials ("Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - Bleacher Rail Color") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "MXP-Hussey-Portable-Metro:36" Row Spacing" | 1 occurrence | material: materials ("Hussey - End Rail Color", "Hussey - Powder Coat - 983 Black", "Hussey - Decking - AlumaDeck - 005 Aluminum", "Hussey - Galvanized Steel") | property sets: Constraints, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "End_Rail-Hussey-Removable:Removable End Rail" | 4 occurrences | material: materials ("Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - Bleacher Rail Color") | property sets: Constraints, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "End_Rail-Hussey-Removable:Removable End Rail" | 1 occurrence | material: materials ("Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - End Rail Color", "Hussey - Bleacher Rail Color") | property sets: Constraints, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements

Property sets
  Pset_ProductRequirements | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Baluster Height = 3.1458333333333335 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Baluster Spacing = 0.33333333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "End_Rail-Hussey-Removable" (IFCLABEL)
    Family and Type = "End_Rail-Hussey-Removable: Removable End Rail" (IFCLABEL)
    Multiple Balusters = TRUE (IFCBOOLEAN)
    Number of Balusters = 8 (IFCINTEGER)
    Single Baluster = FALSE (IFCBOOLEAN)
    Type = "Removable End Rail" (IFCLABEL)
    Type Id = "717386" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Actual Chair Array Width = 6.6666666666666661 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Armrest Visibility = TRUE (IFCBOOLEAN)
    Calculated Chair Array Width = 6.6666666666666661 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Calculated Chair Array Width Maximum = 7. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Calculated Number of Seats per Row = 5 (IFCINTEGER)
    Category = "Specialty Equipment" (IFCLABEL)
    Cup Holder Visibility = FALSE (IFCBOOLEAN)
    End Rail Attachment Height = 0.95833333333333326 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    End Rail Length = 2.8958333333333335 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    End Rail Length Top Tier = 3.9687500000000004 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Family = "MXP-Hussey-Portable-Metro" (IFCLABEL)
    Family and Type = "MXP-Hussey-Portable-Metro: 36" Row Spacing" (IFCLABEL)
    Front Closure Height = 0.6875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Front Rail Bay Dimension = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Front Rail Bay Maximum Dimension = 3.3333333333333335 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Front Rail Width = 2.8333333333333335 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Front Row Height = 1.0208333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Not Truncated Section = TRUE (IFCBOOLEAN)
    Not Truncated and Open or Show in Stowed Position = TRUE (IFCBOOLEAN)
    Number of Front Rail Bays = 4 (IFCINTEGER)
    Number of Front Rails = 3 (IFCINTEGER)
    Number of Non-Truncated End Rails = 2 (IFCINTEGER)
    Number of Non-Truncated Tiers = 2 (IFCINTEGER)
    Number of Operable End Rails = 4 (IFCINTEGER)
    Number of Operable Tiers = 4 (IFCINTEGER)
    Number of Rear Rails = 3 (IFCINTEGER)
    Number of Seats per Row = 5 (IFCINTEGER)
    Number of Truncated Tiers Graphical = 2 (IFCINTEGER)
    Rear Rail Width = 2.8333333333333335 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Row Spacing Graphic Dimension = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Seats Folded Flat Visibility = FALSE (IFCBOOLEAN)
    Seats Upright Visibility = TRUE (IFCBOOLEAN)
    Show End Rail Left and Non-Truncated = FALSE (IFCBOOLEAN)
    Show End Rail Left and Non-Truncated and Open = FALSE (IFCBOOLEAN)
    Show End Rail Left and Truncated = FALSE (IFCBOOLEAN)
    Show End Rail Left and Truncated and Open = FALSE (IFCBOOLEAN)
    Show End Rail Right and Non-Truncated = TRUE (IFCBOOLEAN)
    Show End Rail Right and Non-Truncated and Open = TRUE (IFCBOOLEAN)
    Show End Rail Right and Truncated = FALSE (IFCBOOLEAN)
    Show End Rail Right and Truncated and Open = FALSE (IFCBOOLEAN)
    Show Truncated Section and Open = FALSE (IFCBOOLEAN)
    Truncated Front Rail Elevation = 2.520833333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Truncated Unit Depth = 10.072916666666668 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Type = "36" Row Spacing" (IFCLABEL)
    Type Id = "906749" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Baluster Height = 3.1458333333333335 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Baluster Spacing = 0.33333333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "End_Rail-Hussey-Removable" (IFCLABEL)
    Family and Type = "End_Rail-Hussey-Removable: Removable End Rail" (IFCLABEL)
    Multiple Balusters = TRUE (IFCBOOLEAN)
    Number of Balusters = 11 (IFCINTEGER)
    Single Baluster = FALSE (IFCBOOLEAN)
    Type = "Removable End Rail" (IFCLABEL)
    Type Id = "717386" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 2 type objects
    Category = "Specialty Equipment" (IFCLABEL)
    Family Name = "End_Rail-Hussey-Removable" (IFCTEXT)
  Other | properties | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
    Family Name = "MXP-Hussey-Portable-Metro" (IFCTEXT)
    Not Metro Chair = FALSE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "Removable End Rail" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "36" Row Spacing" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Manufacturer = "Hussey Seating Company" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "Removable End Rail" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "36" Row Spacing" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Scheduled Seat Width = 1.6666666666666665 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 3.2708333333332291 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 3.2708333333332291 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 2.5208333333332327 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 2.5208333333332327 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 1.7708333333332469 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 1.7708333333332469 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 1.020833333333254 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 1.020833333333254 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 4.0208333333333197 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 4.0208333333333197 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 2 type objects
    Default Elevation = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints: 1 more content on 0 objects not shown
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Estimated Seat Count = 25 (IFCINTEGER)
    Number of Tiers = 5 (IFCINTEGER)
    Number of Tiers Truncated = 2 (IFCINTEGER)
    Number of Truncated Tiers Note = "Number of Tiers Truncated must be at least 2; and also must be at least 3 less than Number of Tiers for Revit Family to work" (IFCTEXT)
    Tier Limitation Chart = "Contact Hussey Seating Company" (IFCTEXT)
  Construction | properties | on 1 type object
    Metro Chair = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Area = 4.9502153364838151 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Depth = 2.8958333333333335 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    End Rail Attachment Height = 0.95833333333333326 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 3.6458333333333335 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Row Rise = 0.75 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.22215101451527727 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 3833.043473295415 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Bank Length = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Bank Length Maximum = "20'-0'' - Verify with Hussey Seating Company" (IFCTEXT)
    Bank Length Minimum = "5'-2'' - Verify with Hussey Seating Company" (IFCTEXT)
    Closed Dimension = 4.213541666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Open Dimension = 16.072916666666668 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Unit Depth = 16.072916666666668 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Unit Height = 4.020833333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Row Rise = 0.75 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Row Rise Note = "9'' to 24'' in 1/2'' Increments for High Rise" (IFCTEXT)
    Seat Width = 1.6666666666666665 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Seat Width Standard Sizes Metro = "18'', 19'', 20'', 21'', 22''" (IFCTEXT)
    Tapered Angle 11.25 = TRUE (IFCBOOLEAN)
    Tapered Angle 22.5 = FALSE (IFCBOOLEAN)
    Top Deck Height = 4.020833333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Top Tier Depth = 4.072916666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 322.63364842164583 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 6.0794512420458728 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Depth = 3.9687500000000004 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    End Rail Attachment Height = 0.95833333333333326 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 3.6458333333333335 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Row Rise = 0.75 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.26295811961585669 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Row Spacing = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Row Spacing Note = "32'', 33'', 34'', 35'' or 36''" (IFCTEXT)
  Electrical - Loads | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Graphics | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Show Attachment Bracket = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Seat Down = FALSE (IFCBOOLEAN)
    Seat Up = TRUE (IFCBOOLEAN)
    Seats Folded Flat = FALSE (IFCBOOLEAN)
    Seats Upright = TRUE (IFCBOOLEAN)
    Show Arms = TRUE (IFCBOOLEAN)
    Show Cup Holders = FALSE (IFCBOOLEAN)
    Show End Rails Left = FALSE (IFCBOOLEAN)
    Show End Rails Right = TRUE (IFCBOOLEAN)
    Show Tapered End = TRUE (IFCBOOLEAN)
    Show Top Row Seating = TRUE (IFCBOOLEAN)
    Show Truncated Section = FALSE (IFCBOOLEAN)
    Show in Open Position = TRUE (IFCBOOLEAN)
    Show in Stowed Position = FALSE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Show Attachment Bracket = FALSE (IFCBOOLEAN)
  Materials and Finishes | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    End Rail Color = "Hussey - End Rail Color" (IFCLABEL)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Armrest Finish = "Hussey - Polymer - 301 Blue" (IFCLABEL)
    Seat Back Finish = "Hussey - Polymer - 301 Blue" (IFCLABEL)
    Seat Bottom Cover Finish = "Hussey - Polymer - 301 Blue" (IFCLABEL)
    Stanchion Finish = "Hussey - Powder Coat - 301 Blue" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Deck Material = "Hussey - Decking - AlumaDeck - 005 Aluminum" (IFCLABEL)
    End Rail Color = "Hussey - End Rail Color" (IFCLABEL)
    Front Closure Material = "Hussey - Powder Coat - 983 Black" (IFCLABEL)
    Nose Beam Material = "Hussey - Galvanized Steel" (IFCLABEL)
    Riser Material = "Hussey - Powder Coat - 983 Black" (IFCLABEL)
  Phasing | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Metro Chair Arms Note = "Not Available with 18'' Width" (IFCTEXT)
  Pset_ProvisionForVoid | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Depth = 2.8958333333333335 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Height = 3.6458333333333335 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 3.9687500000000004 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Height = 3.6458333333333335 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 2 type objects
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BIM Version = "v2.1" (IFCTEXT)
    BIM Version Available (Earliest) = "2012" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright Notice = "© Hussey Seating Co. All Rights Reserved." (IFCTEXT)
    Created By = "Revitus" (IFCTEXT)
    Creator URL = "http://www.revituspro.com/" (IFCTEXT)
    Description = "Removable End Rail" (IFCTEXT)
    Manufacturer = "Hussey Seating Company" (IFCTEXT)
    Manufacturer Address 1 = "38 Dyer Street Extension" (IFCTEXT)
    Manufacturer Address 2 = "North Berwick, Maine 03906" (IFCTEXT)
    Manufacturer Email Contact = "mailto:revit@husseyseating.com?Subject=Revit Inquiry" (IFCTEXT)
    Manufacturer Phone Number = "1.800.341.0401" (IFCTEXT)
    Model = "Removable End Rail" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "Removable End Rail" (IFCTEXT)
    URL = "http://www.husseyseating.com/" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "E1020900" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BIM Version = "v3.1" (IFCTEXT)
    BIM Version Available (Earliest) = "2017" (IFCTEXT)
    CSI MasterFormat = "12 66 00" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright Notice = "© Hussey Seating Co. All Rights Reserved." (IFCTEXT)
    Created By = "Revitus" (IFCTEXT)
    Creator URL = "http://www.revituspro.com/" (IFCTEXT)
    Description = "MXP Telescopic Platform with Metro Chairs and Tapered End Option - Portable" (IFCTEXT)
    MXP Literature Downloads = "http://www.husseyseating.com/mxp-literature/" (IFCTEXT)
    Manufacturer = "Hussey Seating Company" (IFCTEXT)
    Manufacturer Address 1 = "38 Dyer Street Extension" (IFCTEXT)
    Manufacturer Address 2 = "North Berwick, Maine 03906" (IFCTEXT)
    Manufacturer Email Contact = "mailto:revit@husseyseating.com?Subject=Revit Inquiry" (IFCTEXT)
    Manufacturer Phone Number = "1.800.341.0401" (IFCTEXT)
    Model = "MXP" (IFCTEXT)
    OmniClass Number = "23.40.50.34.14" (IFCTEXT)
    OmniClass Title = "Gymnasium Equipment" (IFCTEXT)
    Product Page URL = "http://www.husseyseating.com/mxp-overview/" (IFCTEXT)
    Type Comments = "Telescopic Platform" (IFCTEXT)
    Type Name = "36" Row Spacing" (IFCTEXT)
    URL = "http://www.husseyseating.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)