IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2023-01-30T10:06:09"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Basketball-Structure_Wall-Mount_Side-Fold_PKGxxSFRG:PKG82STRG" | object type "Basketball-Structure_Wall-Mount_Side-Fold_PKGxxSFRG:PKG82STRG" | names: "Basketball-Structure_Wall-Mount_Side-Fold_PKGxxSFRG:PKG82STRG:97499" | material: materials ("Finish - IPI by Bison - White Netting", "Powder Coat - Playground Orange", "Powder Coat - Playground Orange", "Powder Coat - Playground Orange", "Powder Coat - Playground Orange", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Fiberglass - Backboard", "Powder Coat - White", "Powder Coat - White", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "Basketball-Structure_Wall-Mount_Side-Fold_PKGxxSFRG:PKG82STRG" | 1 occurrence | material: materials ("Finish - IPI by Bison - White Netting", "Powder Coat - Playground Orange", "Powder Coat - Playground Orange", "Powder Coat - Playground Orange", "Powder Coat - Playground Orange", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support", "Fiberglass - Backboard", "Powder Coat - White", "Powder Coat - White", "Steel - Tubular Support", "Steel - Tubular Support", "Steel - Tubular Support") | property sets: Analytical Model, Constraints, Construction, Dimensions, Identity Data, Materials and Finishes

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Basketball-Structure_Wall-Mount_Side-Fold_PKGxxSFRG" (IFCLABEL)
    Family and Type = "Basketball-Structure_Wall-Mount_Side-Fold_PKGxxSFRG: PKG82STRG" (IFCLABEL)
    Type = "PKG82STRG" (IFCLABEL)
    Type Id = "97474" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Basketball-Structure_Wall-Mount_Side-Fold_PKGxxSFRG" (IFCTEXT)
    Manufacturer Address = "603 L St. Lincoln, NE 68508" (IFCTEXT)
    Manufacturer Fax = "888-438-5312" (IFCTEXT)
    Manufacturer Phone - Toll Free = "888-438-5311" (IFCTEXT)
    Manufacturer Phone = "888-438-5311" (IFCTEXT)
    Manufacturer Website = "http://www.ipibybison.com/" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "PKG82STRG" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "IPI by Bison" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "PKG82STRG" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Width = 5.9999999999999929 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "Basic Wall : Wall 1" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mounting Height = 8. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 type object
    Extension Depth = 8. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    PKG46STRG Extension Range = "48" to 72"" (IFCTEXT)
    PKG68STRG Extension Range = "72" to 96"" (IFCTEXT)
    PKG82STRG Extension Range = "96" to 144"" (IFCTEXT)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 60.858553441118985 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 5.8028091046239796 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Backboard Height = 3.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Support Tubing Diameter = 0.1583333333333341 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Category = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc." (IFCTEXT)
    Description = "IPI by Bison Gymnasium Equipment" (IFCTEXT)
    Drawn By = "Sumex Design, Inc. / Robert S. Weygant, CSI, CDT, SCIP" (IFCTEXT)
    Keynote = "11 66 00" (IFCTEXT)
    Manufacturer = "IPI by Bison" (IFCTEXT)
    Model = "As Specified" (IFCTEXT)
    OmniClass Number = "23.40.50.34.24" (IFCTEXT)
    OmniClass Title = "Nets" (IFCTEXT)
    Revision = "R1_2018-09" (IFCTEXT)
    Type Name = "PKG82STRG" (IFCTEXT)
    URL = "https://ipibybison.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Analytical Model | properties | on 1 type object
    Suspension Type = "Telescoping" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Backboard Frame Material = "Steel - Tubular Support" (IFCLABEL)
    Backboard Material = "Fiberglass - Backboard" (IFCLABEL)
    Hoop Finish = "Powder Coat - Playground Orange" (IFCLABEL)
    Netting = "Finish - IPI by Bison - White Netting" (IFCLABEL)
    Support Tubing Material = "Steel - Tubular Support" (IFCLABEL)
    Wall Plate Material = "Wood" (IFCLABEL)
  Text | properties | on 1 type object
    Building Codes = "https://www.brpbybison.com/submittals.html" (IFCTEXT)
    Construction Details = "https://www.arcat.com/downloads/38554-brpbis/bim/bison/BRP%20by%20bison" (IFCTEXT)
    Green Building-LEED = "https://www.arcat.com/green/green_building.shtml" (IFCTEXT)
    Installation-Fabrication = "http://www.ipibybison.com/InstallersPage.php" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos38/arc38554.html" (IFCTEXT)
    Sales Information = "http://www.ipibybison.com/DealersPage.php" (IFCTEXT)
    Specification = "https://www.arcat.com/arcatcos/cos49/arc49571.html" (IFCTEXT)
    Test Data = "http://www.ipibybison.com/ToolBox.php" (IFCTEXT)