IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-01-09T13:37:29"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Skyroofs_Kalwall_Pre-Engineered-SSRR-Hip-Ends:Shoji 12" x 24"" | object type "Skyroofs_Kalwall_Pre-Engineered-SSRR-Hip-Ends:Shoji 12" x 24"" | names: "Skyroofs_Kalwall_Pre-Engineered-SSRR-Hip-Ends:Shoji 12" x 24":177811" | material: materials ("Kalwall - KCRF - Aluminum 79", "Kalwall - FRP - Crystal", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79") | property sets: Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Constraints, Construction

Types
  IFCWINDOWSTYLE "Skyroofs_Kalwall_Pre-Engineered-SSRR-Hip-Ends:Shoji 12" x 24"" | 1 occurrence | material: materials ("Kalwall - KCRF - Aluminum 79", "Kalwall - FRP - Crystal", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79", "Kalwall - KCRF - Aluminum 79") | property sets: Skyroofs_Kalwall_Pre-Engineered-SSRR-Hip-Ends:Shoji 12" x 24":177811, Analytical Properties, Constraints, Identity Data, Other, Pset_ManufacturerTypeInformation

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCWINDOW) | on 1 type object
    Category = "Windows" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWINDOW)
    20 deg = FALSE (IFCBOOLEAN)
    27 deg = TRUE (IFCBOOLEAN)
    33 deg = FALSE (IFCBOOLEAN)
    45 deg = FALSE (IFCBOOLEAN)
    5' module = FALSE (IFCBOOLEAN)
    Category = "Windows" (IFCLABEL)
    CenterSection = 4.0625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Curb Bottom Offset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Curb Visibility Real = TRUE (IFCBOOLEAN)
    Custom Module = FALSE (IFCBOOLEAN)
    Endwall Length = 2.3057441468582596 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Family = "Skyroofs_Kalwall_Pre-Engineered-SSRR-Hip-Ends" (IFCLABEL)
    Family and Type = "Skyroofs_Kalwall_Pre-Engineered-SSRR-Hip-Ends: Shoji 12" x 24"" (IFCLABEL)
    Hip End Height = 4.5930872902059177 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Hip End Pos = 4.0537483827457965 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    MainHeight = 4.5930872902059177 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberofCenterSections = 1 (IFCINTEGER)
    Outside Curb Length Real = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Outside Curb Width Real = 8. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    OutsidePanel = 12.0625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Section Width = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Sweep Pos = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Top Pos = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Type = "Shoji 12" x 24"" (IFCLABEL)
    Type Id = "177777" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Windows" (IFCLABEL)
    Family Name = "Skyroofs_Kalwall_Pre-Engineered-SSRR-Hip-Ends" (IFCTEXT)
    Shoji 10" x 24" = FALSE (IFCBOOLEAN)
    Shoji 12" x 24" = TRUE (IFCBOOLEAN)
    Shoji 8" x 20" = FALSE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCWINDOW) | on 1 type object
    Manufacturer = "Kalwall" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWINDOW)
    Reference = "Shoji 12" x 24"" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Shoji 12" x 24"" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCWINDOW)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "Basic Wall : Wall 1" (IFCTEXT)
    Limits Note = "Kalwall Revit Models are meant for preliminary design and layout. Always consult with the Kalwall factory to ensure systems are engineered to project-specific design requirements." (IFCTEXT)
    Max Custom Panel Width = 5. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Outside Curb Width = 15. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Min Curb Thickness = 0.45833333333333337 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Min Custom Panel Width = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Min Outside Curb Length = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Min Outside Curb Width = 8. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Slope = 27.250000000000004 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCWINDOW)
    Panel = "4' Panel Width" (IFCTEXT)
    Panel Type Selection = 1 (IFCINTEGER)
    Slope Selection = 1 (IFCINTEGER)
  Dimensions | properties | on 1 object (1 IFCWINDOW)
    Actual Curb Thickness = 0.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Actual Outside Curb Length = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Actual Outside Curb Width = 8. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Actual Panel Width = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Area = 336.16701417377055 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Curb Height = 1. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Curb Thickness = 0.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Desired Custom Panel Width = 3.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Desired Outside Curb Length = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Desired Outside Curb Width = 8. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 3.2380358135249261 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Height Dimension = 3.1215485154281435 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 11. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 7. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 47.851178334678579 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
    Width = 8. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCWINDOW)
    Mark = "7" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Date Created = "2024/02/16" (IFCTEXT)
    Date Updated = "" (IFCTEXT)
    Description = "Flat or curved, these systems span up to 24', offering the ultimate in energy-efficient diffuse daylighting." (IFCTEXT)
    Manufacturer = "Kalwall" (IFCTEXT)
    Model = "Pre-engineered skyroof with Hip Ends" (IFCTEXT)
    OmniClass Number = "23.25.20.14.27.17" (IFCTEXT)
    OmniClass Title = "Translucent Roof Assemblies" (IFCTEXT)
    Product Documentation Link = "https://www.kalwall.com/resources/?resource_type=cad-details" (IFCTEXT)
    Product Page URL = "https://www.kalwall.com/products/skyroofs/pre-engineered-skyroofs/" (IFCTEXT)
    Product data url = "https://bimobject.com/kalwall/product/skyroofs-pre-engineered-ssrr" (IFCTEXT)
    Type Mark = "15" (IFCTEXT)
    Type Name = "Shoji 12" x 24"" (IFCTEXT)
    URL = "https://www.kalwall.com/" (IFCTEXT)
    Version = 1 (IFCINTEGER)
  Materials and Finishes | properties | on 1 object (1 IFCWINDOW)
    Curb Material = "Default Wall" (IFCLABEL)
    Exterior Face Sheet Material = "Kalwall - FRP - Crystal" (IFCLABEL)
    Interior Face Sheet Material = "Kalwall - FRP - White" (IFCLABEL)
    System Finish = "Kalwall - KCRF - Aluminum 79" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCWINDOW)
    Phase Created = "New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCWINDOW)
    Curb Visibility = TRUE (IFCBOOLEAN)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Skyroofs_Kalwall_Pre-Engineered-SSRR-Hip-Ends:Shoji 12" x 24":177811 | predefined | on 1 type object
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)