IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-12-03T13:51:03-05:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "23.0.11.19 - Exporter 23.0.11.19 - Default UI"
Application: "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)" | change NOCHANGE | created 1673537642 (2023-01-12T15:34:02Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCELECTRICAPPLIANCETYPE "Data_Device-Network-Leviton-QuickPort-Angled_Faceplate-4_Port:4-Port Universal Angled Faceplate, Color Black" | object type "Data_Device-Network-Leviton-QuickPort-Angled_Faceplate-4_Port:4-Port Universal Angled Faceplate, Color Black" | names: "Data_Device-Network-Leviton-QuickPort-Angled_Faceplate-4_Port:4-Port Universal Angled Faceplate, Color Black:101790" | material: materials ("Snap Locations - Leviton - Invisible", "Snap Locations - Leviton - Invisible", "Snap Locations - Leviton - Invisible", "Snap Locations - Leviton - Invisible", "Steel-Generic-Galvanized", "Plastic - Leviton - Black", "Clearance Areas - Leviton") | property sets: Pset_DistributionFlowElementCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Data, Dimensions

Types
  IFCELECTRICAPPLIANCETYPE "Data_Device-Network-Leviton-QuickPort-Angled_Faceplate-4_Port:4-Port Universal Angled Faceplate, Color Black" | 1 occurrence | material: materials ("Snap Locations - Leviton - Invisible", "Snap Locations - Leviton - Invisible", "Snap Locations - Leviton - Invisible", "Snap Locations - Leviton - Invisible", "Steel-Generic-Galvanized", "Plastic - Leviton - Black", "Clearance Areas - Leviton") | property sets: Constraints, Data, Dimensions, General, Graphics, Identity Data

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCFLOWTERMINAL) | on 1 type object
    Category = "Data Devices" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Data Devices" (IFCLABEL)
    Family = "Data_Device-Network-Leviton-QuickPort-Angled_Faceplate-4_Port" (IFCLABEL)
    Family and Type = "Data_Device-Network-Leviton-QuickPort-Angled_Faceplate-4_Port: 4-Port Universal Angled Faceplate, Color Black" (IFCLABEL)
    Type = "4-Port Universal Angled Faceplate, Color Black" (IFCLABEL)
    Type Id = "101765" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Data Devices" (IFCLABEL)
    Family Name = "Data_Device-Network-Leviton-QuickPort-Angled_Faceplate-4_Port" (IFCTEXT)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "4-Port Universal Angled Faceplate, Color Black" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "4-Port Universal Angled Faceplate, Color Black" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "Basic Wall : Wall 1" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 2. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    z Offset 1 = 0.01666666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Channel Count = 0 (IFCINTEGER)
    Channel ID = "" (IFCTEXT)
    Port ID = "" (IFCTEXT)
  Data | properties | on 1 type object
    Fiber Type = "" (IFCTEXT)
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.2755375085820202 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 0.0021229869174370945 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Depth = 0.13291666666666668 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 0.20166666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.34116666666666673 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCFLOWTERMINAL)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCFLOWTERMINAL)
    Annotation Symbol = "Symbol : Data" (IFCLABEL)
    Annotation Symbol is Visible = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 type object
    Cable Clearance Rear is Visible = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "1" (IFCTEXT)
    Part Number = "49910-UE4" (IFCTEXT)
    Serial Number = "" (IFCTEXT)
    UPC Code = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "D5030600" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "Copyright © 2013-2014 Leviton Manufacturing Co., Inc." (IFCTEXT)
    Date Last Modified = "October 04, 2023" (IFCTEXT)
    Description = "Universal 4-Port Angled Modular Furniture Faceplate with Labeling Designation Window, black" (IFCTEXT)
    Equipment Abbreviation = "QPA" (IFCTEXT)
    Equipment Type = "" (IFCTEXT)
    Family Version = "1.0.0" (IFCTEXT)
    Manufacturer = "Leviton" (IFCTEXT)
    Model = "" (IFCTEXT)
    Model Disclaimer = "http://www.leviton.com/BIMTERMS" (IFCTEXT)
    OmniClass Number = "23.85.50.17" (IFCTEXT)
    OmniClass Title = "Communication and Data Processing Equipment" (IFCTEXT)
    Original Creation Date = "October 04, 2023" (IFCTEXT)
    Part Description = "Universal 4-Port Angled Modular Furniture Faceplate with Labeling Designation Window, black" (IFCTEXT)
    Product Documentation Link = "https://www.leviton.com/en/docs/Leviton_Spec_49910-UE4_Universal_4-Port_Angled_Modular_Furniture_Faceplate.pdf" (IFCTEXT)
    Technical Support Phone Number = "1-800-824-3005" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "4-Port Universal Angled Faceplate, Color Black" (IFCTEXT)
    URL = "http://www.leviton.com/networksolutions" (IFCTEXT)
  Model Properties | properties | on 1 object (1 IFCFLOWTERMINAL)
    Weight = 0. (IFCFORCEMEASURE) [NEWTON]
  Model Properties | properties | on 1 type object
    Has ID Windows = TRUE (IFCBOOLEAN)
    Shielded = FALSE (IFCBOOLEAN)
  Phasing | properties | on 1 object (1 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  General | properties | on 1 type object
    Minimum Order Quantity = 0 (IFCINTEGER)
    Quantity per Package = 0 (IFCINTEGER)
  Materials and Finishes | properties | on 1 type object
    Faceplate Material = "Plastic - Leviton - Black" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "Leviton" (IFCLABEL)