IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2026-02-25T15:01:55-05:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "23.0.11.19 - Exporter 23.0.11.19 - Default UI"
Application: "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)" | change NOCHANGE | created 1673537642 (2023-01-12T15:34:02Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Partition_Lami_CeilingHung_Metpar:ADA Alcove - Last Common - Bottom at 1" AFF" | object type "Partition_Lami_CeilingHung_Metpar:ADA Alcove - Last Common - Bottom at 1" AFF" | names: "Partition_Lami_CeilingHung_Metpar:ADA Alcove - Last Common - Bottom at 1" AFF:103128" | material: materials ("Laminate - Finish as Specified", "Laminate - Finish as Specified", "Aluminum", "Laminate - Finish as Specified", "Laminate - Finish as Specified", "Aluminum") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction, Dimensions, Graphics

Types
  IFCFURNITURETYPE "Partition_Lami_CeilingHung_Metpar:ADA Alcove - Last Common - Bottom at 1" AFF" | 1 occurrence | material: materials ("Laminate - Finish as Specified", "Laminate - Finish as Specified", "Aluminum", "Laminate - Finish as Specified", "Laminate - Finish as Specified", "Aluminum") | property sets: Constraints, Construction, Dimensions, Graphics, Identity Data, Other

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCFURNISHINGELEMENT) | on 1 type object
    Category = "Casework" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    Category = "Casework" (IFCLABEL)
    Family = "Partition_Lami_CeilingHung_Metpar" (IFCLABEL)
    Family and Type = "Partition_Lami_CeilingHung_Metpar: ADA Alcove - Last Common - Bottom at 1" AFF" (IFCLABEL)
    Type = "ADA Alcove - Last Common - Bottom at 1" AFF" (IFCLABEL)
    Type Id = "103112" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Casework" (IFCLABEL)
    Family Name = "Partition_Lami_CeilingHung_Metpar" (IFCTEXT)
    Manufacturer Address = "95 State St. Westbury, NY 11590" (IFCTEXT)
    Manufacturer Fax = "516-333-2618" (IFCTEXT)
    Manufacturer Phone - Toll Free = "888-METPAR-1" (IFCTEXT)
    Manufacturer Phone = "516-333-2600" (IFCTEXT)
    Manufacturer Website = "http://www.metpar.com/" (IFCTEXT)
    Send Message = "http://www.arcat.com/users.pl?action=UserEmail&company=Metpar%20Corp.&coid=34179&rep=111&fax=516-333-2618&mf=" (IFCTEXT)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    Reference = "ADA Alcove - Last Common - Bottom at 1" AFF" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "Basic Wall : Wall 1" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    GapHng = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    GapStrk = 0.11979166666666666 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    HngPilast2 = 0.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    HngPnlOffset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    StrkPilast2 = 0.29166666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    StrkPnlOffset = 0.25520833333333337 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    offset = 0.47916666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    Ceiling Support Location = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Cross Bracing Location = 1.5240885416666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Wall Extension Length = 2.3958333333333335 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 type object
    Ceiling Height = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Handle Height = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Thickness = 0.072916666666666671 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Thickness = 0.072916666666666671 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pilaster Thickness = 0.10416666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    Area = 80.362872594856327 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Door Width = 1.9947916666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pilaster Height = 8.9166666666666661 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Depth = 5. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 5.6754294121093487 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Door Height = 4.5833333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Height = 4.5833333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Height from Floor = 0.083333333333333343 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pilaster Width_Hinge Side = 1. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pilaster Width_Strike Side = 0.58333333333333337 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Width = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Graphics | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    Has Cross Bracing = FALSE (IFCBOOLEAN)
    Inswing = TRUE (IFCBOOLEAN)
    Outswing = FALSE (IFCBOOLEAN)
    Show Structural Ceiling Support = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 type object
    Has Door = TRUE (IFCBOOLEAN)
    Has Wall extension = FALSE (IFCBOOLEAN)
    Hinge Pilaster = TRUE (IFCBOOLEAN)
    Hinge Side Panel = FALSE (IFCBOOLEAN)
    Offset Hinge Panel = FALSE (IFCBOOLEAN)
    Offset Strike Panel = TRUE (IFCBOOLEAN)
    Strike Pilaster = TRUE (IFCBOOLEAN)
    Strike Side Panel = TRUE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    Bracket Type = "" (IFCTEXT)
    Hardware Finish = "Aluminum" (IFCLABEL)
    Hinge = "[Nylon Cam][Stainless Steel Multi-Cam]" (IFCTEXT)
    Material = "Laminate - Finish as Specified" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "C1010400" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "2011, ARCAT, Inc" (IFCTEXT)
    Description = "Metpar Laminate CH700E Ceiling Hung Toilet Compartment" (IFCTEXT)
    Drawn By = "Robert S. Weygant, CSI, CDT, SCIP" (IFCTEXT)
    Keynote = "10 21 00" (IFCTEXT)
    Manufacturer = "Metpar Corp." (IFCTEXT)
    Model = "CH700E" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Revision = "R1_04-2011" (IFCTEXT)
    Type Comments = "Contact Manufacturer for More Information" (IFCTEXT)
    Type Name = "ADA Alcove - Last Common - Bottom at 1" AFF" (IFCTEXT)
    URL = "http://www.metpar.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Text | properties | on 1 type object
    Building Codes = "http://www.metpar.com/restroomPartitionsSpecifications.asp" (IFCTEXT)
    Construction Details = "http://www.arcat.com/details/metparco/metparco.html?coid=34179" (IFCTEXT)
    Green Building-LEED = "http://www.arcat.com/green/clients/leed_data_34179.html" (IFCTEXT)
    Installation-Fabrication = "http://www.metpar.com/insthelp.asp" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos34/arc34179.html" (IFCTEXT)
    Product Properties = "http://www.arcat.com/bim/bim_info.pl?fn=Metpar" (IFCTEXT)
    Sales Information = "http://www.metpar.com/distributors.asp" (IFCTEXT)
    Specification = "http://www.arcat.com/sdspecs/htm/10155met.htm" (IFCTEXT)
    Test Data = "http://www.metpar.com/firerating.asp" (IFCTEXT)
  Pset_FurnitureTypeCommon | properties | on 1 type object
    Description = "Metpar Laminate CH700E Ceiling Hung Toilet Compartment" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "Metpar Corp." (IFCLABEL)