IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2024-12-13T10:58:10"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "OmegaFlex-TracPipe-Stub_Out-Meter:1-1/4" x 12"" | object type "OmegaFlex-TracPipe-Stub_Out-Meter:1-1/4" x 12"" | names: "OmegaFlex-TracPipe-Stub_Out-Meter:1-1/4" x 12":118933" | material: materials ("Stainless Steel - OmegaFlex", "Stainless Steel - OmegaFlex") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCVALVETYPE "OmegaFlex-TracPipe-Stub_Out-Meter:1-1/4" x 12"" | 1 occurrence | material: materials ("Stainless Steel - OmegaFlex", "Stainless Steel - OmegaFlex") | property sets: Constraints, Construction, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCFLOWCONTROLLER) | on 1 type object
    Category = "Pipe Accessories" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Category = "Pipe Accessories" (IFCLABEL)
    Family = "OmegaFlex-TracPipe-Stub_Out-Meter" (IFCLABEL)
    Family and Type = "OmegaFlex-TracPipe-Stub_Out-Meter: 1-1/4" x 12"" (IFCLABEL)
    Type = "1-1/4" x 12"" (IFCLABEL)
    Type Id = "118918" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Pipe Accessories" (IFCLABEL)
    Family Name = "OmegaFlex-TracPipe-Stub_Out-Meter" (IFCTEXT)
    Lookup Table Name = "OmegaFlex-TracPipe-AutoFlare-Meter_Stub_Out" (IFCTEXT)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "1-1/4" x 12"" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER) | on 1 type object
    Manufacturer = "OmegaFlex" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "1-1/4" x 12"" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.57298592389617642 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Maximum Size = 0.10416666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Minimum Size = 0.10416666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Size = "" (IFCTEXT)
    Volume = 0.0055445223800645637 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Nominal Diameter 1 = 0.10416666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Nominal Radius 1 = 0.052083333333333343 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    TracPipe Diameter = 0.13834635416666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    TracPipe Inner Diameter = 0.11759440104166669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    TracPipe Length = 1. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "15" (IFCTEXT)
    Part Description = "Meter Term Stub-Out - 1-1/4" x 12"" (IFCTEXT)
    Part Number = "FGP-1-1/4X12MT" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "See Part Description" (IFCTEXT)
    Manufacturer = "OmegaFlex" (IFCTEXT)
    Model = "TracPipe CounterStrike" (IFCTEXT)
    OmniClass Number = "23.60.30.11.17" (IFCTEXT)
    OmniClass Title = "Pipework/Ductwork Mechanical Fasteners/Supports" (IFCTEXT)
    Type Name = "1-1/4" x 12"" (IFCTEXT)
    URL = "https://www.omegaflex.com/" (IFCTEXT)
  Insulation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Size = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Undefined" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Construction | properties | on 1 type object
    12" TracPipe = TRUE (IFCBOOLEAN)
    6" TracPipe = FALSE (IFCBOOLEAN)