IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2024-06-13T13:42:21"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.70.21 - Exporter 21.1.70.21 - Default UI"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1686682715 (2023-06-13T18:58:35Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCDOOR | type IFCDOORSTYLE "665_Counter_Btw_Jambs_Mtd_Overhead_Door:Wood Curtain with Wood Hood Manual" | object type "665_Counter_Btw_Jambs_Mtd_Overhead_Door:Wood Curtain with Wood Hood Manual" | names: "665_Counter_Btw_Jambs_Mtd_Overhead_Door:Wood Curtain with Wood Hood Manual:191331" | material: materials ("Wood - Red Oak", "Wood - White Oak", "Countertop") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints

Types
  IFCDOORSTYLE "665_Counter_Btw_Jambs_Mtd_Overhead_Door:Wood Curtain with Wood Hood Manual" | 1 occurrence | material: materials ("Wood - White Oak", "Wood - White Oak", "Wood - Red Oak", "Wood - Red Oak") | property sets: 665_Counter_Btw_Jambs_Mtd_Overhead_Door:Wood Curtain with Wood Hood Manual:191331, Analytical Properties, Constraints, Construction, Dimensions, Identity Data

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "665_Counter_Btw_Jambs_Mtd_Overhead_Door: Wood Curtain with Wood Hood Manual" (IFCLABEL)
    Family and Type = "665_Counter_Btw_Jambs_Mtd_Overhead_Door: Wood Curtain with Wood Hood Manual" (IFCLABEL)
    Head Height = 6.96875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "Basic Wall: Wall 1" (IFCLABEL)
    Type = "665_Counter_Btw_Jambs_Mtd_Overhead_Door: Wood Curtain with Wood Hood Manual" (IFCLABEL)
    Type Id = "665_Counter_Btw_Jambs_Mtd_Overhead_Door: Wood Curtain with Wood Hood Manual" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Doors" (IFCLABEL)
    Family Name = "665_Counter_Btw_Jambs_Mtd_Overhead_Door" (IFCTEXT)
  Pset_ConcreteElementGeneral | properties | on 1 object (1 IFCDOOR) | on 1 type object
    FireRating = "As Specified in 08 36 00" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR) | on 1 type object
    FireRating = "As Specified in 08 36 00" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Wood Curtain with Wood Hood Manual" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Manufacturer = "Overhead Door Corporation" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Reference = "Wood Curtain with Wood Hood Manual" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCDOOR)
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Door Gap From Wall Interior = 0.5875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Elevation From Level = 3.20833333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Left End Cap Thickness = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Right End Cap Thickness = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCDOOR)
    Area = 66.6049280246444 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 10.162886513245 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Height = 6.96875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Maximum Height = "8' 0" (IFCTEXT)
    Maximum Width = "12' 0" (IFCTEXT)
    Panel Height = 2.8671875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Width = 6.38541666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Thickness = 0.0416666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 6.91666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Mark = "17" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2030410" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    CAD Details = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "© 2024 ARCAT" (IFCTEXT)
    Description = "Overhead Door Model 665 Overhead Coiling Wood Counter Door" (IFCTEXT)
    Fire Rating = "As Specified in 08 36 00" (IFCTEXT)
    Keynote = "08 33 13" (IFCTEXT)
    Manufacturer = "Overhead Door Corporation" (IFCTEXT)
    Model = "665" (IFCTEXT)
    OmniClass Number = "23.30.10.17.27.11" (IFCTEXT)
    OmniClass Title = "Overhead Coiling" (IFCTEXT)
    Product Page URL = "" (IFCTEXT)
    Type Mark = "140" (IFCTEXT)
    Type Name = "Wood Curtain with Wood Hood Manual" (IFCTEXT)
    URL = "http://www.overheaddoor.com/" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCDOOR)
    Phase Created = "New Construction" (IFCLABEL)
  Text | properties | on 1 object (1 IFCDOOR)
    Parameter 005 = "" (IFCTEXT)
  Text | properties | on 1 type object
    Construction Details = "https://www.arcat.com/company/overhead-door-corporation-34626/cad" (IFCTEXT)
    Green Building-LEED = "https://www.arcat.com/company/overhead-door-corporation-34626/leed" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos34/arc34626.html" (IFCTEXT)
    SpecWizard = "https://www.arcat.com/company/overhead-door-corporation-34626/sw" (IFCTEXT)
    Specification = "https://www.arcat.com/company/overhead-door-corporation-34626/spec" (IFCTEXT)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  665_Counter_Btw_Jambs_Mtd_Overhead_Door:Wood Curtain with Wood Hood Manual:191331 | predefined | on 2 type objects
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Electrical Operator = FALSE (IFCBOOLEAN)
    Function = "Interior" (IFCIDENTIFIER)
    Has End Caps = TRUE (IFCBOOLEAN)
    Lock Type = "[Thumb Turn Locks] [Cylinder Locks]" (IFCTEXT)
    Manual Operation = TRUE (IFCBOOLEAN)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Materials and Finishes | properties | on 1 type object
    Door Track Material = "Wood - Red Oak" (IFCLABEL)
    Hood Material = "Wood - White Oak" (IFCLABEL)
    Operator Material = "Wood - Red Oak" (IFCLABEL)
    Panel Material = "Wood - White Oak" (IFCLABEL)