IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-06-13T09:41:37"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 13 elements
          7 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 3" ALUMINUM SLAT, TYP." | object type "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 3" ALUMINUM SLAT, TYP." | names: "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 3" ALUMINUM SLAT, TYP.:119018", "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 3" ALUMINUM SLAT, TYP.:119019", "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 3" ALUMINUM SLAT, TYP.:119020" (+4 more) | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 5" ALUMINUM SLAT, TYP." | object type "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 5" ALUMINUM SLAT, TYP." | names: "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 5" ALUMINUM SLAT, TYP.:119021", "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 5" ALUMINUM SLAT, TYP.:119022", "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 5" ALUMINUM SLAT, TYP.:119023" (+3 more) | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 3" ALUMINUM SLAT, TYP." | 7 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum:0.938" X 5" ALUMINUM SLAT, TYP." | 6 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements

Property sets
  Pset_ProductRequirements | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum" (IFCLABEL)
    Family and Type = "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum: 0.938" X 3" ALUMINUM SLAT, TYP." (IFCLABEL)
    Type = "0.938" X 3" ALUMINUM SLAT, TYP." (IFCLABEL)
    Type Id = "118868" (IFCLABEL)
  Other | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum" (IFCLABEL)
    Family and Type = "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum: 0.938" X 5" ALUMINUM SLAT, TYP." (IFCLABEL)
    Type = "0.938" X 5" ALUMINUM SLAT, TYP." (IFCLABEL)
    Type Id = "118841" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
    Constraints = 2 (IFCINTEGER)
    Family Name = "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum" (IFCTEXT)
  Other | properties | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
    Constraints = 1 (IFCINTEGER)
    Family Name = "Nested-Louvers-Palmshield-Mercury-Economic-Alternating-Semi_Private-Aluminum" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Reference = "0.938" X 3" ALUMINUM SLAT, TYP." (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Reference = "0.938" X 5" ALUMINUM SLAT, TYP." (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Manufacturer = "PalmSHIELD" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Reference = "0.938" X 3" ALUMINUM SLAT, TYP." (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Reference = "0.938" X 5" ALUMINUM SLAT, TYP." (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Depth = 4.3020833333333313 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.25 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Depth = 4.3020833333333313 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.41666666666666669 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 1 type object
    Width = 0.25 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 1 type object
    Width = 0.41666666666666669 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 2 type objects
    Default Elevation = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Area = 2.6795117421070507 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 4.302083333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.013938792180856058 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Area = 4.1152756137087509 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 4.302083333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.021407637276158211 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Thickness = 0.078125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Thickness = 0.078125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.41666666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Materials and Finishes | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY)
    Material = "Metal - PalmSHIELD - Grey Beige" (IFCLABEL)
  Model Properties | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY)
    Component Name = "Mercury Economic Alternating Semi Private - Aluminum - Louvers" (IFCTEXT)
    ID = "" (IFCTEXT)
  Phasing | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "F1020100" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "Copyright ©2024 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Mercury Economic Semi Private Alternating - Louvers" (IFCTEXT)
    Instruction Sheet Link = "https://palmshieldlouvers.com/wp-content/uploads/2021/09/PalmSHIELD-Mercury-Series-Post-Panel-Gate-Installation-Instructions-2.docx" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Mercury Economic Semi Private Alternating" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "https://palmshieldlouvers.com/wp-content/uploads/2022/01/Mercury-Economic-Alternating-Semi-Private.pdf" (IFCTEXT)
    Product Page URL = "https://palmshieldlouvers.com/products/mercury-screening/" (IFCTEXT)
    Type Name = "0.938" X 3" ALUMINUM SLAT, TYP." (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "F1020100" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "Copyright ©2024 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Mercury Economic Semi Private Alternating - Louvers" (IFCTEXT)
    Instruction Sheet Link = "https://palmshieldlouvers.com/wp-content/uploads/2021/09/PalmSHIELD-Mercury-Series-Post-Panel-Gate-Installation-Instructions-2.docx" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Mercury Economic Semi Private Alternating" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "https://palmshieldlouvers.com/wp-content/uploads/2022/01/Mercury-Economic-Alternating-Semi-Private.pdf" (IFCTEXT)
    Product Page URL = "https://palmshieldlouvers.com/products/mercury-screening/" (IFCTEXT)
    Type Name = "0.938" X 5" ALUMINUM SLAT, TYP." (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)