IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "RevitIdentifiers [ContentGUID: d11a4d4f-5557-44a8-afe0-33311cb8d256, VersionGUID: bd65ba44-603d-4446-9a64-8e75afe32294, NumberOfSaves: 109]"
File name: "Faux_Brick_Panel.ifc"
Time stamp: "2025-06-13T12:46:34-05:00"
Preprocessor: "ODA SDAI 24.12"
Originating system: "Autodesk Revit 25.3.0.46 (ENU) - IFC 25.3.0.46"
Application: "Autodesk Revit 2025 (ENU)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2025 (ENU)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ENU)" | change NOCHANGE | created 1720020883 (2024-07-03T15:34:43Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 5 elements
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested_Component-L_Frame-Palmshield-Faux_Brick:AL L3" X 3" X 1/4"" | object type "Nested_Component-L_Frame-Palmshield-Faux_Brick:AL L3" X 3" X 1/4"" | names: "Nested_Component-L_Frame-Palmshield-Faux_Brick:AL L3" X 3" X 1/4":208338", "Nested_Component-L_Frame-Palmshield-Faux_Brick:AL L3" X 3" X 1/4":208339" | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Model Properties, Constraints, Dimensions
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested_Component-L_Frame-Palmshield-Faux_Brick:AL L3" X 3" X 1/4"" | object type "Nested_Component-L_Frame-Palmshield-Faux_Brick:AL L3" X 3" X 1/4"" | names: "Nested_Component-L_Frame-Palmshield-Faux_Brick:AL L3" X 3" X 1/4":208340", "Nested_Component-L_Frame-Palmshield-Faux_Brick:AL L3" X 3" X 1/4":208341" | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Model Properties, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested_Component-Aluminum_Sheet-Palmshield-Faux_Brick:1/4" ALUMINUM SHEET" | object type "Nested_Component-Aluminum_Sheet-Palmshield-Faux_Brick:1/4" ALUMINUM SHEET" | names: "Nested_Component-Aluminum_Sheet-Palmshield-Faux_Brick:1/4" ALUMINUM SHEET:208342" | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Model Properties, Constraints, Dimensions

Types
  IFCBUILDINGELEMENTPROXYTYPE "Nested_Component-L_Frame-Palmshield-Faux_Brick:AL L3" X 3" X 1/4"" | 2 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Nested_Component-L_Frame-Palmshield-Faux_Brick:AL L3" X 3" X 1/4"" | 2 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Nested_Component-Aluminum_Sheet-Palmshield-Faux_Brick:1/4" ALUMINUM SHEET" | 1 occurrence | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation

Property sets
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "AL L3" X 3" X 1/4"" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "1/4" ALUMINUM SHEET" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "AL L3" X 3" X 1/4"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "1/4" ALUMINUM SHEET" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Other | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested_Component-L_Frame-Palmshield-Faux_Brick" (IFCLABEL)
    Family and Type = "Nested_Component-L_Frame-Palmshield-Faux_Brick: AL L3" X 3" X 1/4"" (IFCLABEL)
    Type = "AL L3" X 3" X 1/4"" (IFCLABEL)
    Type Id = "208191" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    C Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    C Frame Thickness = 0.020833333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Overall Panel Height = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Overall Panel Width = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested_Component-Aluminum_Sheet-Palmshield-Faux_Brick" (IFCLABEL)
    Family and Type = "Nested_Component-Aluminum_Sheet-Palmshield-Faux_Brick: 1/4" ALUMINUM SHEET" (IFCLABEL)
    Type = "1/4" ALUMINUM SHEET" (IFCLABEL)
    Type Id = "208232" (IFCLABEL)
  Other | properties | on 2 type objects
    C Hole Offset = 0.125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Family Name = "Nested_Component-L_Frame-Palmshield-Faux_Brick" (IFCTEXT)
  Other | properties | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
    Family Name = "Nested_Component-Aluminum_Sheet-Palmshield-Faux_Brick" (IFCTEXT)
  Constraints | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 3 type objects
    Default Elevation = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    A-Side Cut Angle = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Area = 1.9204936727630337 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    B-Side Cut Angle = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Length = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.038378139008219313 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    A-Side Cut Angle = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Area = 2.8269145920224359 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    B-Side Cut Angle = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Length = 5.8333333333333286 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.056604931399277809 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    A-Side Cut Angle = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Area = 2.8269145920224359 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    B-Side Cut Angle = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Length = 5.8333333333331385 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.056604931399277809 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 23.128472222222953 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Height = 5.7916666666666661 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.47761140046242906 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
    Width = 3.958333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 2 type objects
    Thickness = 0.020833333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Thickness = 0.020833333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 2 type objects
    Assembly Code = "F1020100" (IFCTEXT)
    Copyright = "Copyright ©2024 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Faux Brick - L Frame" (IFCTEXT)
    Instruction Sheet Link = "http://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Post-Panel-Gate-Installation-Instructions-REV-1.pdf" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Faux Brick" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "Contact Manufacturer for More Information" (IFCTEXT)
    Product Page URL = "https://palmshieldlouvers.com/products/brick-infill/" (IFCTEXT)
    Type Name = "AL L3" X 3" X 1/4"" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "F1020100" (IFCTEXT)
    Copyright = "Copyright ©2024 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Faux Brick - Aluminum Sheet" (IFCTEXT)
    Instruction Sheet Link = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Post-Panel-Gate-Installation-Instructions-REV-1.pdf" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Faux Brick" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "Contact Manufacturer for More Information" (IFCTEXT)
    Product Page URL = "https://palmshieldlouvers.com/products/brick-infill/" (IFCTEXT)
    Type Name = "1/4" ALUMINUM SHEET" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Model Properties | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Component Name = "Faux Brick - Aluminum - L Frame" (IFCTEXT)
    ID = "Not Assigned" (IFCTEXT)
  Model Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Component Name = "Faux Brick - Aluminum Sheet" (IFCTEXT)
  Materials and Finishes | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Material = "Metal - PalmSHIELD - Grey Beige" (IFCLABEL)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Material = "Metal - PalmSHIELD - Grey Beige" (IFCLABEL)
    Surface Finish = "Metal Finish - Palmshield - Faux Brick - Antique Select - Dark Red with Dark Grout" (IFCLABEL)
  Phasing | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 3 type objects
    Manufacturer = "PalmSHIELD" (IFCLABEL)