IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-06-13T12:10:53"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 67 elements
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl:6063 T6 ALUM 3" X 3" POSTS" | object type "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl:6063 T6 ALUM 3" X 3" POSTS" | names: "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl:6063 T6 ALUM 3" X 3" POSTS:135313", "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl:6063 T6 ALUM 3" X 3" POSTS:135316", "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl:6063 T6 ALUM 3" X 3" POSTS:135319" (+1 more) | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl:3" x 3" x 3/4"" | object type "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl:3" x 3" x 3/4"" | names: "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl:3" x 3" x 3/4":135314", "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl:3" x 3" x 3/4":135317", "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl:3" x 3" x 3/4":135320" (+1 more) | material: materials ("Metal - PalmSHIELD - Dusty Grey", "Metal - PalmSHIELD - Dusty Grey"); "Metal - PalmSHIELD - Dusty Grey" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl:8" x 8" x 1/2"" | object type "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl:8" x 8" x 1/2"" | names: "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl:8" x 8" x 1/2":135315", "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl:8" x 8" x 1/2":135318", "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl:8" x 8" x 1/2":135321" (+1 more) | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          30 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | object type "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | names: "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135322", "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135323", "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135324" (+27 more) | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | object type "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | names: "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135334", "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135343", "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135352" | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | object type "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | names: "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135335", "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135344", "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135353" | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL" | object type "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL" | names: "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL:135336", "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL:135345", "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL:135354" | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | object type "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | names: "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135363", "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135364", "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135365" (+7 more) | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL" | object type "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL" | names: "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL:135369" | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | object type "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | names: "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135370" | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | object type "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | names: "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL:135371" | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl:8" x 8" x 1/2"" | object type "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl:8" x 8" x 1/2"" | names: "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl:8" x 8" x 1/2":135372" | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl:3" x 3" x 3/4"" | object type "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl:3" x 3" x 3/4"" | names: "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl:3" x 3" x 3/4":135373" | material: materials ("Metal - PalmSHIELD - Dusty Grey", "Metal - PalmSHIELD - Dusty Grey") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl:6063 T6 ALUM 3" X 3" POSTS" | object type "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl:6063 T6 ALUM 3" X 3" POSTS" | names: "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl:6063 T6 ALUM 3" X 3" POSTS:135374" | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl:6063 T6 ALUM 3" X 3" POSTS" | 4 occurrences | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl:3" x 3" x 3/4"" | 4 occurrences | material: materials ("Metal - PalmSHIELD - Dusty Grey", "Metal - PalmSHIELD - Dusty Grey") | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl:8" x 8" x 1/2"" | 4 occurrences | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | 30 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | 3 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | 3 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL" | 3 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | 10 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL" | 1 occurrence | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | 1 occurrence | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum:6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" | 1 occurrence | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl:8" x 8" x 1/2"" | 1 occurrence | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl:3" x 3" x 3/4"" | 1 occurrence | material: materials ("Metal - PalmSHIELD - Dusty Grey", "Metal - PalmSHIELD - Dusty Grey") | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl:6063 T6 ALUM 3" X 3" POSTS" | 1 occurrence | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Constraints, Dimensions, Identity Data, Other, Pset_ManufacturerTypeInformation, Pset_ProductRequirements

Property sets
  Pset_ProductRequirements | properties | on 67 objects (67 IFCBUILDINGELEMENTPROXY) | on 14 type objects
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 40 objects (40 IFCBUILDINGELEMENTPROXY)
    C Cut Distance = 0.0625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum" (IFCLABEL)
    Family and Type = "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum: 6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" (IFCLABEL)
    Field Cut = FALSE (IFCBOOLEAN)
    Type = "6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" (IFCLABEL)
    Type Id = "134925" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl" (IFCLABEL)
    Family and Type = "Nested-Top_Cap-Palmshield-Mercury_Economic-Solid-Vinyl: 3" x 3" x 3/4"" (IFCLABEL)
    Type = "3" x 3" x 3/4"" (IFCLABEL)
    Type Id = "134977" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl" (IFCLABEL)
    Family and Type = "Nested-Base_Plate-Palmshield-Mercury_Economic-Solid-Vinyl: 8" x 8" x 1/2"" (IFCLABEL)
    Type = "8" x 8" x 1/2"" (IFCLABEL)
    Type Id = "134975" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Corner Post Down = FALSE (IFCBOOLEAN)
    Corner Post Up = FALSE (IFCBOOLEAN)
    End Post = FALSE (IFCBOOLEAN)
    Family = "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl" (IFCLABEL)
    Family and Type = "Nested-Square_Post-Palmshield-Mercury_Economic-Solid-Vinyl: 6063 T6 ALUM 3" X 3" POSTS" (IFCLABEL)
    Middle Post = TRUE (IFCBOOLEAN)
    Post Position = 1 (IFCINTEGER)
    Type = "6063 T6 ALUM 3" X 3" POSTS" (IFCLABEL)
    Type Id = "134981" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    C Cut Distance = 0.19791666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum" (IFCLABEL)
    Family and Type = "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum: 6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" (IFCLABEL)
    Field Cut = TRUE (IFCBOOLEAN)
    Type = "6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" (IFCLABEL)
    Type Id = "134925" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    C Cut Distance = 0.21875000000047987 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum" (IFCLABEL)
    Family and Type = "Nested-Louvers-Palmshield-Mercury_Economic-Solid-Aluminum: 6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" (IFCLABEL)
    Field Cut = TRUE (IFCBOOLEAN)
    Type = "6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" (IFCLABEL)
    Type Id = "134925" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum" (IFCLABEL)
    Family and Type = "Nested-U_Channel-Palmshield-Mercury_Economic-Solid-Aluminum: 6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL" (IFCLABEL)
    Type = "6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL" (IFCLABEL)
    Type Id = "134929" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other: 7 more contents on 2 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 48 objects (48 IFCBUILDINGELEMENTPROXY)
    Reference = "6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "6063 T6 ALUM 3" X 3" POSTS" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "3" x 3" x 3/4"" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "8" x 8" x 1/2"" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 67 objects (67 IFCBUILDINGELEMENTPROXY) | on 14 type objects
    Manufacturer = "PalmSHIELD" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 48 objects (48 IFCBUILDINGELEMENTPROXY)
    Reference = "6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "6063 T6 ALUM 3" X 3" POSTS" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "3" x 3" x 3/4"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "8" x 8" x 1/2"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 36 objects (36 IFCBUILDINGELEMENTPROXY)
    Depth = 4.083333333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.5 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY)
    Depth = 4.4166666666666652 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.5 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY) | on 6 type objects
    Width = 0.25 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Depth = 0.04166666666666665 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Height = 0.66666666666666696 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.66666666666666663 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Depth = 4.0833333333333339 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.25 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 4.4166666666666661 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.25 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 0.04166666666666665 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Height = 0.66666666666667473 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.66666666666666663 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 6 type objects
    Width = 0.5 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid: 1 more content on 0 objects not shown
  Constraints | properties | on 67 objects (67 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 14 type objects
    Default Elevation = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 30 objects (30 IFCBUILDINGELEMENTPROXY)
    Area = 2.6396752241532586 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Desired Cut Distance = 0.14583333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 4.0833333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.15604571759286848 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Area = 2.8520393014083929 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Desired Cut Distance = 0.14583333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 4.4166666666666661 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.16878414351881693 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Area = 0.14158676270008255 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 0.0026041666666583819 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Area = 0.50409356849396048 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 0.018007174146348129 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Area = 30.095920138898226 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 5.9583333333334405 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.040405273437483603 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Area = 2.0429643481882036 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Desired Cut Distance = 0.19791666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 4.0833333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.1212452256946641 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Area = 1.9562664315195395 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Desired Cut Distance = 0.21875000000047987 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 4.0833333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.11459563078709264 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Area = 2.2784830729166701 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 4.0833333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.011741355613425954 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions: 10 more contents on 5 objects not shown
  Electrical - Loads | properties | on 67 objects (67 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Materials and Finishes | properties | on 52 objects (52 IFCBUILDINGELEMENTPROXY)
    Material = "Metal - PalmSHIELD - Grey Beige" (IFCLABEL)
  Materials and Finishes | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Material = "Metal - PalmSHIELD - Dusty Grey" (IFCLABEL)
  Model Properties | properties | on 48 objects (48 IFCBUILDINGELEMENTPROXY)
    Component Name = "Mercury Economic Solid - Aluminum - Louvers" (IFCTEXT)
    ID = "Not Assigned" (IFCTEXT)
  Model Properties | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Component Name = "Mercury Economic Solid - Aluminum - Post" (IFCTEXT)
    ID = "" (IFCTEXT)
  Model Properties | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Component Name = "Mercury Economic Solid - Aluminum - Top Cap" (IFCTEXT)
    ID = "Not Assigned" (IFCTEXT)
  Model Properties | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Component Name = "Mercury Economic Solid - Aluminum - Base Plate" (IFCTEXT)
    ID = "Not Assigned" (IFCTEXT)
  Model Properties | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Component Name = "Mercury Economic Solid - Aluminum - U Channel" (IFCTEXT)
    ID = "Not Assigned" (IFCTEXT)
  Phasing | properties | on 67 objects (67 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 6 type objects
    Assembly Code = "F1020100" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "Copyright ©2024 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Mercury Economic Solid - Louvers" (IFCTEXT)
    Instruction Sheet Link = "Contact Manufacturer for More Information" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Mercury Economic Solid" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "Contact Manufacturer for More Information" (IFCTEXT)
    Product Page URL = "Contact Manufacturer for More Information" (IFCTEXT)
    Type Name = "6063 T6 ALUM 6" TONGUE AND GROOVE INFILL" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Identity Data | properties | on 2 type objects
    Assembly Code = "F1020100" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©2023 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Mercury Economic Solid - Aluminum - Post" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Mercury Economic Solid" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "Contact Manufacturer for More Information" (IFCTEXT)
    Product Page URL = "Contact Manufacturer for More Information" (IFCTEXT)
    Type Name = "6063 T6 ALUM 3" X 3" POSTS" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Identity Data | properties | on 2 type objects
    Assembly Code = "F1020100" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©2023 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Mercury Economic Solid - Aluminum - Top Cap" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Mercury Economic Solid" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "Contact Manufacturer for More Information" (IFCTEXT)
    Product Page URL = "Contact Manufacturer for More Information" (IFCTEXT)
    Type Name = "3" x 3" x 3/4"" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Identity Data | properties | on 2 type objects
    Assembly Code = "F1020100" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©2023 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Mercury Economic Solid - Aluminum - Base Plate" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Mercury Economic Solid" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "Contact Manufacturer for More Information" (IFCTEXT)
    Product Page URL = "Contact Manufacturer for More Information" (IFCTEXT)
    Type Name = "8" x 8" x 1/2"" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Identity Data | properties | on 2 type objects
    Assembly Code = "F1020100" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "Copyright ©2024 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Mercury Economic Solid - U Channel" (IFCTEXT)
    Instruction Sheet Link = "Contact Manufacturer for More Information" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Mercury Economic Solid" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "Contact Manufacturer for More Information" (IFCTEXT)
    Product Page URL = "Contact Manufacturer for More Information" (IFCTEXT)
    Type Name = "6063 T6 ALUM 3" X 2" GATE FRAME U CHANNEL" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)