IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "RevitIdentifiers [ContentGUID: d11a4d4f-5557-44a8-afe0-33311cb8d256, VersionGUID: 15113d74-a9f0-491a-b492-31621dd16e2f, NumberOfSaves: 109]"
File name: "Palmshield-Palisade-Fortress-Array.ifc"
Time stamp: "2025-06-13T13:38:26-05:00"
Preprocessor: "ODA SDAI 24.12"
Originating system: "Autodesk Revit 25.3.0.46 (ENU) - IFC 25.3.0.46"
Application: "Autodesk Revit 2025 (ENU)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2025 (ENU)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ENU)" | change NOCHANGE | created 1720020883 (2024-07-03T15:34:43Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 89 elements
          5 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Top_Cap-Palmshield-Palisade:4" x 4" x 1/4"" | object type "Nested-Top_Cap-Palmshield-Palisade:4" x 4" x 1/4"" | names: "Nested-Top_Cap-Palmshield-Palisade:4" x 4" x 1/4":282837", "Nested-Top_Cap-Palmshield-Palisade:4" x 4" x 1/4":282862", "Nested-Top_Cap-Palmshield-Palisade:4" x 4" x 1/4":282897" (+2 more) | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Model Properties, Constraints, Dimensions
          5 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Square_Post-Palmshield-Palisade:TS 4" X 4" X 1/4"" | object type "Nested-Square_Post-Palmshield-Palisade:TS 4" X 4" X 1/4"" | names: "Nested-Square_Post-Palmshield-Palisade:TS 4" X 4" X 1/4":282838", "Nested-Square_Post-Palmshield-Palisade:TS 4" X 4" X 1/4":282863", "Nested-Square_Post-Palmshield-Palisade:TS 4" X 4" X 1/4":282898" (+2 more) | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Model Properties, Constraints, Dimensions
          5 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Base_Plate-Palmshield-Palisade:10" x 10" x 3/4"" | object type "Nested-Base_Plate-Palmshield-Palisade:10" x 10" x 3/4"" | names: "Nested-Base_Plate-Palmshield-Palisade:10" x 10" x 3/4":282839", "Nested-Base_Plate-Palmshield-Palisade:10" x 10" x 3/4":282864", "Nested-Base_Plate-Palmshield-Palisade:10" x 10" x 3/4":282899" (+2 more) | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Model Properties, Constraints, Dimensions
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" | object type "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" | names: "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8":282840", "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8":282858", "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8":282859" (+1 more) | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Constraints, Dimensions, Materials and Finishes
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Cont_Alum_Horizontal-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3"" | object type "Nested-Cont_Alum_Horizontal-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3"" | names: "Nested-Cont_Alum_Horizontal-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3":282841", "Nested-Cont_Alum_Horizontal-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3":282860", "Nested-Cont_Alum_Horizontal-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3":282861" (+3 more) | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Constraints, Dimensions, Materials and Finishes
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" | object type "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" | names: "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8":282842", "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8":282865", "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8":282881" (+1 more) | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Constraints, Dimensions, Materials and Finishes
          44 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" | object type "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" | names: "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8":282843", "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8":282844", "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8":282845" (+41 more) | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Constraints, Dimensions, Materials and Finishes
          8 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Rect_Tube-Palmshield-Palisade:ALUM RECT TUBE 2" X 3" X 1/8"" | object type "Nested-Rect_Tube-Palmshield-Palisade:ALUM RECT TUBE 2" X 3" X 1/8"" | names: "Nested-Rect_Tube-Palmshield-Palisade:ALUM RECT TUBE 2" X 3" X 1/8":282854", "Nested-Rect_Tube-Palmshield-Palisade:ALUM RECT TUBE 2" X 3" X 1/8":282855", "Nested-Rect_Tube-Palmshield-Palisade:ALUM RECT TUBE 2" X 3" X 1/8":282877" (+5 more) | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Constraints, Dimensions, Phasing
          8 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nested-Cont_Alum-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3"" | object type "Nested-Cont_Alum-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3"" | names: "Nested-Cont_Alum-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3":282856", "Nested-Cont_Alum-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3":282857", "Nested-Cont_Alum-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3":282879" (+5 more) | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Other, Model Properties, Constraints, Dimensions

Types
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Top_Cap-Palmshield-Palisade:4" x 4" x 1/4"" | 5 occurrences | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Square_Post-Palmshield-Palisade:TS 4" X 4" X 1/4"" | 5 occurrences | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Base_Plate-Palmshield-Palisade:10" x 10" x 3/4"" | 5 occurrences | material: "Metal - PalmSHIELD - Dusty Grey" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" | 4 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Cont_Alum_Horizontal-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3"" | 6 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" | 4 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Pickets-Palmshield-Palisade:ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" | 44 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Rect_Tube-Palmshield-Palisade:ALUM RECT TUBE 2" X 3" X 1/8"" | 8 occurrences | material: "<Unnamed>" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Nested-Cont_Alum-Palmshield-Palisade:CONT. ALUM FB 1/4" X 3"" | 8 occurrences | material: "Metal - PalmSHIELD - Grey Beige" | property sets: Other, Constraints, Dimensions, Identity Data, Pset_ManufacturerTypeInformation

Property sets
  Pset_BuildingElementProxyCommon | properties | on 52 objects (52 IFCBUILDINGELEMENTPROXY)
    Reference = "ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY)
    Reference = "CONT. ALUM FB 1/4" X 3"" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Reference = "ALUM RECT TUBE 2" X 3" X 1/8"" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "4" x 4" x 1/4"" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "TS 4" X 4" X 1/4"" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "10" x 10" x 3/4"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 52 objects (52 IFCBUILDINGELEMENTPROXY)
    Reference = "ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY)
    Reference = "CONT. ALUM FB 1/4" X 3"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Reference = "ALUM RECT TUBE 2" X 3" X 1/8"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "4" x 4" x 1/4"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "TS 4" X 4" X 1/4"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "10" x 10" x 3/4"" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Other | properties | on 44 objects (44 IFCBUILDINGELEMENTPROXY)
    C Hole Offset = 0.125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Component Vis = TRUE (IFCBOOLEAN)
    Cut In Place = FALSE (IFCBOOLEAN)
    Family = "Nested-Pickets-Palmshield-Palisade" (IFCLABEL)
    Family and Type = "Nested-Pickets-Palmshield-Palisade: ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" (IFCLABEL)
    Type = "ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" (IFCLABEL)
    Type Id = "282331" (IFCLABEL)
  Other | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    C Hole Offset = 0.125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Component Vis = TRUE (IFCBOOLEAN)
    Cut In Place = TRUE (IFCBOOLEAN)
    Family = "Nested-Pickets-Palmshield-Palisade" (IFCLABEL)
    Family and Type = "Nested-Pickets-Palmshield-Palisade: ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" (IFCLABEL)
    Type = "ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" (IFCLABEL)
    Type Id = "282331" (IFCLABEL)
  Other | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Rect_Tube-Palmshield-Palisade" (IFCLABEL)
    Family and Type = "Nested-Rect_Tube-Palmshield-Palisade: ALUM RECT TUBE 2" X 3" X 1/8"" (IFCLABEL)
    Type = "ALUM RECT TUBE 2" X 3" X 1/8"" (IFCLABEL)
    Type Id = "282342" (IFCLABEL)
  Other | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Cont_Alum-Palmshield-Palisade" (IFCLABEL)
    Family and Type = "Nested-Cont_Alum-Palmshield-Palisade: CONT. ALUM FB 1/4" X 3"" (IFCLABEL)
    Type = "CONT. ALUM FB 1/4" X 3"" (IFCLABEL)
    Type Id = "282337" (IFCLABEL)
  Other | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Cont_Alum_Horizontal-Palmshield-Palisade" (IFCLABEL)
    Family and Type = "Nested-Cont_Alum_Horizontal-Palmshield-Palisade: CONT. ALUM FB 1/4" X 3"" (IFCLABEL)
    Type = "CONT. ALUM FB 1/4" X 3"" (IFCLABEL)
    Type Id = "282487" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Top_Cap-Palmshield-Palisade" (IFCLABEL)
    Family and Type = "Nested-Top_Cap-Palmshield-Palisade: 4" x 4" x 1/4"" (IFCLABEL)
    Type = "4" x 4" x 1/4"" (IFCLABEL)
    Type Id = "282430" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Square_Post-Palmshield-Palisade" (IFCLABEL)
    Family and Type = "Nested-Square_Post-Palmshield-Palisade: TS 4" X 4" X 1/4"" (IFCLABEL)
    Type = "TS 4" X 4" X 1/4"" (IFCLABEL)
    Type Id = "282428" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Nested-Base_Plate-Palmshield-Palisade" (IFCLABEL)
    Family and Type = "Nested-Base_Plate-Palmshield-Palisade: 10" x 10" x 3/4"" (IFCLABEL)
    Type = "10" x 10" x 3/4"" (IFCLABEL)
    Type Id = "282425" (IFCLABEL)
  Other: 9 more contents on 3 objects not shown
  Constraints | properties | on 89 objects (89 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 9 type objects
    Default Elevation = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 44 objects (44 IFCBUILDINGELEMENTPROXY)
    Area = 7.4440400285861443 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Desired Cut In Place = 0.041666666666666664 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 0.33333333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 9.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Real Height = 0.33333333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.077456581013026771 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Area = 4.6135130352742149 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Desired Cut In Place = 0.20833333333333334 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 0.20833333333333334 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 9.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Real Height = 0.20833333333333334 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.046974599313154564 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Area = 3.1132434600348242 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 3.958333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.032401233072243824 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Area = 0.12276332925807742 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 0.0022837585193995168 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Area = 11.888722739705646 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 9.916666666666881 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.24715977317770282 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Area = 0.8108857221255874 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 0.042635747114845808 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Area = 3.1419270833334187 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 3.9583333333334472 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.032642505787037951 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Area = 3.1419270833334187 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Length = 3.9583333333334467 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.032642505787037951 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions: 9 more contents on 9 objects not shown
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 3 type objects
    Assembly Code = "F1020100" (IFCTEXT)
    Copyright = "©2023 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Palisade - Pickets" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Palisade" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "https://palmshieldlouvers.com/cad-drawings/palisade-louvers/" (IFCTEXT)
    Product Page URL = "https://palmshieldlouvers.com/products/palisade-louvers/" (IFCTEXT)
    Type Name = "ALUM RECT TUBE PICKETS 1" X 4" X 1/8"" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Identity Data | properties | on 2 type objects
    Assembly Code = "F1020100" (IFCTEXT)
    Copyright = "©2023 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Palisade - Cont Alum" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Palisade" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "https://palmshieldlouvers.com/cad-drawings/palisade-louvers/" (IFCTEXT)
    Product Page URL = "https://palmshieldlouvers.com/products/palisade-louvers/" (IFCTEXT)
    Type Name = "CONT. ALUM FB 1/4" X 3"" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "F1020100" (IFCTEXT)
    Copyright = "©2023 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Palisade - Top Cap" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Palisade" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "https://palmshieldlouvers.com/products/louvers/" (IFCTEXT)
    Product Page URL = "https://palmshieldlouvers.com/cad-drawings/economic-louvers/asia-commercial-horizontal-louver/" (IFCTEXT)
    Type Name = "4" x 4" x 1/4"" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "F1020100" (IFCTEXT)
    Copyright = "©2023 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Palisade - Post" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Palisade" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "https://palmshieldlouvers.com/products/louvers/" (IFCTEXT)
    Product Page URL = "https://palmshieldlouvers.com/wp-content/uploads/2021/04/ASIA-HORIZONTAL-LOUVER-CHANNEL-PANEL-BASE-PLATE-DETAIL.pdf" (IFCTEXT)
    Type Name = "TS 4" X 4" X 1/4"" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "F1020100" (IFCTEXT)
    Copyright = "©2023 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Palisade - Base Plate" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Palisade" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "https://palmshieldlouvers.com/wp-content/uploads/2021/04/ASIA-HORIZONTAL-LOUVER-CHANNEL-PANEL-BASE-PLATE-DETAIL.pdf" (IFCTEXT)
    Product Page URL = "https://palmshieldlouvers.com/products/louvers/" (IFCTEXT)
    Type Name = "10" x 10" x 3/4"" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "F1020100" (IFCTEXT)
    Copyright = "©2023 The American Fence Company and PalmSHIELD. All Rights Reserved." (IFCTEXT)
    Description = "Palisade - Rect Tube" (IFCTEXT)
    Keynote = "05 10 00" (IFCTEXT)
    Manufacturer = "PalmSHIELD" (IFCTEXT)
    Manufacturer Address = "12330 Cary Circle, La Vista, NE 68128" (IFCTEXT)
    Manufacturer Email = "mailto: info@palmshieldlouvers.com" (IFCTEXT)
    Manufacturer Fax Number = "Consult Manufacturer Website for More Information" (IFCTEXT)
    Manufacturer Phone Number = "531-329-4406" (IFCTEXT)
    Model = "Palisade" (IFCTEXT)
    OmniClass Number = "23.55.00.00" (IFCTEXT)
    OmniClass Title = "Manufactured Structures" (IFCTEXT)
    Product Documentation Link = "https://palmshieldlouvers.com/cad-drawings/palisade-louvers/" (IFCTEXT)
    Product Page URL = "https://palmshieldlouvers.com/products/palisade-louvers/" (IFCTEXT)
    Type Name = "ALUM RECT TUBE 2" X 3" X 1/8"" (IFCTEXT)
    URL = "https://palmshieldlouvers.com/" (IFCTEXT)
    Version = "2020 - v1.0a" (IFCTEXT)
    Warranty URL = "https://palmshieldlouvers.com/wp-content/uploads/2020/01/PalmSHIELD-Warranty-NO-SIGN-LINE.pdf" (IFCTEXT)
  Model Properties | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Component Name = "Atlas - Post Cap" (IFCTEXT)
    ID = "Not Assigned" (IFCTEXT)
  Model Properties | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Component Name = "Atlas - Square Post" (IFCTEXT)
    ID = "Not Assigned" (IFCTEXT)
  Model Properties | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Component Name = "Atlas - Base Plate" (IFCTEXT)
    ID = "Not Assigned" (IFCTEXT)
  Model Properties | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Component Name = "Atlas - Right L-Frame" (IFCTEXT)
    ID = "Not Assigned" (IFCTEXT)
  Model Properties | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Component Name = "Atlas - Left L-Frame" (IFCTEXT)
    ID = "Not Assigned" (IFCTEXT)
  Materials and Finishes | properties | on 66 objects (66 IFCBUILDINGELEMENTPROXY)
    Material = "Metal - PalmSHIELD - Grey Beige" (IFCLABEL)
  Materials and Finishes | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Material = "Metal - PalmSHIELD - Dusty Grey" (IFCLABEL)
  Phasing | properties | on 89 objects (89 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 9 type objects
    Manufacturer = "PalmSHIELD" (IFCLABEL)