IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2023-01-26T11:28:14"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20220517_1515(x64) - Exporter 20.2.90.12 - Default UI"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1671211015 (2022-12-16T17:16:55Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Dryer_Weight-Rated_Milnor_M190-Steam" | object type "Dryer_Weight-Rated_Milnor_M190-Steam:Dryer_Weight-Rated_Milnor_M190-Steam" | names: "Dryer_Weight-Rated_Milnor_M190-Steam:Dryer_Weight-Rated_Milnor_M190-Steam:117508" | material: materials ("Paint - Milnor - Black", "Glazing - Milnor - as Specified", "Metal - Stainless Steel - Milnor - Powder Coat as Specified", "ARCAT Clearance") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction

Types
  IFCBUILDINGELEMENTPROXYTYPE "Dryer_Weight-Rated_Milnor_M190-Steam" | 1 occurrence | material: materials ("Paint - Milnor - Black", "Glazing - Milnor - as Specified", "Metal - Stainless Steel - Milnor - Powder Coat as Specified", "ARCAT Clearance") | property sets: Analytical Model, Constraints, Construction, Dimensions, Electrical - Loads, Identity Data

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Dryer_Weight-Rated_Milnor_M190-Steam" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Pellerin Milnor Corp" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Dryer_Weight-Rated_Milnor_M190-Steam" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Work Plane = "???" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    exhaustrad = 0.833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    fsswaterrad = 0.03125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    gasrad = 0.0520833333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Steam Damper System = "[Air Powered][Electromechanical]" (IFCTEXT)
  Construction | properties | on 1 type object
    Reversing = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 238.673766641012 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 255.488226693007 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Cylinder Depth = 3.625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Cylinder Diameter = 4.63541666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Base from FF = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Opening = 2.61458333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Opening Depth = 3.15625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Thickness = 0.114583333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Depth = 4.14583333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Height = 8.77083333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Width = 5. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Total Motor Watt Draw = 0. (IFCPOWERMEASURE) [WATT]
  Electrical - Loads | properties | on 1 type object
    Circuit Breaker Size = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Frequency = 0. (IFCFREQUENCYMEASURE) [HERTZ]
    MEP Amperage = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Number of Poles = 1 (IFCINTEGER)
    Number of Wires = 0 (IFCINTEGER)
    Phase = 0 (IFCINTEGER)
    Voltage_MEP = 0. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Clearance Visible = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "21" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "E1010610" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc." (IFCTEXT)
    Description = "" (IFCTEXT)
    Drawn By = "Sumex Design, Inc. / Robert S. Weygant, CSI, CDT, SCIP" (IFCTEXT)
    Keynote = "11110" (IFCTEXT)
    Manufacturer = "Pellerin Milnor Corp" (IFCTEXT)
    Model = "As Specified" (IFCTEXT)
    OmniClass Number = "23.45.70.11.14.17" (IFCTEXT)
    OmniClass Title = "Clothes Dryers" (IFCTEXT)
    Revision = "R1_04-2011" (IFCTEXT)
    Type Name = "Dryer_Weight-Rated_Milnor_M190-Steam" (IFCTEXT)
    URL = "http://www.milnor.com/" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Cabinet Finish = "Metal - Stainless Steel - Milnor - Powder Coat as Specified" (IFCLABEL)
    Door Finish = "Paint - Milnor - Black" (IFCLABEL)
    Door Glazing = "Glazing - Milnor - as Specified" (IFCLABEL)
    Interior Finish = "Metal - Stainless Steel - Milnor - as Specified" (IFCLABEL)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Exhaust Air,Power,Undefined,Fire Protection Wet" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
    Exhaust CL from FF = 1.66666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Exhaust CL from Side = 1.33333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Exhaust Diameter = 1.66666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Steam Boiler HP = 0. (IFCREAL)
    Steam Consumption = "as Specified" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Dryer_Weight-Rated_Milnor_M190-Steam: Dryer_Weight-Rated_Milnor_M190-Steam" (IFCLABEL)
    Family and Type = "Dryer_Weight-Rated_Milnor_M190-Steam: Dryer_Weight-Rated_Milnor_M190-Steam" (IFCLABEL)
    Type = "Dryer_Weight-Rated_Milnor_M190-Steam: Dryer_Weight-Rated_Milnor_M190-Steam" (IFCLABEL)
    Type Id = "Dryer_Weight-Rated_Milnor_M190-Steam: Dryer_Weight-Rated_Milnor_M190-Steam" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Dryer_Weight-Rated_Milnor_M190-Steam" (IFCTEXT)
    Manufacturer Address = "700 Jackson St. Kenner, LA 70062" (IFCTEXT)
    Manufacturer Fax = "504-468-3094" (IFCTEXT)
    Manufacturer Phone - Toll Free = "800-469-8780" (IFCTEXT)
    Manufacturer Phone = "504-467-9591" (IFCTEXT)
    Manufacturer Website = "http://www.milnor.com/" (IFCTEXT)
    Send Message = "http://www.arcat.com/users.pl?action=UserEmail&company=Pellerin+Milnor+Corp.&coid=34740&rep=108&fax=504-468-3094&mf=" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Analytical Model | properties | on 1 type object
    Capacity = "" (IFCTEXT)
    Cylinder Volume = 0. (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
    Unit Weight = 0. (IFCREAL)
  Mechanical - Flow | properties | on 1 type object
    Air Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Plumbing | properties | on 1 type object
    Compressed Air Connection Diameter = 0.0208333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    FSS Water Connection CL from FF = 7.45833333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    FSS Water Connection Diameter = 0.0625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    FSS Water Connection from Side = 0.583333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Piping_Max Operating Pressure = 0. (IFCPRESSUREMEASURE) [PASCAL]
    Steam Return Connection Diameter = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Steam Supply Connection Diameter = 0.104166666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Text | properties | on 1 type object
    Construction Details = "" (IFCTEXT)
    Green Building-LEED = "" (IFCTEXT)
    Installation-Fabrication = "" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos34/arc34740.html" (IFCTEXT)
    Product Properties = "" (IFCTEXT)
    Sales Information = "http://www.milnor.com/contact_us.aspx" (IFCTEXT)
    SpecWizard = "" (IFCTEXT)
    Specification = "" (IFCTEXT)

Other addresses and roles
  2 x postal address (none given)