IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2026-05-15T15:08:05-05:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "23.0.11.19 - Exporter 23.0.11.19 - Default UI"
Application: "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)" | change NOCHANGE | created 1673537642 (2023-01-12T15:34:02Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire:Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire" | object type "Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire:Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire" | names: "Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire:Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire:102545" | material: materials ("ARCAT Clearance", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304 Perforated") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Analytical Model, Constraints, Construction

Types
  IFCBUILDINGELEMENTPROXYTYPE "Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire:Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire" | 1 occurrence | material: materials ("ARCAT Clearance", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304", "Metal - Steel - PoweredAire - Stainless 304 Perforated") | property sets: Analytical Model, Constraints, Construction, Dimensions, Electrical - Loads, Identity Data

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire" (IFCLABEL)
    Family and Type = "Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire: Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire" (IFCLABEL)
    Type = "Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire" (IFCLABEL)
    Type Id = "102520" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire" (IFCTEXT)
    Manufacturer Address = "109 Mortensen Rd. Greenville, PA 16125" (IFCTEXT)
    Manufacturer Fax = "724-588-3371" (IFCTEXT)
    Manufacturer Phone - Toll Free = "888-321-2473" (IFCTEXT)
    Manufacturer Phone = "724-588-3305" (IFCTEXT)
    Manufacturer Website = "http://www.poweredaire.com/" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire" (IFCIDENTIFIER)
  Analytical Model | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Available Options = "as Specified" (IFCTEXT)
  Analytical Model | properties | on 1 type object
    Sound Pressure = "53 dBA" (IFCTEXT)
    Standards Conformance = "ETL ; Made in USA" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "Basic Wall : Wall 1" (IFCTEXT)
    Mounting Height = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Projection from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Clearance_Bottom = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Clearance_Intake = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Clearance_Side A = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Clearance_Side B = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Clearance_Top = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 type object
    Max Height = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 32.211291792202502 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Dia = 0.083333333333333343 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 9.4356887438341204 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Mounting Width = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Nozzle Width = 2.916666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Depth = 1.2333984375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Height = 0.70833333333333326 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Width = 6.0833333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Width Notes = "Other Widths available." (IFCTEXT)
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Electrical_Amperage = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Electrical_Frequency = 0. (IFCFREQUENCYMEASURE) [HERTZ]
    Electrical_Phase = 2 (IFCINTEGER)
    Electrical_Voltage = 0. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Electrical_Wattage = 0. (IFCPOWERMEASURE) [WATT]
  Electrical - Loads | properties | on 1 type object
    Heating Element Load = 0. (IFCPOWERMEASURE) [WATT]
    Power Rating = 0. (IFCPOWERMEASURE) [WATT]
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Include Clearance = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "D3090400" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc." (IFCTEXT)
    Description = "EVE-2-72HW" (IFCTEXT)
    Drawn By = "" (IFCTEXT)
    Keynote = "23 34 33" (IFCTEXT)
    Manufacturer = "Powered Aire, Inc" (IFCTEXT)
    Model = "EVE-2-72HW" (IFCTEXT)
    OmniClass Number = "23.75.35.17.21" (IFCTEXT)
    OmniClass Title = "Air Curtains" (IFCTEXT)
    Revision = "" (IFCTEXT)
    Type Name = "Air-Curtain_Climate-Control_EVE-Steam-Unit_Powered-Aire" (IFCTEXT)
    URL = "http://www.poweredaire.com/" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Clearance Material = "ARCAT Clearance" (IFCLABEL)
    Frame Finish = "Metal - Steel - PoweredAire - Stainless 304" (IFCLABEL)
    Front Grating Material = "Metal - Steel - PoweredAire - Stainless 304 Perforated" (IFCLABEL)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Power,Undefined" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
    Motor Count = 1 (IFCINTEGER)
    Motor HP = 0.20000000000000001 (IFCREAL)
    Motor RPM = 1075. (IFCREAL)
  Mechanical - Flow | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    HVAC_Outlet Velocity = 0. (IFCLINEARVELOCITYMEASURE) [derived]
    HVAC_Outlet Volume = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    HVAC_Temperature Rise = -17.777777777777743 (IFCTHERMODYNAMICTEMPERATUREMEASURE) [DEGREE_CELSIUS]
  Mechanical - Flow | properties | on 1 type object
    HVAC_Outlet Velocity Uniformity = 0.87 (IFCREAL)
    Outlet Velocity_Range = "1316 FPM" (IFCTEXT)
    Outlet Volume_Range = "961 CFM" (IFCTEXT)
    Temperature Rise_Range = "27" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Structural | properties | on 1 type object
    Unit Weight = 59. (IFCREAL)
  Text | properties | on 1 type object
    Building Codes = "" (IFCTEXT)
    Construction Details = "http://www.arcat.com/details/powair/prod3336.html" (IFCTEXT)
    Green Building-LEED = "http://www.arcat.com/green/clients/leed_data_47623.html" (IFCTEXT)
    Installation-Fabrication = "" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos47/arc47623.html" (IFCTEXT)
    Product Properties = "" (IFCTEXT)
    Sales Information = "https://poweredaire.com/contact" (IFCTEXT)
    SpecWizard = "" (IFCTEXT)
    Specification = "http://www.arcat.com/sdspecs/htm04/23_34_33pai.htm" (IFCTEXT)
    Test Data = "" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "Powered Aire, Inc" (IFCLABEL)