IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2026-02-26T08:43:58-05:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "23.0.11.19 - Exporter 23.0.11.19 - Default UI"
Application: "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)" | change NOCHANGE | created 1673537642 (2023-01-12T15:34:02Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window_Vinyl_Atrium-SilentGuard_720-Casement:as Specified" | object type "Window_Vinyl_Atrium-SilentGuard_720-Casement:as Specified" | names: "Window_Vinyl_Atrium-SilentGuard_720-Casement:as Specified:134849" | material: materials ("Glass - AtriumSG - Clear", "Metal - AtriumSG - Window Screen", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Analysis Results, Constraints, Construction

Types
  IFCWINDOWSTYLE "Window_Vinyl_Atrium-SilentGuard_720-Casement:as Specified" | 1 occurrence | material: materials ("Glass - AtriumSG - Clear", "Metal - AtriumSG - Window Screen", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White", "Vinyl - AtriumSG - White") | property sets: Window_Vinyl_Atrium-SilentGuard_720-Casement:as Specified:134849, Analytical Model, Analytical Properties, Construction, Dimensions, Identity Data

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCWINDOW) | on 1 type object
    Category = "Windows" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
    Family = "Window_Vinyl_Atrium-SilentGuard_720-Casement" (IFCLABEL)
    Family and Type = "Window_Vinyl_Atrium-SilentGuard_720-Casement: as Specified" (IFCLABEL)
    Head Height = 2.9583333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "134848" (IFCLABEL)
    Type = "as Specified" (IFCLABEL)
    Type Id = "134830" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Windows" (IFCLABEL)
    Family Name = "Window_Vinyl_Atrium-SilentGuard_720-Casement" (IFCTEXT)
    Manufacturer Address = "9001 Ambassador Row Dallas, TX 75247" (IFCTEXT)
    Manufacturer Fax = "214-630-5010" (IFCTEXT)
    Manufacturer Phone - Toll Free = "800-421-6292" (IFCTEXT)
    Manufacturer Phone = "214-630-5757" (IFCTEXT)
    Manufacturer Website = "http://www.silent-guard.com/" (IFCTEXT)
    Send Message = "http://www.arcat.com/users.pl?action=UserEmail&amp;company=Atrium+SilentGuard+Acoustical+Windows+and+Doors&amp;coid=45763&amp;rep=108&amp;fax=214-630-5010&amp;mf=95">Send Email" (IFCTEXT)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWINDOW)
    Reference = "as Specified" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "as Specified" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Analysis Results | properties | on 1 object (1 IFCWINDOW)
    EWR = 0 (IFCINTEGER)
    OITC = 0 (IFCINTEGER)
    Sound Transmission Class (STC) = 0 (IFCINTEGER)
  Constraints | properties | on 1 object (1 IFCWINDOW)
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    glassheight = 2.5625000000000004 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    glasswidth = 2.5625000000000004 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCWINDOW)
    Frame Design_Finless = FALSE (IFCBOOLEAN)
    Frame Design_Finned = TRUE (IFCBOOLEAN)
    Include Screen = TRUE (IFCBOOLEAN)
    Inset from Exterior Wall = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 type object
    RO Spacing_Bottom = 0.020833333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    RO Spacing_Sides = 0.020833333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    RO Spacing_Top = 0.020833333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Wall Closure = "By host" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCWINDOW)
    Area = 29.689547013556439 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 1.1588837236883347 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Frame Thickness = 0.27083333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Glass Thickness = 0.072916666666666671 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 2.9583333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Swing Projection = 2.786783854166667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 2.9583333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Energy Analysis | properties | on 1 object (1 IFCWINDOW)
    SHGC = 0. (IFCREAL)
    U-Factor = 0. (IFCREAL)
    VLT = 0. (IFCREAL)
  Graphics | properties | on 1 object (1 IFCWINDOW)
    Grid Count_Horizontal = 0 (IFCINTEGER)
    Grid Count_Vertical = 0 (IFCINTEGER)
    Grid_Grids Between Glass = TRUE (IFCBOOLEAN)
    Grid_Surface Applied = FALSE (IFCBOOLEAN)
    Nailing Fin Location from Inside Edge of Frame = 0.15104166666666666 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Open Left = FALSE (IFCBOOLEAN)
    Open Right = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCWINDOW)
    Mark = "5" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2020100" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc." (IFCTEXT)
    Description = "Atrium SilentGuard Vinyl Casement Window - 720 Model as Specified as Specified" (IFCTEXT)
    Drawn By = "Sumex Design, Inc. / Robert S. Weygant, CSI, CDT, SCIP" (IFCTEXT)
    Keynote = "as Specified" (IFCTEXT)
    Manufacturer = "Atrium Companies, Inc." (IFCTEXT)
    Model = "as Specified" (IFCTEXT)
    OmniClass Number = "23.30.20.17.21.14" (IFCTEXT)
    OmniClass Title = "Casement Windows" (IFCTEXT)
    Type Mark = "5" (IFCTEXT)
    Type Name = "as Specified" (IFCTEXT)
    URL = "http://www.silent-guard.com/" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCWINDOW)
    Frame Finish = "Vinyl - AtriumSG - White" (IFCLABEL)
    Glazing Configuration = "as Specified" (IFCTEXT)
    Glazing Tint = "Glass - AtriumSG - Clear" (IFCLABEL)
    Glazing Type = "as Specified" (IFCTEXT)
    Screen Material = "Metal - AtriumSG - Window Screen" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCWINDOW)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Window_Vinyl_Atrium-SilentGuard_720-Casement:as Specified:134849 | predefined | on 1 type object
  Analytical Model | properties | on 1 type object
    Air Infiltration = "Less than 0.01 cfm/ft^2" (IFCTEXT)
    Forced Entry Rating = "Grade 10 ; No Entry" (IFCTEXT)
    Meets Egress = "as Specified" (IFCTEXT)
    Miami Dade Conformance = "as Specified" (IFCTEXT)
    Standards Conformance = "C-R-55" (IFCTEXT)
    Structural Test Pressure = "Test Size: 36 x 72 ; DP-55 ; 82.76 psf" (IFCTEXT)
    Water Penetration = "10.65 psf" (IFCTEXT)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Text | properties | on 1 type object
    Construction Details = "http://www.silent-guard.com/professional/technical-data/" (IFCTEXT)
    Green Building-LEED = "http://www.arcat.com/green/clients95/leed_data_45763.html" (IFCTEXT)
    Installation-Fabrication = "" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos9545/arc45763.html" (IFCTEXT)
    Product Properties = "" (IFCTEXT)
    Sales Information = "http://www.silent-guard.com/contact/" (IFCTEXT)
    SpecWizard = "" (IFCTEXT)
    Specification = "" (IFCTEXT)
    Test Data = "http://www.silent-guard.com/learning-center/" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "Atrium Companies, Inc." (IFCLABEL)
  IfcPermeableCoveringProperties | properties | on 1 type object
    FrameThickness = 0.27083333333333331 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  IfcWindowPanelProperties | properties | on 1 type object
    FrameThickness = 0.27083333333333331 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]