IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-07-18T17:50:01"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker:Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker" | object type "Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker:Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker" | names: "Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker:Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker:241777" | material: materials ("Alluminum", "Glass") | property sets: Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Constraints, Dimensions

Types
  IFCWINDOWSTYLE "Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker:Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker" | 1 occurrence | material: materials ("Alluminum", "Glass") | property sets: Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker:Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker:241777, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCWINDOW) | on 1 type object
    Category = "Windows" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
    Family = "Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker" (IFCLABEL)
    Family and Type = "Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker: Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker" (IFCLABEL)
    Head Height = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "241767" (IFCLABEL)
    Type = "Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker" (IFCLABEL)
    Type Id = "241749" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Windows" (IFCLABEL)
    Default Sill Height = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Family Name = "Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCWINDOW) | on 1 type object
    Manufacturer = "Quaker Windows & Doors" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWINDOW)
    Reference = "Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCWINDOW)
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCWINDOW)
    Area = 99.052662518486059 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 0.83642059332991991 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Height = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 5. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCWINDOW)
    Mark = "24" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©ARCAT" (IFCTEXT)
    Keynote = "08 51 13" (IFCTEXT)
    Manufacturer = "Quaker Windows & Doors" (IFCTEXT)
    OmniClass Number = "23.30.20.00" (IFCTEXT)
    OmniClass Title = "Windows" (IFCTEXT)
    Product Page URL = "https://www.arcat.com/company/quaker-windows-doors-39937" (IFCTEXT)
    Type Mark = "24" (IFCTEXT)
    Type Name = "Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker" (IFCTEXT)
    URL = "https://www.quakercommercialwindows.com/" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCWINDOW)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker:Window_Commercial_Aluminum_CF-Right-Split_1_H450_Quaker:241777 | predefined | on 1 type object
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Construction Type = "" (IFCTEXT)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Materials and Finishes | properties | on 1 type object
    Glass = "Glass" (IFCLABEL)
    Window Frame = "Alluminum" (IFCLABEL)