IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2024-04-30T11:43:28"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.70.21 - Exporter 21.1.70.21 - Default UI"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1686682715 (2023-06-13T18:58:35Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCDOOR | type IFCDOORSTYLE "Auto-Door_Sliding_BiPart_Wall_Tormax_TX9500:Glass Sidelight with Transom" | object type "Auto-Door_Sliding_BiPart_Wall_Tormax_TX9500:Glass Sidelight with Transom" | names: "Auto-Door_Sliding_BiPart_Wall_Tormax_TX9500:Glass Sidelight with Transom:105660" | material: materials ("Metal - Tormax - Aluminum Finished as Specified", "Metal - Tormax - Black", "Glass - Tormax - Glazing as Specified") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints

Types
  IFCDOORSTYLE "Auto-Door_Sliding_BiPart_Wall_Tormax_TX9500:Glass Sidelight with Transom" | 1 occurrence | material: materials ("Metal - Tormax - Aluminum Finished as Specified", "Metal - Tormax - Black", "Glass - Tormax - Glazing as Specified", "Glass - Tormax - Glazing as Specified") | property sets: Auto-Door_Sliding_BiPart_Wall_Tormax_TX9500:Glass Sidelight with Transom:105660, Analytical Model, Analytical Properties, Constraints, Construction, Dimensions

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "Auto-Door_Sliding_BiPart_Wall_Tormax_TX9500: Glass Sidelight with Transom" (IFCLABEL)
    Family and Type = "Auto-Door_Sliding_BiPart_Wall_Tormax_TX9500: Glass Sidelight with Transom" (IFCLABEL)
    Head Height = 11. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "Basic Wall: Wall 1" (IFCLABEL)
    Type = "Auto-Door_Sliding_BiPart_Wall_Tormax_TX9500: Glass Sidelight with Transom" (IFCLABEL)
    Type Id = "Auto-Door_Sliding_BiPart_Wall_Tormax_TX9500: Glass Sidelight with Transom" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Doors" (IFCLABEL)
    Family Name = "Auto-Door_Sliding_BiPart_Wall_Tormax_TX9500" (IFCTEXT)
    Manufacturer Address = "12859 Wetmore Rd. San Antonio, TX 78247" (IFCTEXT)
    Manufacturer Fax = "210-494-5930" (IFCTEXT)
    Manufacturer Phone - Toll Free = "888-685-3707" (IFCTEXT)
    Manufacturer Phone = "210-494-3551" (IFCTEXT)
    Manufacturer Website = "http://www.tormaxusa.com" (IFCTEXT)
    Send Message = "http://www.arcat.com/users.pl?action=UserEmail&company=Tormax+Technologies,+Inc.&coid=43969&rep=108&fax=210-494-5930&mf=" (IFCTEXT)
  Pset_ConcreteElementGeneral | properties | on 1 object (1 IFCDOOR) | on 1 type object
    FireRating = "as Specified" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireRating = "as Specified" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glass Sidelight with Transom" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 type object
    FireRating = "as Specified" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Glass Sidelight with Transom" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Manufacturer = "TORMAX USA Inc." (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Reference = "Glass Sidelight with Transom" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCDOOR)
    Inset from Exterior Wall = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Offset from Exterior Wall = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    HD Drive = FALSE (IFCBOOLEAN)
    Max Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Width = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    headerdepth = 0.666666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCDOOR)
    Backset from Offset Plane = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Threshold = "No Threshold" (IFCLABEL)
    Offset Plane from Exterior Wall Face = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 type object
    Include Transom = TRUE (IFCBOOLEAN)
    RO Spacing_Sides = 0.0208333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    RO Spacing_Top = 0.0208333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Wall Closure = "By host" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCDOOR)
    Area = 165.234354583014 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Clear Door Opening Height = 6.96875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Clear Door Opening Width = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Egress Width = 4.66666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Glazing Thickness_Transom = 0.0416666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Width = 2.53125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 11.0208333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 10.0416666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 10.4752376602604 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
    Width = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Air Space Below Door = 0.0260416666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Frame Thickness = 0.375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Glazing Thickness_Fixed Panel = 0.0416666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Glazing Thickness_Sliding Panel = 0.0416666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 11. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Thickness = 0.145833333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Thickness = 0.145833333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Transom Height = 3.33333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Energy Analysis | properties | on 1 object (1 IFCDOOR)
    SHGC = 0. (IFCREAL)
    U-Factor = 0. (IFCREAL)
    VLT = 0. (IFCREAL)
  Graphics | properties | on 1 object (1 IFCDOOR)
    Breakout Angle = 30. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Graphics | properties | on 1 type object
    Has Partial Breakout Capability = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2030110" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc." (IFCTEXT)
    Description = "Tormax Automatic Sliding BiPart Door - All Glass TX9500 as Specified" (IFCTEXT)
    Drawn By = "Sumex Design, Inc. / Robert S. Weygant, CSI, CDT, SCIP" (IFCTEXT)
    Fire Rating = "as Specified" (IFCTEXT)
    Keynote = "08463" (IFCTEXT)
    Manufacturer = "TORMAX USA Inc." (IFCTEXT)
    Model = "TX9500 as Specified" (IFCTEXT)
    OmniClass Number = "23.30.10.17.11" (IFCTEXT)
    OmniClass Title = "Sliding Doors" (IFCTEXT)
    Type Mark = "8" (IFCTEXT)
    Type Name = "Glass Sidelight with Transom" (IFCTEXT)
    URL = "http://www.tormaxusa.com" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCDOOR)
    Fixed Panel Finish = "Glass - Tormax - Glazing as Specified" (IFCLABEL)
    Frame Finish = "Metal - Tormax - Aluminum Finished as Specified" (IFCLABEL)
    Glazing Tint = "Glass - Tormax - Glazing as Specified" (IFCLABEL)
    Sensor Color = "Metal - Tormax - Black" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCDOOR)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Auto-Door_Sliding_BiPart_Wall_Tormax_TX9500:Glass Sidelight with Transom:105660 | predefined | on 2 type objects
  Analytical Model | properties | on 1 type object
    Air Infiltration = "N/A" (IFCTEXT)
    Available Options = "[Standard Weatherstripping][Electric Lock][Battery Backup][Door Position Monitoring][I/O Module][Key Switch]" (IFCTEXT)
    Miami Dade Conformance = "Does Not Apply" (IFCTEXT)
    Operating Temperature Range = "Ambient -30F to 130F" (IFCTEXT)
    Standards Conformance = "ANSI A156.10 ; NFPA 101 ; UL325 ; C-UL" (IFCTEXT)
    Structural Test Pressure = "N/A" (IFCTEXT)
    Water Penetration = "as Specified" (IFCTEXT)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Text | properties | on 1 type object
    Construction Details = "http://www.arcat.com/details/tormax/tormax.html?coid=43969" (IFCTEXT)
    Green Building-LEED = "http://www.arcat.com/green/clients/leed_data_43969.html" (IFCTEXT)
    Installation-Fabrication = "" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos43/arc43969.html" (IFCTEXT)
    Product Properties = "" (IFCTEXT)
    Sales Information = "http://www.tormaxusa.com/contact.php" (IFCTEXT)
    SpecWizard = "" (IFCTEXT)
    Specification = "http://www.arcat.com/sdspecs/htm/08463tor.htm" (IFCTEXT)
    Test Data = "" (IFCTEXT)