IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-01-29T09:22:01"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCDOOR | type IFCDOORSTYLE "Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:Doors_Integrated_Single-LR-Hold-Open-180_Total-Door" | object type "Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:Doors_Integrated_Single-LR-Hold-Open-180_Total-Door" | names: "Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:271827" | material: materials ("Magnet Finish", "Push Pull Panic Bar", "Push Pull Panic Bar", "Door Panel Finish", "Door Panel Finish", "Total Door - Concealed Hinge", "Total Door - Concealed Hinge", "Total Door - Concealed Hinge", "Total Door - Concealed Hinge", "Metal") | property sets: Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, IfcDoorPanelProperties, Constraints

Types
  IFCDOORSTYLE "Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:Doors_Integrated_Single-LR-Hold-Open-180_Total-Door" | 1 occurrence | material: materials ("Magnet Finish", "Push Pull Panic Bar", "Push Pull Panic Bar", "Door Panel Finish", "Door Panel Finish", "Total Door - Concealed Hinge", "Total Door - Concealed Hinge", "Total Door - Concealed Hinge", "Total Door - Concealed Hinge", "Metal") | property sets: Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:271827, Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:271827:1, Analytical Properties, Construction, Dimensions, Identity Data

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "Doors_Integrated_Single-LR-Hold-Open-180_Total-Door" (IFCLABEL)
    Family and Type = "Doors_Integrated_Single-LR-Hold-Open-180_Total-Door: Doors_Integrated_Single-LR-Hold-Open-180_Total-Door" (IFCLABEL)
    Head Height = 7.90625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "271817" (IFCLABEL)
    Type = "Doors_Integrated_Single-LR-Hold-Open-180_Total-Door" (IFCLABEL)
    Type Id = "271799" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Doors" (IFCLABEL)
    Family Name = "Doors_Integrated_Single-LR-Hold-Open-180_Total-Door" (IFCTEXT)
    Frame Projection Ext. = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Frame Projection Int. = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Frame Width = 0.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Doors_Integrated_Single-LR-Hold-Open-180_Total-Door" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Manufacturer = "Total Door" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR)
    Reference = "Doors_Integrated_Single-LR-Hold-Open-180_Total-Door" (IFCIDENTIFIER)
  IfcDoorPanelProperties | properties | on 1 object (1 IFCDOOR) | on 1 type object
    PanelWidth (no value)
  Constraints | properties | on 1 object (1 IFCDOOR)
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCDOOR)
    Area = 47.410029647427187 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 6.0120298489632997 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    2D DOOR PLAN = 2.84375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 7.90625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel height = 7.84375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 3.15625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    panel width = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Mark = "9" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    CAD Details = "https://www.arcat.com/company/total-door-systems-40592/cad" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "ARCAT" (IFCTEXT)
    Keynote = "08 17 00" (IFCTEXT)
    Manufacturer = "Total Door" (IFCTEXT)
    OmniClass Number = "23.30.10.00" (IFCTEXT)
    OmniClass Title = "Doors" (IFCTEXT)
    Product Page URL = "https://www.arcat.com/company/total-door-systems-40592" (IFCTEXT)
    Specification = "https://www.arcat.com/company/total-door-systems-40592/spec" (IFCTEXT)
    Type Mark = "9" (IFCTEXT)
    Type Name = "Doors_Integrated_Single-LR-Hold-Open-180_Total-Door" (IFCTEXT)
    URL = "https://totaldoor.com/" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCDOOR)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:271827 | predefined | on 1 type object
  Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:Doors_Integrated_Single-LR-Hold-Open-180_Total-Door:271827:1 | predefined | on 1 type object
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Materials and Finishes | properties | on 1 type object
    Magnet Finish = "Magnet Finish" (IFCLABEL)
    Panel Finish = "Door Panel Finish" (IFCLABEL)
    Push Pull Panic Bar = "Push Pull Panic Bar" (IFCLABEL)